{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["虹桥三期"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"虹桥三期","index":0,"n_rows":16,"n_cols":5,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["序号","名称","型号及规格","单位","数量"]
[1,"阻燃型导线穿管敷设","WDZB1-BYJ-750V-2.5mm2","米",900]
[2,"阻燃型导线穿管敷设","WDZB1-BYJ-750V-4mm2","米",800]
[3,"耐火型导线穿管敷设","WDZB1N-BYJ-750V-2.5mm2","米",200]
[4,"防火堵料",null,"公斤",10]
[5,"防火漆","10kg/桶","桶",2]
[6,"镀锌钢管","SC20","米",580]
[7,"接地线","热浸镀锌扁钢25x4","米",50]
[8,"局部等电位端子箱",null,"个",2]
[9,"双联单控照明开关","~250V 10A","个",4]
[10,"密闭双联单控照明开关","~250V 10A","个",4]
[11,"配合空调室外机移位",null,"项",1]
[12,"应急照明灯","220V，10W","套",4]
[13,"门禁",null,"套",4]
[14,"配电线路改移","开槽、移点位等","项",1]
[15,"烘手器插座","220V，10A，密闭型","个",2]