{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":97,"n_cols":11,"rows_kept":97,"cut":false,"hidden":false,"merged":[]}
["编号","名称","规格","内径","外径","厚度","内倒角","外倒角","高度","千件重","型号"]
[51,"ASME B18.21.1/B18.22.1 美制B型","0#","1.60-1.72","3.05-3.18","0.56-0.71",null,null,null,2.9000000000000001E-2,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","0#","1.60-1.72","4.65-4.78","0.56-0.71",null,null,null,7.8E-2,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","0#","1.60-1.72","6.22-6.35","0.56-0.71",null,null,null,0.14599999999999999,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1#","2.01-2.13","3.84-3.96","0.56-0.71",null,null,null,4.4999999999999998E-2,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1#","2.01-2.13","5.44-5.56","0.56-0.71",null,null,null,0.104,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1#","2.01-2.13","7.01-7.14","0.71-0.91",null,null,null,0.23400000000000001,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2#","2.26-2.39","4.65-4.78","0.56-0.71",null,null,null,6.8000000000000005E-2,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2#","2.26-2.39","6.22-6.35","0.71-0.91",null,null,null,0.17499999999999999,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2#","2.26-2.39","8.61-8.74","0.71-0.91",null,null,null,0.35499999999999998,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3#","2.64-2.77","5.44-5.56","0.56-0.71",null,null,null,9.1999999999999998E-2,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3#","2.64-2.77","7.80-7.92","0.56-0.71",null,null,null,0.27800000000000002,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3#","2.64-2.97","10.19-10.52","0.91-1.14",null,null,null,0.63900000000000001,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","4#","3.05-3.18","6.22-6.35","0.71-0.91",null,null,null,0.154,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","4#","3.05-3.38","9.40-9.73","0.91-1.14",null,null,null,0.52600000000000002,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","4#","3.05-3.38","11.00-11.33","0.91-1.14",null,null,null,0.73299999999999998,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","5#","3.45-3.78","7.01-7.14","0.71-0.91",null,null,null,0.19500000000000001,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","5#","3.45-3.78","10.19-10.52","0.91-1.14",null,null,null,0.60799999999999998,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","5#","3.45-3.78","12.57-12.90","0.91-1.14",null,null,null,0.95199999999999996,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","6#","3.84-3.96","7.80-7.92","0.71-0.91",null,null,null,0.23899999999999999,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","6#","3.84-4.17","11.00-11.33","0.91-1.14",null,null,null,0.7,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","6#","3.84-4.17","14.15-14.48","0.91-1.14",null,null,null,1.2010000000000001,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","8#","4.65-4.98","9.40-9.73","0.91-1.14",null,null,null,0.45400000000000001,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","8#","4.65-4.98","12.57-12.90","0.91-1.14",null,null,null,0.90100000000000002,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","8#","4.65-4.98","15.75-16.26","1.42-1.80",null,null,null,2.3929999999999998,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","10#","5.03-5.36","10.19-10.52","0.91-1.14",null,null,null,0.53100000000000003,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","10#","5.03-5.36","14.15-14.48","0.91-1.14",null,null,null,1.147,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","10#","5.03-5.36","18.47-19.02","1.42-1.80",null,null,null,3.3170000000000002,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","12#","5.82-6.15","11.00-11.33","0.91-1.14",null,null,null,0.58799999999999997,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","12#","5.82-6.15","15.75-16.26","1.42-1.80",null,null,null,2.2719999999999998,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","12#","5.82-6.15","22.05-22.61","1.42-1.80",null,null,null,4.7060000000000004,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1/4","7.01-7.52","12.57-13.08","1.42-1.80",null,null,null,0.90700000000000003,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1/4","7.01-7.52","18.47-19.02","1.42-1.80",null,null,null,1.8140000000000001,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1/4","7.01-7.52","25.22-25.78","1.42-1.80",null,null,null,5.4429999999999996,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","5/16","8.61-9.12","15.75-16.26","1.42-1.80",null,null,null,1.875,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","5/16","8.61-9.12","22.05-22.61","1.42-1.80",null,null,null,4.3090000000000002,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","5/16","8.61-9.12","28.40-28.96","1.42-1.80",null,null,null,7.5380000000000003,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3/8","10.19-10.69","18.47-19.02","1.42-1.80",null,null,null,2.5430000000000001,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3/8","10.19-10.69","25.22-25.78","1.42-1.80",null,null,null,5.5279999999999996,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3/8","10.19-10.69","31.57-32.51","2.29-2.84",null,null,null,14.68,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","7/16","11.79-12.29","22.05-22.61","1.42-1.80",null,null,null,3.669,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","7/16","11.79-12.29","28.40-28.96","1.42-1.80",null,null,null,6.8979999999999997,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","7/16","11.79-12.29","37.13-38.07","2.29-2.84",null,null,null,20.18,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1/2","13.36-13.87","25.22-25.78","1.42-1.80",null,null,null,4.7919999999999998,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1/2","13.36-13.87","31.57-32.51","2.29-2.84",null,null,null,13.53,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1/2","13.36-13.87","44.27-45.21","2.29-2.84",null,null,null,28.73,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","9/16","14.96-15.47","28.40-28.96","1.42-1.80",null,null,null,6.0620000000000003,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","9/16","14.96-15.47","37.13-38.07","2.29-2.84",null,null,null,18.87,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","9/16","14.96-15.47","50.62-51.56","2.29-2.84",null,null,null,37.5,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","5/8","16.48-17.42","31.57-32.51","2.29-2.84",null,null,null,12.09,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","5/8","16.48-17.42","44.27-45.21","2.29-2.84",null,null,null,27.3,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","5/8","16.48-17.42","56.97-57.91","3.71-4.42",null,null,null,75.959999999999994,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3/4","20.45-21.39","34.75-35.69","2.29-2.84",null,null,null,13.18,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3/4","20.45-21.39","50.62-51.56","2.29-2.84",null,null,null,34.51,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3/4","20.45-21.39","63.63-64.26","3.71-4.42",null,null,null,91.47,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","7/8","23.65-24.59","37.13-38.07","2.29-2.84",null,null,null,13.71,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","7/8","23.65-24.59","56.97-57.91","3.71-4.42",null,null,null,68.87,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","7/8","23.65-24.59","69.67-70.61","3.71-4.42",null,null,null,109.1,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1\"","26.80-27.74","44.27-45.21","2.29-2.84",null,null,null,20.420000000000002,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1\"","26.80-27.74","63.32-64.26","3.71-4.42",null,null,null,84.08,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1\"","26.80-27.74","76.02-76.96","3.71-4.42",null,null,null,128.30000000000001,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-1/8","30.00-30.94","50.62-51.56","2.29-2.84",null,null,null,27.09,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-1/8","30.00-30.94","69.67-70.61","3.71-4.42",null,null,null,100.7,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-1/8","30.00-30.94","82.37-83.31","3.71-4.42",null,null,null,148.9,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-1/4","33.15-34.09","56.97-57.91","3.71-4.42",null,null,null,55.57,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-1/4","33.15-34.09","76.02-76.96","3.71-4.42",null,null,null,118.9,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-1/4","33.07-34.47","88.65-90.04","5.94-6.76",null,null,null,280.89999999999998,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-3/8","36.35-37.29","63.32-64.26","3.71-4.42",null,null,null,69.22,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-3/8","36.35-37.29","82.37-83.31","3.71-4.42",null,null,null,138.5,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-3/8","36.27-37.67","95.00-96.39","5.94-6.76",null,null,null,319.5,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-1/2","39.50-40.44","69.67-70.61","3.71-4.42",null,null,null,84.43,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-1/2","39.42-40.82","88.65-90.04","5.94-6.76",null,null,null,262.5,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-1/2","39.42-40.82","101.35-102.74","5.94-6.76",null,null,null,360.6,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-5/8","44.27-45.21","76.02-76.96","3.71-4.42",null,null,null,97.68,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-5/8","44.20-45.59","95.00-96.39","5.94-6.76",null,null,null,293.89999999999998,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-5/8","44.20-45.59","107.70-109.09","5.94-6.76",null,null,null,398.4,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-3/4","47.45-48.39","82.37-83.31","3.71-4.42",null,null,null,115.6,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-3/4","47.37-48.77","101.35-102.74","5.94-6.76",null,null,null,332.9,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-3/4","47.37-48.77","114.05-115.44","5.94-6.76",null,null,null,443.9,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-7/8","50.55-51.94","88.65-90.04","5.94-6.76",null,null,null,222.4,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-7/8","50.55-51.94","107.70-109.09","5.94-6.76",null,null,null,374.3,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","1-7/8","50.55-51.94","120.40-121.79","5.94-6.76",null,null,null,491.8,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2\"","53.72-55.12","95.00-96.39","5.94-6.76",null,null,null,256.60000000000002,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2\"","53.72-55.12","114.05-115.44","5.94-6.76",null,null,null,418.2,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2\"","53.72-55.12","126.75-128.14","5.94-6.76",null,null,null,542.1,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2-1/4","60.07-61.47","101.35-102.74","5.94-6.76",null,null,null,278.3,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2-1/4","60.07-61.47","126.75-128.14","5.94-6.76",null,null,null,513.20000000000005,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2-1/4","60.07-61.98","139.45-141.35","9.07-9.98",null,null,null,958.4,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2-1/2","66.42-67.82","114.05-115.44","5.94-6.76",null,null,null,357.1,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2-1/2","66.42-68.33","139.45-141.35","9.07-9.98",null,null,null,911.4,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2-1/2","66.42-68.33","152.15-154.05","9.07-9.98",null,null,null,1131,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2-3/4","72.77-74.17","126.75-128.14","5.94-6.76",null,null,null,445.6,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2-3/4","72.77-74.68","152.15-154.05","9.07-9.98",null,null,null,1079,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","2-3/4","72.77-74.68","164.85-166.75","9.07-9.98",null,null,null,1318,"W/宽型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3\"","79.12-81.03","139.45-141.35","9.07-9.98",null,null,null,803.2,"N/窄型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3\"","79.12-81.03","164.85-166.75","9.07-9.98",null,null,null,1261,"R/标准型"]
[51,"ASME B18.21.1/B18.22.1 美制B型","3\"","79.12-81.03","177.55-179.45","9.07-9.98",null,null,null,1519,"W/宽型"]