{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":2206,"n_cols":8,"rows_kept":2206,"cut":false,"hidden":false,"merged":[]}
["产品编号","入库数量（千件）","名称","规格","材质",null,"表色","硬度"]
["F00000P6$7AA00000",25884,"PW6-7","5.5*18*1.6","A3普碳钢",null,"本色"]
["F00000P8$9AA00000",12579,"PW8-9","7.4*22*2.3","A3普碳钢",null,"本色"]
["F0000P6$10AA00000",9385,"PW6-10","5.5*18*2","A3普碳钢",null,"本色"]
["F00000P8$3AA00000",8508,"PW8-3","7.4*18*1.6","A3普碳钢",null,"本色"]
["F0000P10$8AA00000",7456,"PW10-8","9.4*26*2.6","A3普碳钢","NULL","本色","NULL"]
["F00000P6$2AA00000",6425,"PW6-2","5.5*12.5*1.6","A3普碳钢",null,"本色"]
["F00000P6$6AA00000",6424,"PW6-6","5.5*23*1.6","A3普碳钢",null,"本色"]
["G009785008AA00000",6065.51,"GB97-85","M8","碳钢",null,"本色"]
["F0004X015X016AA00",5678,88800093,"4*15*1.6","碳钢","NULL","本色140HV","NULL"]
["F047X15X1A0000000",5157.3,"P1H0515010-01-DQ","4.7*15*1","20#",null,"本色上蜡"]
["F074X16XAA0000000",4943.1000000000004,"2-127DQ","7.4*16*2","SPCC",null,"本色"]
["F0040121PW2030011",4895.8,"PW203-P-1","M5(非标外据齿）","65锰","NULL","不热处理本色","NULL"]
["F0040121PW5930011",4707.1000000000004,"PW593-11","M8/NFE25-511M","50#钢",null,"不热处理本色"]
["F0000P8$19AA00000",4600,"PW8-19","7.4*15.5*1.6","A3普碳钢",null,"本色"]
["G009785016AA00000",4323.4799999999996,"GB97-85","M16","碳钢","NULL","本色","100HV"]
["F000000JA24542085",4318.5,300583,"10*14.65*1.6","紫铜",null,"紫铜（退火）","HV≤55,原24542085"]
["G009785012AA00000",4274.1099999999997,"GB97-85","M12","碳钢",null,"本色"]
["F0040121PW5940011",4069.29,"PW594-9","10/NFE25-511M","50#钢",null,"不热处理本色"]
["G009785006AA00000",3439.76,"GB97-85","M6","碳钢","NULL","本色","NULL"]
["F00000P8$5AA00000",3332,"PW8-5","7.4*20*2.3","A3普碳钢",null,"本色"]
["G907424010AA200HV",3259.1,"GB9074.24","M10","碳钢",null,"本色","200HV"]
["F074X26X003GA0000",3169.3530000000001,"P1I0826030-00-DQ","7.4*26*3","35#钢",null,"热处理本色","300-370HV"]
["GB97850M08AK200HV",2503,"GB97-85","M8","碳钢",null,"三价锌72/144/5","200-300HV"]
["D006796008GG012UM",2228.1999999999998,"DIN6796","M8","65锰","NULL","达克罗三涂三烘+封闭96/500/12","420-490HV"]
[2081316,2095.1,297122,"7.05*25.65*1.7","Q235","NULL","三价锌5um","NULL"]
["G009785010AA00000",1962.52,"GB97-85","M10","碳钢",null,"本色"]
["D006796012MG0000F",1943.28,"DIN6796","M12","65锰",null,"环保达克罗500无红","420-490HV"]
["F055X132X2AA00000",1928.1,"P1H0613220-00","5.5*13.2*2","20#",null,"本色"]
["XXT0000016",1668.2,"7.05*25.65*1.7","7.05*25.65*1.7","Q235","NULL","三价锌5um","NULL"]
["GB9785M012AA140HV",1650.09,"GB97-85","M12","碳钢","NULL","本色","140-250HV"]
["D006796010GG012UM",1627.4,"DIN6796","M10","65锰","423k封存","达克罗 三涂三烘+封闭96/500/12","420-490HV"]
["G009685008AA00000",1584.41,"GB96-85","M8","碳钢","NULL","本色","140HV"]
["D00125A006AKHV140",1569,"DIN125A","M6","碳钢",null,"三价锌","140-250HV"]
["F00037X016X015AA0",1558.8,88800092,"3.7*16*1.5","碳钢","NULL","本色140HV","NULL"]
["D106796008MR00000",1552.2,"DIN6796","M8","65锰",null,"环保达克罗500无红","420-490HV"]
["F0007X15X2AA200HV",1535.7,"7*15*2","7*15*2","Q235",null,"本色","200-300HV"]
["F00074X26X003GA00",1408.2,"Q180826030","7.4*26*3","35#钢","NULL","热处理本色","300-370HV"]
["D01D6796M800000H1",1405.5,"DIN6796","M8","65锰","NULL","热处理本色上油","420-490HV"]
["D00125A004AK005UM",1372,"DIN125A","M4","碳钢",null,"三价锌5um","140-250HV"]
["F0000P10$3AA00000",1312.5,"PW10-3","9.4*22*2","A3普碳钢","NULL","本色","NULL"]
["D106796010MR00000",1297.76,"DIN6796","M10","65锰",null,"环保达克罗500无红","420-490HV"]
["X002000000M6PW435",1294.9000000000001,"PW435-P-3","M6组合用锥垫","65锰",null,"不热处理本色"]
["G009785004AAHV200",1294.5,"GB97-85","M4","碳钢",null,"本色","200-300HV"]
["G009785006ABHV140",1288,"GB97-85","M6","碳钢",null,"镀锌","140-250HV"]
["GB974LM05AA0200HV",1245.0999999999999,"GB97.4L-2002","M5","Q235","NULL","本色","200HV"]
["F00PWH14$50CAA000",1203,"PWH14-50C","13.2*28*3","S50C",null,"热处理本色","HRC40-48"]
["F055178012AA00000",1173.7,"5.5*17.8*1.2","5.5*17.8*1.2","A3普碳钢","菊龙","本色","NULL"]
["F00011X28X3MA0000",1171.1500000000001,"P1N1228030-00-DQ","11*28*3","65锰",null,"不热处理本色"]
["D009021M06ALHV140",1152.0999999999999,"DIN9021","M6","碳钢",null,"三价锌48/72/5","140-250HV"]
["G009785008AAHV200",1121.9000000000001,"GB97-85","M8","碳钢",null,"本色","200-300HV"]
["F0065X012X001AD00",1103.8,"AF194805","6.5*12*1","碳钢","NULL","发黑","NULL"]
["DIN137A003MA00000",1092.53,"DIN137A","M10","65锰",null,"不热处理本色"]
["X00000M08HA25511S",1087.0999999999999,"PW932-P-2","M8/NFE25-511S","50#钢",null,"不热处理本色"]
["ISO7093M08AL200HV",1069.5999999999999,"ISO7093","M8","碳钢",null,"三价彩锌72/120/8上封闭","200-300HV"]
["F0063X012X007AB00",1068.8,"6.3*12*0.7","6.3*12*0.7","碳钢","新乡红旗","镀锌","NULL"]
["GB97850M10AM200HV",1036,"GB97-85","M10","碳钢",null,"三价锌72/144/5","200-300HV"]
["F0PWH12$1CAA00000",1025,"PWH12-1C","11.4*24*2.5","50#钢","NULL","不热处理本色","85-95HRB"]
["G009785008ABHV140",1016,"GB97-85","M8","碳钢",null,"镀锌","140-250HV"]
["F0105X22X32AK0000",1000.5,"DH400703","10.5*22*3.2","SPCC","NULL","三价锌TNTUV12/144/5","86HRB"]
["D00125A008AKHV200",1000,"DIN125A","M8","碳钢",null,"三价锌","200-250HV"]
["X0NFE25-51106AA00",986,"NFE25-511M","M6","不锈钢304",null,"不锈钢304","锥形压花垫"]
["G086087004MJ00000",985,"GB860(同DIN137A)","M4","65锰","NULL","机械镀锌24/96","HRC43-50"]
["F0060841PW39800H8",896.1,"PW398-8","8.4*18*1","50#钢",null,"热处理本色(锥形）","HRC40-45"]
["G009785010AAHV200",892.6,"GB97-85","M10","碳钢",null,"本色","200-300HV"]
["D006796012GG012UM",871.08,"DIN6796","M12","65锰","NULL","达克罗 三涂三烘+封闭96/500/12","420-490HV"]
["XXT0000041",871,"GB97-85","M6","Q235","NULL","本色","140HV"]
["F000000jA10146516",870,"24542085（停用）","10*14.65*1.6","紫铜","NULL","紫铜","依工"]
["F030640918X2GA000",864.46,"P1I1035030-00-DQ","9.5*35*3","35#钢",null,"不热处理本色"]
["G907424008AA200HV",862.6,"GB9074.24","M8","碳钢","NULL","本色","200HV"]
["F030640937X2GA000",836.68,"P1I1234030-00-DQ","11*34*3","35#钢",null,"不热处理本色"]
["G009785M08AA00000",825,"GB97-85","M8","碳钢","NULL","本色","140-250HV"]
["D00125A010AKHV200",797.3,"DIN125A","M10","碳钢",null,"三价锌","200-250HV"]
["D0006796010MG000F",792.2,"DIN6796","M10","50CrV4",null,"上海环保达克罗500无红","420-490HV"]
["XNFE25-51108AA000",775.7,"NFE25-511M","M8","不锈钢304",null,"不锈钢304","锥形压花垫"]
["D00125A008AAHV140",770.6,"DIN125A","M8","碳钢",null,"本色","140-250HV"]
["G009785012GAHV200",769.4,"GB97-85","M12","碳钢",null,"本色","200-300HV"]
["F00000P6$8AA00000",760,"PW6-8","5.5*20*3.2","A3普碳钢",null,"本色"]
["0002362AW003900H1",751,"AW0039-6","2.8*6.6","65锰",null,"热处理本色","HRC26-34"]
["F006160PW125800@M",729.5,"PW1258-2","6.4*14*1.1","65锰","NULL","机械镀锌48/96/12","HRC40-45"]
["XXT0000273",724.7,"5.53*18.5*1.2","5.53*18.5*1.2","Q235","NULL","本色","NULL"]
["D00127B004ID00000",717.5,"DIN127B","M4","弹簧钢",null,"热处理发黑","430-530HV"]
["F094X24X3GA000000",714.68,88800197,"9.4*24*3","45#钢",null,"不热处理本色"]
["D00125A012AKHV200",674,"DIN125A","M12","碳钢",null,"三价锌","200-250HV"]
["X06798A004BA00000",672,"DIN6798A","M4","不锈钢304","NULL","不锈钢304","NULL"]
["D0004332x5AKHV140",665,"DIN433","M2.5","碳钢",null,"三价锌","140-250HV"]
["G009685006AA00000",649,"GB96-85","M6","碳钢","NULL","本色","140-250HV"]
["G009785010ABHV200",641.5,"GB97-85","M10","碳钢",null,"镀锌","200-300HV"]
["G009785006ABHV200",640,"GB97-85","M6","碳钢",null,"镀锌","200-300HV"]
["D00125A010AKHV140",640,"DIN125A","M10","碳钢",null,"三价锌","140-250HV"]
["G009685012AA00000",639.41999999999996,"GB96-85","M12","碳钢","NULL","本色","100HV"]
[100280,637.9,100280,100280,"A3普碳钢",null,"本色","美国WHTTESELL"]
["D00125A005AKHV200",628,"DIN125A","M5","碳钢",null,"三价锌","200-250HV"]
["D00125A006MKHV200",620,"DIN125A","M6","碳钢",null,"三价锌","200-250HV"]
["G009785016AA140HV",612.03,"GB97-85","M16","碳钢",null,"本色","140-250HV"]
["F064015015BA200HV",608.79999999999995,"BN91170 6166321","6.4*15*1.5","不锈钢304",null,"不锈钢304","200-300HV"]
["GB97850M12AM200HV",604.68399999999997,"GB97-85","M12","碳钢",null,"三价锌72/144/5","200-300HV"]
["F0000000024M70550",598.1,"24M7055","8.4*16*1.6（8/125A)）","Q235","NULL","三价锌TNTUV12/144/5","200-300HV"]
["D009021008AKHV140",596.6,"DIN9021","M8","碳钢",null,"三价锌","140-250HV"]
["G009785012AG00720",581.5,"GB97-85","M12","碳钢",null,"达克罗720无红","200-300HV"]
["F012032032GD00000",580.70000000000005,"BN45729/3327545","12*32*3.2","45#钢","NULL","发黑","HRC40-50"]
["F0011X021X025GA03",573.29999999999995,"DQ130039(A3)","11*21*2.5","45#钢",null,"不热处理本色上油"]
["G907425005AA00000",556.9,"GB9074.25","M5","碳钢","NULL","本色","NULL"]
["F06675X13235X0179",554.18499999999995,"BN90701/4084995","0.6675*1.3235*0.179","碳钢",null,"黄锌96无白12um"]
["G009785020AA140HV",550.35,"GB97-85","M20","碳钢","NULL","本色","140-250HV"]
["D00127B006II00000",544.9,"DIN127B","M6","弹簧钢",null,"机械镀锌"]
["D006796006GG012UM",543,"DIN6796","M6","65锰","NULL","达克罗三涂三烘+封闭96/500/12","420-490HV"]
["A200004945",540,200004945,"DIN125A M8","碳钢",null,"蓝白锌","200-250HV"]
["GB9685M08AA000000",538,"GB96-85","M8","碳钢","NULL","本色","NULL"]
["G009685006AAHV200",533.5,"GB96-85","M6","碳钢",null,"本色","200-300HV"]
["F0BN45854$3334202",521.1,"BN45854/3334202","12*24*1","45#钢",null,"机械镀锌","44-53HRC"]
["DIN9021M06ALHV200",515,"DIN9021","M6","碳钢",null,"三价锌48/72/5","200-250HV"]
["G97.185008ABHV200",514,"GB97-85","M8（停用）","碳钢","NULL","镀锌","200-300HV"]
["GB09785M12AK100HV",513,"GB97-85","M12","碳钢","NULL","三价锌12/24/3","100HV"]
["F0000PW8$14AA0000",513,"PW8-14","7.4*25*1.6","A3普碳钢",null,"本色"]
["XXT0000021",512,"DIN433","M2.5","Q235","NULL","三价锌5um","200-250HV"]
["G009785005AA200HV",508.6,"GB97-85","M5","碳钢",null,"本色","200-300HV"]
["X010000M10HA25511",507.4,"NFE25-511M","M10(停用）","50#钢","NULL","不热处理本色","友汇不用"]
["F0000P12$2AA00000",504,"PW12-2","11.3*41*3.2","A3普碳钢",null,"本色"]
["D10125A008AH140HV",502,"DIN125A","M8","碳钢",null,"三价黑锌12/24/3","140-250HV"]
["GB09785008ACHV100",501.02,"GB97-85","M8","碳钢","NULL","黄锌48/72/5","100HV"]
["FEPW1712389MD0000",489.9,"弹簧卡","EPW17/1.2-3-7-9","65锰","NULL","黑磷化（等温淬火回火）","440-480HV"]
["D106796006MR00000",481.5,"DIN6796","M6","65锰",null,"环保达克罗500无红","420-490HV"]
["XXT0000046",480,"PCW M11-5","PCW M11-5","Q235","NULL","本色","NULL"]
["GB09785006ABHV100",476.35,"GB97-85","M6","碳钢","NULL","三价锌24/96/5","100HV"]
["G009785005AA00000",475,"GB97-85","M5","碳钢",null,"本色"]
["G009685006ABHV140",473.8,"GB96-85","M6","碳钢",null,"镀锌","140-250HV"]
["F0505X1X005MD0000",465.7,"ERVW05-160","0.505*1*0.05","65锰",null,"发黑","HRC47-51"]
["F030741283X2GA000",464.3,"P5J32310240-00-DQ-C401-WG","11*32.3*4","45#钢",null,"不热处理本色上蜡"]
["D00127B010IG05000",463.6,"DIN127B","M10","弹簧钢","NULL","黑色环保达克罗500无红","NULL"]
["F005X0018X001AA00",462.2,"P1B6018010-00-DQ","5*18*1","SPCC",null,"本色上蜡","140HV"]
["GB09785M10AK100HV",458.1,"GB97-85","M10","碳钢","NULL","三价锌24/96/5","100HV"]
["F074X0226X0015GA0",450.6,"P1J0822615-00-DQ","7.4*22.6*1.5","45#钢",null,"热处理本色上蜡","300-390HV"]
["G009785004AA00000",450,"GB97-85","M4","碳钢",null,"本色"]
["DIN9021006AKHV200",440.5,"DIN9021","M6  厚度1.7-1.8","碳钢","NULL","三价锌48无红5um","220-300HV"]
["F0074X0226X0015GA",439.3,"Q180822615","7.4*22.6*1.5","45#钢","NULL","热处理本色上蜡","300-390HV"]
["F093X258X015GA000",438,"P1J1025215-00-DQ","9.3*25.8*1.5","45#钢",null,"热处理本色上蜡","300-390HV"]
["G009685005AA00000",436,"GB96-85","M5","碳钢",null,"本色"]
[100263,432.7,100263,100263,"10#钢",null,"本色","美国WHTTESELL"]
["X000NS70093010MR0",431,"SN70093","M10","65锰",null,"环保达克罗500无红","440-520HV"]
["F054X13X12AB00000",426,"P2H0613012-00-DQ","5.4*13*1.2","20#钢",null,"本色"]
["G009785006KA00000",425,"GB97-85","M6","黄铜","NULL","黄铜","NULL"]
["D00125A006BA00000",416.8,"DIN125A","M6","不锈钢304","NULL","不锈钢304","140HV"]
["G009785020AA00000",414.5,"GB97-85","M20","碳钢","NULL","本色","100HV"]
["F0013X24X25GA0000",411.93,"LVU30500","13*24*2.5","45#钢",null,"本色","300HV"]
["F000000024M709600",405.6,"24M7096","10.5*18*1.6","Q235",null,"三价锌TNTUV12/144/5","200-300HV"]
["F000000000R311136",405.07,"R311136","R311136","Q235","NULL","黑色环保达克罗240无红","NULL"]
["F0205X38X34AA0000",400.54,"美制平垫","3/4（20.5*38*3.4）","碳钢","NULL","本色","140-220HV"]
["G009685006AB200HV",399,"GB96-85","M6","碳钢",null,"镀锌","200-300HV"]
["F01D6796MA00000H1",397.3,"DIN6796","M10","65锰","NULL","热处理本色上油","420-470HV"]
["F00000000AA2054152",394.38,200794,"20.5*41*5","45#钢原24540512",null,"本色","300-370HV"]
["F002677PW116000H1",393.9,"PW1160-1","6.6*19*2","45#钢",null,"热处理本色","HRC36-42"]
["X06797J003MK00000",389,"DIN6798J","M3","65锰","NULL","三价锌","350-425HV"]
["F00000000024M71390",388,"24M7139","6.4*18*1.6(6/9021)","碳钢","NULL","三价锌TNTUV12/144/5","200-300HV"]
["F0000P6$13AA00000",384,"PW6-13","5.5*22*1.6","A3普碳钢","NULL","本色","NULL"]
["A300004761",384,300004761,"5.5*18*1.6","Q235","NULL","本色"]
["D00125A004CA00000",380,"DIN125A","M4","不锈钢316","NULL","不锈钢316","140HV"]
["DIN127B010II00000",377.6,"DIN127B","M10","弹簧钢","NULL","机械镀锌96无红","NULL"]
["F0010501PW69100HV",377,"PW691-8","M5双面压花锥垫","65锰","NULL","黑磷化","399-478HV"]
["D00127B012MR01000",374,"DIN127B","M12","弹簧钢","NULL","黑色环保达克罗500无红","NULL"]
["F00000P8$8AA00000",373.6,"PW8-8","7.3*42*2.3","A3普碳钢",null,"本色"]
["G009785012ABHV200",371.5,"GB97-85","M12","碳钢",null,"镀锌","200-300HV"]
["G009785005AB00000",365,"GB97-85","M5","碳钢",null,"镀锌"]
["G0097X4008AA200HV",361.34,"GB97.4N","M8","Q235","NULL","本色","200-300HV"]
["D00137BM03MI00000",361,"DIN137B","M3","65锰","NULL","机械镀锌","NULL"]
["F0000000000N41839",357.9,"美制标准型弹垫","10#","不锈钢304",null,"不锈钢304"]
["G009785008AB00000",356,"GB97-85","M8","碳钢",null,"镀锌"]
["GB96850M08AM200HV",356,"GB96-85","M8","碳钢",null,"三价锌72/144/5","200-300HV"]
["F0362X78X05MK0000",355.8,"外锯齿锁紧垫","3.62*7.8*0.5","65锰","NULL","三价锌5um","HRC30-40"]
["GB09785M08ALHV200",355,"GB97-85","M8","碳钢",null,"三价彩锌48/72/5","200-300HV"]
["G085987006IG00000",354,"GB859-87","M6","70#钢","NULL","达克罗500无红","NULL"]
["D00125A003AKLHV140",354,"DIN125A","M3","碳钢",null,"三价锌48/72/5","140-250HV"]
["F055X24X23AA00000",353,"P1B0624023-00","5.5*24*2.3","SPCC","NULL","本色上蜡","NULL"]
["F01127X37X3GA0000",351.5,88800194,"11.27*37*3","45#钢",null,"不热处理本色"]
["F0000002TV3005600",349.1,"2TV300560","0.388*0.990*0.049","Q235","NULL","三价黄锌 518Y","96无白5UM"]
["G009685010AA00000",348.27,"GB96-85","M10","碳钢","NULL","本色","100HV"]
["F105025020BA200HV",345.3,"BN91170 6166323","10.5*25*2","不锈钢304",null,"不锈钢304","200-300HV"]
["FBN48367$340129300",342.1,"BN48367/3401293","0.438*1*0.083（3/8W）","碳钢",null,"三价锌3-5um"]
["G009387008IG00000",342,"GB93-87","M8","65锰","NULL","达克罗500无红","42-50HRC"]
["D00125A006AAHV140",342,"DIN125A","M6","碳钢",null,"本色","140-250HV"]
["D01D6796M600000H1",340.8,"DIN6796","M6","65锰","NULL","热处理本色上油","420-490HV"]
["X00000M08MA25511F",340.5,"NFE25-511M","M8","65锰","NULL","不热处理本色","NULL"]
["X06798A006MK00000",330,"DIN6798A","M6","65锰","NULL","三价锌","350-425HV"]
["XXT0000042",328.7,"NFE25-511S","M8","50#","NULL","本色不热处理","NULL"]
["D00137A005AA00000",320.8,"DIN137A","M5","65锰",null,"热处理本色","430-530HV"]
["F006149AW00870011",320,"AW0087-2","3.2*8*0.8","碳钢","NULL","本色","NULL"]
["F0125X255X003GA04",314.8,"DQ140019(A4)","13.5*25.5*3","45#钢",null,"不热处理本色上油"]
["GB972002M06AK0000",313,"GB97.1-2002","M6","碳钢","NULL","三价锌48/72/5","200-300HV"]
["G009387010BA00000",312,"GB93-87","M10","不锈钢304",null,"不锈钢304"]
["G009785010AB00000",306,"GB97-85","M10","碳钢",null,"镀锌"]
["F0275X8X05AA00000",304.2,"Q110308005","2.75*8*0.5","SPCC",null,"本色"]
["A0000005$16MI0000",300,"美制标准型弹垫","'5/16","65锰","其中17K柏中不能发","机械镀锌","NULL"]
["XXT0000178",295,"DIN125A","M8","45#","NULL","环保达克罗0/720","300-370HV"]
["F0010501PW6540005",292,"PW654-5","6/SN70093","50#钢",null,"不热处理本色"]
["D00125A005AKHV140",290,"DIN125A","M5","碳钢",null,"三价锌","140-250HV"]
["D0004332X5AKHV200",290,"DIN433","M2.5","碳钢","NULL","三价锌","200-300HV"]
["F00000P8$4AA00000",288,"PW8-4","7.4*14*1.6","A3普碳钢",null,"本色"]
["D00137A006AI00000",287,"DIN137A","M6","65锰","NULL","机械镀锌","430-530HV"]
["F000000024M718000",286.43,"24M7180","13*37*3(12/9021)","Q235","NULL","三价锌TNTUV12/144/5","200-300HV"]
["F00PWH14$51CAA000",286.39999999999998,"PWH14-51C","13.2*38*2.8","50#钢",null,"热处理本色","HRC40-48"]
["D00125A008AKHV140",284,"DIN125A","M8","碳钢",null,"三价锌","140-250HV"]
["F084020025BA200HV",284,"BN91170 6166322","8.4*20*2","不锈钢304","NULL","不锈钢304","200-300HV"]
["G001230016GG00720",282.89999999999998,"GB1230","M16","45#钢","NULL","达克罗720无红","NULL"]
["F001050DW00110011",280.89999999999998,"DW0011-P-1","3.5*9.8*0.8 组合锥垫","50#钢","NULL","不热处理本色","NULL"]
["F00000000024M7293",279.60000000000002,"24M7293","6.5*13*1.6","1035钢",null,"机械镀锌48/96/8","300-370HV"]
["XXT0000233",279,"NFE25-511M","M6","不锈钢304","NULL","A2","NULL"]
["F0023621PW4330011",278.8,"AW001-6","8*0.4","不锈钢304","NULL","不锈钢304  钝化","NULL"]
["00000AKL401P28B43",277,"BN90719 6074858","L401P28B43","65锰",null,"三价锌72无红5um"]
["A300001422",276.5,300001422,"NFE25-511M M8 锥形压花","50#",null,"本色"]
["A200004958",276,200004958,"DIN125A M12","碳钢",null,"蓝白锌","200-250HV"]
["D00137A006AA00000",274,"DIN137A","M6","65锰","NULL","热处理本色","430-530HV"]
["F1000P6$16AA00000",272.5,"PW6-16","5.5*24*2.3","A3普碳钢",null,"本色"]
["G009785012ABHV140",272,"GB97-85","M12","碳钢",null,"镀锌","140-250HV"]
["DIN9021M04AL200HV",272,"DIN9021","M4","碳钢",null,"三价彩锌72/120/5上封闭","200-300HV"]
["X010000M08HA25511",268.39999999999998,"NFE25-511M","M8","50#钢",null,"本色（未热处理）","友汇不用"]
["G907424012AA200HV",268.2,"GB9074.24","M12","碳钢",null,"本色","200HV"]
["D06796012MG50CRV4",267.39999999999998,"DIN6796","M12","50CrV4",null,"上海环保达克罗500无红","420-490HV"]
["G009785010AG00720",265.5,"GB97-85","M10","碳钢",null,"达克罗720无红","200-300HV"]
["GB96850M10AM200HV",264.60000000000002,"GB96-85","M10","碳钢",null,"三价锌72/144/5","200-300HV"]
["F000000000N282054",264.5,"N282054","0.641X0.938X0.48","50#钢","NULL","热处理本色","HRC38-45"]
["D006796006ML00000",264,"DIN6796","M6","65锰","NULL","机械镀锌","420-490HV"]
["XNFE25-51108AC000",261.8,"PW779-1","M8/NFE25-511M","不锈钢316","15k友汇不用","不锈钢316","270-335HV"]
["GB09785M08AL200HV",261,"GB97-85","M8","碳钢","NULL","三价彩锌72/144/5","200-300HV"]
["G009685004AA200HV",260,"GB96-85","M4","碳钢",null,"本色","200-300HV"]
["ISO7089M08ARHV200",260,"ISO7089","M8","碳钢",null,"达克罗1000无红","200-300HV"]
["F0101X2X01345GA00",260,"BN90700/4084984","1.01*2*0.1345","50#钢",null,"本色","HRC40-50"]
["G009685016AA00000",256.86,"GB96-85","M16","碳钢","NULL","本色","100HV"]
["X000SN70093006MG0",256.3,"SN70093","M6","65锰",null,"环保达克罗500无红","440-520HV"]
["D00137A004AI00000",255,"DIN137A","M4","65锰",null,"机械镀锌"]
["F000P10$11AA00000",252,"PW10-11","9.4*18*2","A3普碳钢","NULL","本色","NULL"]
["G009785005ABHV200",251,"GB97-85","M5","碳钢",null,"镀锌","200-300HV"]
["D00127B003II00000",250,"DIN127B  ","M3","弹簧钢","67K艾维不用","机械镀锌","NULL"]
["D00125A012AKHV140",250,"DIN125A","M12","碳钢",null,"三价锌","140-250HV"]
["F0000000FH3044540",249.5,"FH304454","10.15*21.4*2.7","Q345","NULL","三价锌 TNTUV12/144/5","NULL"]
["F00000P8$7AA00000",248.4,"PW8-7","7.4*32*2.3","A3普碳钢",null,"本色"]
["X0100000M8MG2551H",248,"PW382-2","8/NFE25-511M","65锰","NULL","达克罗三涂三烘+封闭96/500/12","HRC42-49"]
["F0475X011X005BA00",247.9,"组合波形弹垫","4.75*11*0.5","不锈钢304",null,"不锈钢304","昇沪"]
["D00125A016AK200HV",246.8,"GB97-85","M16","碳钢",null,"三价锌72/144/5","200-300HV"]
["D00125A010AAHV140",246.1,"DIN125A","M10","碳钢",null,"本色","140-250HV"]
["GB972002M10AK0000",246,"GB97.1-2002","M10","碳钢","NULL","三价锌48/72/5","200-300HV"]
["DIN6796004MR00000",243.4,"DIN6796","M4","65锰",null,"环保达克罗500无红","420-490HV"]
["F053X12X15BA200HV",242,"BN91170 6166320","5.3*12*1.5","不锈钢304",null,"不锈钢304","200-300HV"]
["F084X24X5GA000000",240.35,"P1J0924050-00-DQ-HT","8.4*24*5","45#钢",null,"不热处理本色上蜡"]
["XXT0000030",240,"PCWM10-20","PCWM10-20","Q235","NULL","本色","NULL"]
["DIN9021M05AL200HV",240,"DIN9021","M5","碳钢",null,"三价彩锌72/120/3","200-250HV"]
["F030640905X2AA000",239.93,"P1H0630016-00-DQ","5.6*30*1.6","20#钢",null,"本色上蜡"]
["F095X024X025AA000",237.8,88800168,"9.5*24*2.5","45#钢",null,"本色+干油"]
["G009785010AGHV200",237.5,"GB97-85","M10","碳钢",null,"达克罗500无红","200-300HV"]
["X000000M005MJ25514",237,"NFE25-514M","M5","碳钢","NULL","三价彩锌72/120/8","160-250HV"]
["F014X12X0049AL000",235.6,"BN90700/4052330","1/4*1/2*0.049","Q235",null,"三价黄锌(518Y)72/120/8"]
["F0000000219387439",234.67,219.387439,"23*32*2.5",null,null,"本色","盛派"]
["ISO7089M04ALHV200",233,"ISO7089","M4","碳钢","NULL","三价彩锌72/120/3","200-300HV"]
["ISO7094M06AH00000",231.3,"24M7309","6/ISO7094","碳钢","NULL","三价黑锌TNTUV12/144/5","100-200HV"]
["X0000000M8MG2551H",231,"NFE25-511M","M8","65锰","NULL","上海环保达克罗500无红","NULL"]
["F030640914X2GA000",230.75,"P1I1438030-00-DQ","12.9*38*3","35#钢",null,"不热处理本色"]
["F012X020X153TK000",230.3,"SH1290(异形垫）","12*20*1.53","50#钢","NULL","三价锌5um","HRC45-50"]
["DIN125A010ALHV200",230,"DIN125A","M10","碳钢","NULL","三价彩锌 72/144/8","200-250HV"]
["GB97850M06AM200HV",228.88200000000001,"GB97-85","M6","碳钢",null,"三价锌72/144/5","200-300HV"]
["X06798A008MK00000",227,"DIN6798A","M8","65锰","NULL","三价锌","350-425HV"]
["F0000000024M71170",224,"24M7117","4.3*9*0.8","Q235B",null,"三价锌TNTUV12/144/5","200-300HV"]
["F105025025AK00000",223.3,"BN90701 6009325","10.5*25*2.5","碳钢","NULL","三价锌","NULL"]
["D0006796008GI0000",221.9,"DIN6796","M8","65锰","NULL","机械镀锌","420-490HV"]
["DIN6796012GI012UM",220.8,"DIN6796","M12","65锰","NULL","机械镀锌72/144/12","420-490HV"]
["A200001183",220,200001183,"NFE25-511M M10","50#",null,"本色"]
["F0BN91170$4014838",220,"BN91170/4014838","0.143*0.267*0.016","不锈钢304","NULL","不锈钢304 钝化","NULL"]
["D006796008BA00000",219.8,"DIN6796","M8","不锈钢304",null,"不锈钢304"]
["A000001$2WAA00000",219.7,"美制W型","1/2W","碳钢","NULL","本色","NULL"]
["A200001592",218.7,200001592,"DIN6796 M10","65Mn",null,"环保达克罗0/500","420-490HV"]
["X06798A006BA00000",217.8,"DIN6798A","M6","不锈钢304",null,"不锈钢304","西门子"]
["F0000002610927724",217,"BN90701   6009269",2610927724,"Q235",null,"三价黑锌","不上油"]
["F0355X017X002AA00",215.5,"P1A0417020-00-DQ","3.55*17*2","Q195B",null,"本色上蜡"]
["D000440006AKHV100",215.3,"DIN440","M6","碳钢",null,"三价锌","100-250HV"]
["D00127B008II00000",215,"DIN127B","M8","弹簧钢",null,"机械镀锌"]
["D0067960086ML00000",214,"DIN6796","M6","50CrV4",null,"环保达克罗500无红","420-490HV"]
[6082943,213,"NFE27620B","M2.5","不锈钢304","NULL","不锈钢304","NULL"]
["D00125A006AKHV200",212,"DIN125A","M6","碳钢",null,"三价锌96无白5um","200-250HV"]
["D00125A010BA00000",210.5,"DIN125A","M10","不锈钢304","NULL","不锈钢304","140HV"]
["XNFE2551106CA0000",209.2,"NFE25-511M","M6","不锈钢316",null,"不锈钢316"]
["F00000000MWA00201",208.5,"WA-0002-00(REV1)","WA-0002-00(REV1)","碳钢","NULL","三价锌3um","NULL"]
["G009785016ABHV200",207.4,"GB97-85","M16","碳钢",null,"镀锌","200-300HV"]
["G009387012MG00000",207.27,"GB93-87","M12","65锰",null,"达克罗720无红","42-50HRC"]
["G009685008ABHV200",206.5,"GB96-85","M8","碳钢",null,"镀锌","200-300HV"]
["G084885006AA200HV",206,"GB848-85","M6","碳钢",null,"本色","200-300HV"]
["F084020020BA00000",206,"8.4*20*2","8.4*20*2","不锈钢304","NULL","不锈钢304","NULL"]
["F0455X13X1GA300HV",205.6,"Q190513011","4.55*13*1","50#钢","NULL","热处理本色","300-370HV"]
["G085987004IL00000",204,"GB859","M4","70#钢","NULL","三价彩锌48/72","NULL"]
["F000000024M704000",203.1,"24M7040","11*20*2","Q235B",null,"三价锌TNTUV12/144/5","100-200HV"]
["X06798J006MA00000",202.5,"DIN6798J","M6","65锰",null,"不热处理本色"]
["F0142X245X585MR00",202.3,"BN90704 6172339","14.2*24.5*3.5  弹垫,高度5.85","65锰","NULL","黑色环保达克罗500无红","HRC42-50"]
["GB862X287M08MI000",201,"GB862.2-87","M8","65锰","NULL","机械镀锌24/96","HRC43-50"]
["NFE25$513M008BA0L",200.4,"NFE25-513L","M8","不锈钢304","NULL","不锈钢304","NULL"]
["GB9785M10IK000000",200,"GB97-85","M10","碳钢",null,"三价锌24/72/8","200-300HV"]
["D00127BM05IK00000",200,"DIN127B","M5","弹簧钢","NULL","三价彩锌","NULL"]
["D009021005AAHV140",200,"DIN9021","M5","碳钢",null,"本色","140-250HV"]
["A300004796",199,300004796,"5/16 美制标准型弹垫","65Mn","NULL","机械镀锌"]
["G009685010ABHV200",198.4,"GB96-85","M10","碳钢",null,"镀锌","200-300HV"]
["X006798A005MA0000",198,"DIN6798A","M5","65锰",null,"不热处理本色"]
["A200001591",197.96,200001591,"DIN6796 M12","65Mn",null,"环保达克罗0/500","420-490HV"]
["A300000550",197.8,300000550,"AW001-6 8*0.4 圆片(停用）","304不锈钢","NULL","洗白钝化","NULL"]
["GB9785M010AL200HV",197,"GB97-85","M10","碳钢","NULL","三价彩锌","200-300HV"]
["D00127B005II00000",196,"DIN127B","M5","弹簧钢",null,"机械镀锌"]
["ISO7093M08AKHV200",194.5,"ISO7093","M8","碳钢",null,"三价彩锌72/216/8","200-300HV"]
["F00011X038X003AL0",190.5,"BN90701 6124621","11*38*3","碳钢",null,"三价彩锌48/72/5"]
["F30670592X2GA0000",190,"P1I1024030-00-DQ","9.5*24*3","35#钢",null,"不热处理本色"]
["G009387006IK005UM",187.8,"GB93-87","M6","65锰",null,"三价锌48无红5um","42-50HRC"]
["X000000M10BA25511",187.8,"NFE25-511M","M10","不锈钢304",null,"不锈钢304","锥形压花垫"]
["F016X262X005MR000",187.59,"BN90704/6172385","16.2*26.2*3.5（弹垫）","65锰","NULL","黑色环保达克罗500无红","HRC43-50"]
["G0096850010ABHV140",187.2,"GB96-85","M10","碳钢",null,"镀锌","140-250HV"]
["D000433006BA00000",187,"DIN433","M6","不锈钢304",null,"不锈钢304"]
["F0000000024M74530",186.9,"24M7453","5.5*15*1(5/ISO7093-2)","Q235B","NULL","三价黑锌TNTUV12/144/8","100-200HV"]
["F1000P6$17AA00000",186,"PW6-17","5.5*26*1.6","A3普碳钢",null,"本色"]
["F0155X40X55GA0000",185.32,"P1J1640055-00","15.5*40*5.5","45#钢","NULL","不热处理本色","NULL"]
["XXT0000211",183,"DIN137B","M3","65Mn","NULL","机械镀锌24/72/5um","44-48HRC"]
["D00125A004BA00000",181,"DIN125A","M4","不锈钢304",null,"不锈钢304","140-250HV"]
["XXT0000080",180,"DIN6798A","M8","65Mn","NULL","三价锌72无红","300HV"]
["ISO7089M08AK200HV",180,"ISO7089","M8","碳钢",null,"三价彩锌72/120/3","200-300HV"]
["F0266X075X006AH00",179.8,"T134530","0.266*0.75*0.06","Q235",null,"三价黑锌TNTVU12/144/5","<302HV"]
["F03$8*0875BA00000",179.6,"BN91170/3868171","3/8*0.875","不锈钢304","NULL","不锈钢304","NULL"]
["F87X017X002GK0000",178.5,"8.7*17*2","8.7*17*2","45#钢",null,"机械镀锌48/96/8摩擦0.14-0.2","300-370HV"]
["F006149AW00940011",177,"AW0094-4","3.2*10*0.8","Q235",null,"本色"]
["A200001745",177,200001745,"SN70093 M10","65Mn",null,"环保达克罗0/500","440-520HV"]
["D00127B006IK00000",176,"DIN127B","M6","弹簧钢",null,"三价锌48/72/5"]
["XXT0000287",176," WA-0001-00 3/8N"," WA-0001-00 3/8N","Q235","NULL","三价锌3um","NULL"]
["GB97200014AKHV300",174.7,"GB97.2-2002","M14","45#钢",null,"三价彩锌","300-370HV"]
["D006796010Gi00000",174.1,"DIN6796","M10","65锰","NULL","机械镀锌","420-490HV"]
["F0025661PW7230011",171.8,"PW723-2","0.123*0.505*0.04","SPCC",null,"本色"]
["D01D6796N200000H1",171.16,"DIN6796","M12","65锰","NULL","热处理本色上油","420-490HV"]
["XXT0000231",170.69,"LVU30500","LVU30500","45#","NULL","热处理本色","310-360HV"]
["A300004652",170.2,300004652,"N282054","45#","NULL","本色"]
["D00125A2x5BA00000",170,"DIN125A","M2.5","不锈钢304","NULL","不锈钢304","140HV"]
["GB96850M06AM200HV",170,"GB96-85","M6","碳钢",null,"三价锌72/144/5","200-300HV"]
["F0023621AW013GW1S",169.7,"AW0013-4","4.17*15*1.0","不锈钢304",null,"不锈钢304"]
["F0000000MK0600000",169,"美制标准弹垫","6#","65锰",null,"机械镀锌8um"]
["F005X012X015HV160",168,"BN90701 6115400","5*12*1.5","碳钢","NULL","三价彩锌72/120/5","160HV"]
["GB972002M08AK0000",168,"GB97.1-2002","M8","碳钢","NULL","三价锌48/72/5","200-300HV"]
["D00125A006CA00000",167.9,"DIN125A","M6","不锈钢316",null,"不锈钢316"]
["DIN6796M12NJ00000",166.8,"DIN6796","M12","50CrV4","NULL","机械黄锌96/144/12","420-470HV"]
["F021X34X3GA000000",165.7,"KK54932","21*34*3","35#钢","NULL","热处理本色","300-370HV"]
["F00000000024M7453",165.3,"24M7453","24M7453",null,null,"三价黑锌"]
["F0025X0562X0049BA",165,"BN48346/3464341","0.25*0.562*0.049","不锈钢304","NULL","不锈钢304","NULL"]
["X06797J004MG00000",165,"DIN6797J","M4","不锈钢304",null,"不锈钢304","西门子"]
["ISO7089M06AN200HV",163,"ISO7089","M6","碳钢","NULL","灰色锌镍96/150","200-300HV"]
["F0091X016X012J000",163,"143-1DQ","9.1*16*1.2","紫铜","NULL","紫铜","机械性能≤HV45"]
["A300000250",163,300000250,"1/4 弹垫","304不锈钢",null,"本色"]
["D00127B005ID00000",162,"DIN127B","M5","弹簧钢",null,"发兰"]
["D00127B004BA00000",162,"DIN127B","M4","不锈钢304",null,"不锈钢304"]
["F13X025X003GI0000",160.4,"13*25*3","13*25*3","45#钢","NULL","机械镀锌48/96/8,摩擦0.14-0.22","300-370HV"]
["G084885004AA00000",160,"GB848-85","M4","碳钢",null,"本色"]
["F0000000219387438",160,219.387438,"0.649*1.28*0.16","Q235",null,"本色","盛派"]
["G0097X4006AA200HV",159.65,"GB97.4N","M6","Q235",null,"本色","200HV"]
["F463077073CA00000",158.75,"BN91170   6056055","0.463*0.77*0.073","不锈钢316",null,"不锈钢316","敲316字"]
["G009387010MD00000",157,"GB93-87","M10","65锰",null,"发黑","42-50HRC"]
["G009685012AG00720",156,"GB96-85","M12","碳钢",null,"达克罗720无红","200-300HV"]
["ISO7089M06AL200HV",156,"ISO7089","M6","碳钢",null,"三价彩锌72/120/5上封闭","200-300HV"]
["X00862.2-87008MB0",156,"GB862.2-87","M8","65锰",null,"镀锌","西门子"]
["G009785012AB00000",155.5,"GB97-85","M12","碳钢",null,"镀锌"]
["F002677PW112500H1",155,"PW1125-1","6.5*22*2.5","45#钢",null,"热处理本色","HRC36-42"]
["A0000001$4BA00000",155,"美制标准型弹垫","'1/4","不锈钢304",null,"不锈钢304"]
["D0090212X5AKHV140",155,"DIN9021","M2.5","碳钢",null,"三价锌","140-250HV"]
["F043X10X01BA200HV",154.6,"BN91170 6166327","4.3*10*1","不锈钢304",null,"不锈钢304","200-300HV"]
["F00055X15X15AK000",152.9,"3810S.050.001.C96","5.5*15*1.5","碳钢","NULL","三价彩锌96无红","NULL"]
["F002362AW004100H1",152,"AW0041-5","2.2*7*0.7","65锰",null,"热处理本色","HRC26-34"]
["D00125A005AAHV200",151,"DIN125A","M5","碳钢",null,"本色","200-250HV"]
["X000SN70093005MI0",151,"SN70093","M5","65锰",null,"机械镀锌","440-520HV"]
["A0000003$8BA00000",150.69999999999999,"美制标准型弹垫","'3/8","不锈钢304",null,"不锈钢304"]
["D00125A016AKHV200",150.5,"DIN125A","M16","碳钢",null,"三价锌","200-250HV"]
["F000000AK24M74370",150.5,"24M7437","6.5*35*3","Q235",null,"三价黑锌TNTVU12/144/5","<302HV"]
["XXT0000050",150.03,"GB97-85","M12","Q235","NULL","本色","140HV"]
["F00000P6$3AAHV200",150,"PW6-3","5.5*14*1","A3普碳钢",null,"本色","200-300HV"]
["F0000002610912616",150,"BN90701  6009312",2610912616,"65锰","NULL","发黑干油","HRC45-50"]
["F000000024M713800",150,"24M7138","5.3*15*1.0(5/ISO7093)","Q235B","NULL","三价锌TNTUV12/144/5","200-300HV"]
["GB96200M04AK0000",149,"GB96.1-2002","M4","碳钢","NULL","三价锌48/72/5","200-300HV"]
["FBN907046140860MG",148.80000000000001,"BN90704  6140860","'5/16 锥垫","65锰","NULL","环保达克罗500无红","NULL"]
["D00127B010II00000",148.5,"DIN127B","M10","弹簧钢",null,"机械镀锌"]
["D006796006BA0000A",148,"DIN6796","M6","不锈钢304",null,"不锈钢304"]
["F002566PW116400H1",147.75,"PW1164-2","10*31*1","65锰",null,"热处理本色","调整垫片HRC40-45"]
["G009685008ABHV140",147.5,"GB96-85","M8","碳钢",null,"镀锌","140-250HV"]
["D006796008GR012UM",145.4,"DIN6796","M8","65锰","NULL","环保机械黄锌72/144/12","420-490HV"]
["F005X125X0083AK00",145.38,"24H1226","0.5*1.25*0.083","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["F001050DW00100011",144,"DW0010-P-1","4.5*10*0.8 组合锥垫","50#钢","NULL","不热处理本色","NULL"]
["XXT0000068",144,"PWH M14-9","PWH M14-9","Q235","NULL","本色","NULL"]
["GB96850M12AM200HV",143.4,"GB96-85","M12","碳钢",null,"三价锌72/144/5","200-300HV"]
["000000A315DIN2093",142,"DIN2093","31.5 A型","65锰",null,"Geomet321A +ML","500无红"]
["F064X25X15AK00000",141.1,"BN732  8027315","6.4*25*1.5","碳钢","NULL","三价锌","140HV"]
["F093X28X3GA000000",140.6,"P1I1028030-00-DQ","9.3*28*3","35#钢",null,"热处理本色","300-370HV"]
["G085987004IE00000",140,"GB859","M4","70#钢","NULL","黄锌48/72","NULL"]
["XXT0000244",139.81,"GB97-85","M12","Q235B","NULL","本色","100HV"]
["GB97200206AA200HV",139.19999999999999,"GB97.1-2002","M6","碳钢",null,"本色","200-300HV"]
["GB8482002M06AC000",138,"GB848-2002","M6","碳钢","NULL","黄锌","200-300HV"]
["D30125A008AKHV200",138,"DIN125A","M8","碳钢",null,"三价锌48/72/5","200-250HV"]
["F00000000G24M7617",137.69999999999999,"24M7617","17*30*3","45#钢",null,"环保达克罗960无红","300-370HV"]
["SN70093M08MK00000",137.6,"SN70093","M8","65锰",null,"机械镀锌48/144/12","440-520HV"]
["GB9785M12IK000000",136.80000000000001,"GB97-85","M12","碳钢",null,"三价锌24/72/8","200-300HV"]
["GB09685M05AA200HV",136,"GB96-85","M5","碳钢",null,"本色","200-300HV"]
["A300001424",135.5,300001424,"NFE25-511M M10 锥形压花","50#",null,"本色"]
["000000B315DIN2093",135,"DIN2093","31.5 B型","65锰",null,"Geomet321A + VL","500无红"]
["0000000BAN402AP11",135,"BN91170  6130882","N402AP11","不锈钢304",null,"不锈钢304"]
["XXT0000227",135,"DIN9021","M3","Q235","NULL","三价彩锌","200HV"]
["G009785012AGHV200",134.5,"GB97-85","M12","碳钢",null,"达克罗500无红","200-300HV"]
["X000000M08MK25511",134.1,"NFE25-511M","M8","65锰",null,"机械镀锌","锥形压花垫"]
["A200002097",134,200002097,"DIN1440 M8","Q235",null,"三价黑锌","160-250HV"]
["F0095X35X3GA300HV",133.87,"P1J1035030-00","9.5*35*3","45#钢",null,"热处理本色","300-370HV"]
["F0455012008AA0000",133.69999999999999,"P1B0512008-00-DQ","4.55*12*0.8","SPHC",null,"本色上蜡 HV140"]
["X0000000M6MR25511",133,"NFE25-511M","M6","65锰","NULL","上海环保达克罗500无红","NULL"]
["GB97200212AK200HV",132,"GB97.1-2002","M12","碳钢","NULL","三价锌48/72/5","200-300HV"]
["G009387M10IF00000",131.30000000000001,"GB93-87","M10","65锰",null,"热锌","HRC30"]
["ISO7092M06AKHV200",131,"ISO7092","M6","碳钢",null,"三价锌12/36/3","200-300HV"]
["GB97200014AKHV200",130.69999999999999,"GB97.2","M14","碳钢",null,"三价锌72/144/5","200-300HV"]
["NFE25$511020MG000",130.5,"JB/ZQ4340","M20","65锰",null,"达克罗"]
["F00175X30X035GA04",129.9,"DQ120755(A4)","17.5*30*3.5","45#钢","NULL","不热处理本色上油","NULL"]
["DIN137BM05MN00000",129,"DIN137B","M5","65锰","NULL","黑磷化","NULL"]
["F000000024M709100",128.62,"24M7091","26*44*4","Q235B","NULL","三价锌TNTUV12/144/5","100-200HV"]
["D00127B012II00000",128.6,"DIN127B","M12","弹簧钢",null,"机械镀锌"]
["F047X15X1GA000000",128.30000000000001,"Q190515010A","4.7*15*1","50#钢",null,"本色"]
["NF25514M05AN0000M",128,"NFE25-514M","M5","碳钢","NULL","灰色锌镍150无红","160-250HV"]
["F0064X11X2AN300HV",128,"BN90701 6009200","6.4*11*2","65锰",null,"灰色锌镍72无白5um","300-370HV"]
["ISO7089M10AH200HV",127,"ISO7089","M10","碳钢",null,"三价彩锌72/120/8上封闭","200-300HV"]
["D009021008AAHV140",126.9,"DIN9021","M8","碳钢",null,"本色","140-250HV"]
["G009785012AC200HV",126.5,"GB97-85","M12","碳钢",null,"黄锌","200-300HV"]
["D000433004CA00000",125,"DIN433","M4","不锈钢316",null,"不锈钢316"]
["01B0011619P01535L",124.5,"BN90701   6009267","1619P01535L","碳钢","NULL","三价锌","NULL"]
["D006796008GI012UM",124.3,"DIN6796","M8","65锰","NULL","机械镀锌72/144/12","420-490HV"]
["D00125A006BAHV200",124,"DIN125A","M6","不锈钢304",null,"不锈钢304","200HV"]
["F84X18X1MJ0000000",124,"RT22124-M8","8.4*18*1","65锰","NULL","机械镀锌24/96","HRC42-50"]
["A300004776",123.85,300004776,"18*30*0.5 DIN522A","碳钢","NULL","本色上油"]
["F00000GK012X10000",122.4,"BN90700/3327059","12*1","1050钢","NULL","三价锌72无白5um","44-53HRC"]
["G009685M06AA00000",122,"GB96-85","M6","碳钢","NULL","本色","NULL"]
["A300000248",121.95,300000248,"3/8 弹垫","304不锈钢",null,"本色"]
["F005X0875X01BA000",121.2,"BN91170/4059422","0.5*0.875*0.1","不锈钢304","NULL","不锈钢304","NULL"]
["F0184X0375X0030AK",121,"0.184*0.375*0.03","0.184*0.375*0.03","Q235B",null,"三价锌48/72/5","140-250HV"]
["F063011006AA00000",121,"PW212-1","6.3*11*0.6","碳钢",null,"本色"]
["G009387006BA00000",120.7,"GB93-87","M6","不锈钢304",null,"不锈钢304"]
["F00000000024M7523",120.15,"24M7523","10.5*30*2.5","Q235",null,"环保达克罗960无红","200-300HV"]
["F0000P10$2SAPH440",120,"PW10-6","9.4*27*3.2","SAPH440",null,"本色"]
["F000000024M708700",120,"24M7087","5.5*10*1","Q235B","NULL","三价锌TNTUV12/144/5","100-200HV"]
["D009021004AKHV140",120,"DIN9021","M4","碳钢",null,"三价锌","140-250HV"]
["F00011X25X003GA01",119.7,"DQ140241(A1)","11*25*3","45#钢",null,"不热处理本色上油"]
["F09X1657X136AK000",119.2,"9*16.57*1.36","9*16.57*1.36(外倒角）","Q235B",null,"三价彩锌72/216/8","140-250HV"]
["F0105X22X12MI0000",119,"RT22124-M10","10.5*22*1.2","65锰","NULL","机械镀锌24/96","HRC42-50"]
["DIN127BM03NA00000",119,"DIN127B","M3","磷青铜","NULL","磷青铜","NULL"]
["D00127B003BA00000",119,"DIN127B","M3","不锈钢304",null,"不锈钢304"]
["G009387012IFHRC30",118.9,"GB93-87","M12","65锰",null,"热锌","HRC30"]
["D007980008ID00000",118.8,"DIN7980","M8","弹簧钢",null,"发黑"]
["D00127B003ID00000",118,"DIN127B","M3","弹簧钢",null,"热处理发黑","430-530HV"]
["001B0012610931247",118,"BN90701 6009243",2610931247,"碳钢","NULL","三价锌","NULL"]
["F053X27X21X2GA000",117.64,"200-2(矩DQ）","5.3*27*21*2","50#钢","NULL","热处理本色","360-430HV"]
["F142X30X45GK00000",117.15,"DJ222014-TZ","14.2*30*4.5","45#钢","NULL","三价锌 48无白5um ","HRC39-44"]
["G009685012AA140HV",117.08,"GB96-85","M12","碳钢","NULL","本色","140-250HV"]
["ISO7090M06BA200HV",117,"ISO7090-2000","M6","不锈钢304",null,"不锈钢304","200-300HV"]
["D00125B006B200HV",117,"DIN125B","M6","不锈钢304",null,"不锈钢304","200HV"]
["F055X18X16GA00000",116.36,88800196,"5.5*18*1.6","45#钢",null,"不热处理本色"]
["F0000000024M70440",116,"24M7044","13*20*2","Q235B","NULL","三价锌TNTUV12/144/5","200-300HV"]
["F0219X0437X0045AK",115,"BN90701   6214738","0.219*0.437*0.045","A3普碳钢",null,"三价锌","140HV"]
["D009021010AKHV140",115,"DIN9021","M10","碳钢",null,"三价锌","140-250HV"]
["F0000000AK24H1347",114.77,"24H1347","0,531 x 2 x 0,194","碳钢",null,"三价锌TNTUV12/144/5","<302HV"]
["XXT0000005",114.7,"BN45689 3330204","24M7027","Q235","NULL","三价锌TNTUV","NULL"]
["A300004066",114.45,300004066,"2020-01-02","中碳钢",null,"机械镀锌5um","38-45HRC"]
["F0000001$2AA00000",114.28,"美制弹垫（扩孔）","'1/2","65猛",null,"本色","内径：0.522-0.532"]
["F018X30X05AA00000",114.25,"DIN522A","18*30*0.5","碳钢",null,"本色上油"]
["DIN6796006BA200HV",114,"DIN6796","M6","不锈钢304",null,"不锈钢304","200HV"]
["XXT0000296",114,"DIN9021","M3.5","Q235","NULL","三价锌0/96/8um","200-300HV"]
["X06798A004MK00000",113.8,"DIN6798A","M4","65锰","NULL","三价锌","350-425HV"]
["GB96X22002M060000",113.5,"GB96.2-2002","M6","碳钢","NULL","三价彩锌72无白","100-200HV"]
["FBN90701$40558820",111.83,"BN90701/4055882","11*43*3","Q235B",null,"三价锌12无白5um上封闭","140HV"]
["F0BN90701$4078302",111.5,"BN90701/4078302","10.5*20*1","Q235","NULL","三价锌","NULL"]
["X000SN70093M06MI0",111,"BN90700  6188743","M6/SN70093（六足高度增加）","65锰","NULL","机械镀锌","NULL"]
["F00000000BA99CB50",111,"99CB50(REV.4)","12.7*23.62*1.575","不锈钢304",null,"不锈钢304"]
["A00000010NAH00000",111,"美制N型","10#N","碳钢",null,"三价黑锌96无红8um"]
["DIN125A004ALHV200",111,"DIN125A","M4","碳钢",null,"三价彩锌48/72/5","200-250HV"]
["GB84885006GA300HV",110.5,"GB848-85","M6","45#钢",null,"热处理本色","300-370HV"]
["A000005$16BA00000",110.4,"美制标准型弹垫","'5/16","不锈钢304",null,"不锈钢304"]
["D00125B006BA00000",110,"DIN125B","M6","不锈钢304",null,"不锈钢304","140HV"]
["D00125A016AKHV140",110,"DIN125A","M16","碳钢",null,"三价锌","140-250HV"]
["D00127B006CA00000",110,"DIN127B","M6","不锈钢316",null,"不锈钢316"]
["D006796010MG00000",110,"DIN6796","M10","65锰",null,"达克罗500无红","420-490HV"]
["F0000000024M70270",110,"24M7027","5.3*10*1","Q235",null,"三价锌TNTUV12/144/5","200-300HV"]
["X020000M06ZN25514",110,"NFE25-514Z","M6","碳钢","NULL","灰色锌镍150无红","200-300HV"]
["F0122X26X32GK0000",108.49,"DJ222012-TZ","12.2*26*3.2","45#钢","NULL","三价锌 48无白5um ","HRC39-43 "]
["ISO7092010AAHV200",108,"ISO7092","M10","碳钢",null,"三价锌12/36/5","200-300HV"]
["X06798A003BA00000",108,"DIN6798A","M3","不锈钢304","NULL","不锈钢304","NULL"]
["D006796008GI00000",107.5,"DIN6796","M8","65锰","NULL","机械镀锌48/72/8","420-490HV"]
["F014X27X4GL000000",106.5,"110181751（原12601-02167）","14*27*4","45#钢","NULL","三价彩锌96/120/8","HRC38-45"]
["G009387003ID00000",106,"GB93-87","M3","65锰",null,"发黑","42-50HRC"]
["XNFE25-51106AA316",105.9,"PW730-2","M6/NFE25-511M","不锈钢316",null,"不锈钢316","270-335HV"]
["D007349010AKHV140",105.5,"DIN7349","M10","碳钢","NULL","三价锌","140HV"]
["F000000000T209296",105.25,"T209296","17.35*38.1*2.769","45#","NULL","热处理本色","36-48HRC"]
["0861287008MI0000",105,"GB861.2-87","M8","65锰","NULL","机械镀锌24/96","HRC43-50"]
["XXT0000182",105,"N402AP11","N402AP11","不锈钢304","NULL","本色","NULL"]
["F062X18X08MD00000",105,"BN806 1282581","6.2*18*0.8","50CrV4","NULL","黑磷化","锥垫"]
["A300004812",104.6,300004812,"N405P39B13","65Mn","NULL","三价锌72无红5um"]
["F53X12X015CA200HV",104.2,"5.3*12*1.5","5.3*12*1.5","不锈钢316",null,"不锈钢316","200-300HV"]
["F00000000024M7396",104.1,"24M7396","24*34*3","35#钢","NULL","机械镀锌48/96/8","300-370HV"]
["G009685010AAHV140",104,"GB96-85","M10","碳钢",null,"本色","140-250HV"]
["X0100000M6MR25511",104,"NFE25-511S","M6","65锰","NULL","环保达克罗1000无红","NULL"]
["F53X26X19X2GA0000",102.83,"200-1(矩DQ)","5.3*26*19*2","50#钢","NULL","热处理本色","360-430HV"]
["XXT0000217",102.5,"10.5*22*.3.2","10.5*22*.3.2","SPCC","NULL","三价锌TNTUV12/144/5um","不热处理"]
["F00000P6$9AA00000",102.5,"PW6-9","5.5*26*2","A3普碳钢",null,"本色"]
["ISO7089M08AKHV200",102,"ISO7089","M8","碳钢","NULL","三价锌72无白8um","200-300HV"]
["D006796008MD00000",101.6,"DIN6796","M8","65锰","NULL","发黑","420-490HV"]
["D00137B005MI00000",101,"DIN137B","M5","65锰",null,"机械镀锌24无白"]
["00000001$2MI00000",100.8,"美制标型准弹垫","'1/2","65锰","NULL","机械镀锌","HRC38-46"]
["X0000000M16BA2551",100.4,"NFE25-511M","M16","不锈钢304","NULL","不锈钢304","NULL"]
["NFE25$513M04AN000",100,"NFE25-513M","M4","碳钢","NULL","灰色锌镍72无白5um","100HV"]
["X00SN70093005MI00",100,"SN70093","M5","65锰",null,"机械镀锌不上封闭Oil  WD40","440-520HV"]
["X06797A003CA00000",100,"DIN6797A","M3","不锈钢304","NULL","不锈钢304","NULL"]
["X06798A008MK07200",100,"DIN6798A","M8","65锰","NULL","三价锌72无红5um","350-425HV"]
["G009685004AA00000",100,"GB96-85","M4","碳钢",null,"本色"]
["G971002M04AA200HV",100,"GB97.1-2002","M4","碳钢",null,"本色","200-300HV"]
["F00602801PW0101TO",100,"PW0101-11","4.1*8*0.8(非标六足）","65锰","NULL","达克罗三涂三烘+封闭96/500/12","HRC42-47"]
["F0024481AW0170011",100,"AW017-1","5.53*18.5*1.2","碳钢","NULL","本色","NULL"]
["F0182X36X45MK0000",99.4,"DJ222018-TZ","18.2*36*4.5","45#钢",null,"三价锌","HRC39-45"]
["D00127B012ID00000",99,"DIN127B","M12","弹簧钢",null,"发黑"]
["D00128A003MR00000",99,"DIN128A","M3","弹簧钢",null,"环保达克罗500无红","44-51HRC"]
["G009387006ID00000",99,"GB93-87","M6","65锰",null,"发黑","42-50HRC"]
["F013X30X4CA000000",98.28,"BN91170/3697940","13*30*3","不锈钢316",null,"不锈钢316"]
["F00L400P30AK00000",98.18,"3810R.100.001.C96","L400P30","碳钢","NULL","三价彩锌96无红","NULL"]
["D006796012BA00000",98,"DIN6796","M12","不锈钢304",null,"不锈钢304"]
["ISO7089010RG300HV",98,"ISO7089","M10","45#钢",null,"环保达克罗720无红","300-370HV"]
["F00000000024M756",97.5,"24M7546","8.4*25*2","1035钢","NULL","环保达克罗960无红","300-370HV"]
["F0055X122X001CA00",96.9,"BN91170   6145697","5.5*12.2*1","不锈钢316",null,"不锈钢316","200-300HV"]
["ISO7093M12AL200HV",96.3,"ISO7093","M12","碳钢",null,"三价锌48/72/5","200-300HV"]
["G085987005II00000",96,"GB859-87","M5","70#钢",null,"机械镀锌","72无白72无红"]
["D10125A012AKHV200",96,"DIN125A","M12","碳钢",null,"三价锌48/72/5","200-250HV"]
["D00127B008IK00000",96,"DIN127B","M8","弹簧钢",null,"三价锌"]
["F0225X44X6GK00000",95.1,"DJ222022-TZ","22.5*44*6","45#钢","NULL","三价锌48无白5um ","HRC39-43 "]
["DIN127B005IR01000",95,"DIN127B","M5","弹簧钢","NULL","黑色环保达克罗500无红","NULL"]
["X00862.2-87010MB0",94.7,"GB862.2-87","M10","65锰",null,"镀锌","西门子"]
["G009685010AGHV200",93.6,"GB96-85","M10","碳钢",null,"达克罗500无红","200-300HV"]
["D00127B005IB00000",93.4,"DIN127B","M5","弹簧钢",null,"镀锌"]
["DIN9021M10AL200HV",93.1,"DIN9021","M10","碳钢",null,"三价彩锌72/120/8上封闭","200-300HV"]
["DIN433M008AK140HV",93,"DIN433","M8","碳钢",null,"三价锌48/72/5","140-250HV"]
["F000000024H172200",92.5,"24H1722","24H1722","Q235B","NULL","三价锌TNTUV12/144/5","＜302HV"]
["F0084X16X015RT000",92,"BN90701 6147451","8.4*16*1.5(8/125A)","碳钢","NULL","黑色环保达克罗500无红","200HV"]
["XXT0000314",92,"DIN125A","M4","Q235","NULL","三价锌8um","140HV"]
["F053X15X2GA000000",91.7,"200-2(圆DQ)","5.3*15*2","50#钢","NULL","热处理本色","360-430HV"]
["A000000008AA00000",91,"美制平垫","8#","碳钢","NULL","本色上油","NULL"]
["F0142X25X42GI0000",90.9,"T215873","14.2*25*4.2","45#钢","NULL","机械镀锌48/96/8","HRC39-45"]
["GB972002M16AK0000",90.6,"GB97.1-2002","M16","碳钢","NULL","三价锌48/72/5","200-300HV"]
["F01905X334X3K0000",90.42,"'03040207","5/8(19.05*33.4*3)","Q235B",null,"三价锌72/120/8"]
["F0129X30X3GA300HV",90.19,"P1J1430030-00","12.9*30*3","45#钢",null,"热处理本色","300-370HV"]
["F000000000R232527",90.09,"R232527","R232527","45#钢","NULL","机械镀锌48/96/8","300-370HV"]
["F000024M7226GG000",90,"24M7226","13*35*5","45#钢",null,"机械镀锌48/96/8"]
["F020X40X6GK000000",90,"XJ222020-TZ","20*40*6","45#钢","NULL","三价锌48无红5um"," HRC39-43"]
["A00005$16NAC00000",90,"美制N型","5/16N","碳钢","NULL","黄锌","NULL"]
["DIN134M008AK200HV",90,"DIN134","M8","碳钢","NULL","三价锌72无白8um","200-250HV"]
["ISO7089M05AK200HV",90,"ISO7089","M5","碳钢","NULL","三价锌48/72/5","200-300HV"]
["ISO7089M03AN200HV",90,"ISO7089","M3","碳钢","NULL","灰色锌镍96/150","200-300HV"]
["X000000M08MC25514",89,"NFE25-514M","M8","碳钢",null,"黄锌","160HV"]
["A00003$8BA0000000",89,"美制标准型弹垫","'3/8","不锈钢304","NULL","不锈钢304(钝化)","NULL"]
["D000433005AKHV140",88,"DIN433","M5","碳钢","NULL","三价锌8un","140-250HV"]
["D00125B006CA00000",88,"DIN125B","M6","不锈钢316",null,"不锈钢316","140HV"]
["F011X22X32GK00000",88,"110181750（原12601-01621）","11*22*3.2","45#钢","NULL","三价彩锌上封闭96/120/8","HRC38-45"]
["DIN6796M08NJ00000",88,"DIN6796","M8","50CrV4","NULL","机械黄锌96/144/12","420-490HV"]
["ISO7089M05AN200HV",88,"ISO7089","M5","碳钢","NULL","灰色锌镍96/150","200-300HV"]
["F043010008BA00000",88,"4.3*10*0.8","4.3*10*0.8","不锈钢304",null,"不锈钢304"]
["D00125A016AL008UM",87.3,"DIN125A","M16","碳钢",null,"三价彩锌 120/360/8","140-250HV"]
["D00125A004BAHV200",87,"DIN125A","M4","不锈钢304",null,"不锈钢304","200HV"]
["F0000000MK1000000",87,"美制标准弹垫","10#","65锰",null,"机械镀锌5um"]
["X0200000M6MG25511",87,"PW657-2","M6/NFE25-511M","65锰","NULL","达克罗三涂三烘+封闭96/500/12","420-470HV"]
["X000SN70093012MR0",86.4,"SN70093","M12","65锰",null,"环保达克罗500无红","440-520HV"]
["X00000M12MG2551F",86.3,"NFE25-511M","M12","65锰","NULL","上海环保达克罗500无红","NULL"]
["F002677PW11440011",86.22,"PW1144-1","20.6*38*6","45#钢",null,"不热处理本色"]
["F000000024H134100",86,"24H1341","0.531*0.938*0.06","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["F0064X016X016AK00",85.5,"BN737/1271091","6.4*16*1.6","A3普碳钢","内销柏中 马来西亚","三价锌140HV","NULL"]
["ISO7093M06AK100HV",85.5,"ISO7093-2","M6","碳钢",null,"三价锌12/36/3","100HV"]
["F00025661PW722011",85,"PW722-4","4.46*14.48*1.14","SPCC",null,"本色"]
["D007349004AKHV200",85,"DIN7349","M4","碳钢","NULL","三价锌","200HV"]
["F013X34X03BA200HV",84.88,"BN91170 6166324","13*34*3","不锈钢304",null,"不锈钢304","200-300HV"]
["F002362AW004200H1",84.85,"AW0042-H-1","6.3*14*2","45#钢",null,"热处理本色","HRC40-44"]
["F64X14X12BA000000",84.5,"BN91170/3365517","6.4*14*1.2","不锈钢304",null,"不锈钢304"]
["DIN6796016GG012UM",84.38,"DIN6796","M16","50CrV4","NULL","达克罗三涂三烘+封闭96/500/12","420-490HV"]
["D00127B008IK005UM",84,"DIN127B","M8","弹簧钢",null,"三价锌48/72/5"]
["A200004915",84,200004915,"DIN125A M6","碳钢",null,"蓝白锌5um+封闭96/0","200-250HV"]
["F00022X035X035GA3",83.27,"DQ130428(A3)","22*35*3.5","45#钢",null,"不热处理本色上油"]
["F625018001AA00000",82.6,"PW149-3","6.4*18*1","碳钢","NULL","本色","NULL"]
["G009685012ABHV140",82.4,"GB96-85","M12","碳钢",null,"镀锌","140-250HV"]
["F0013X22X05AK0000",82.1,"BN90701 6304955","13*22*0.5","碳钢",null,"三价彩锌24/48/3上封闭","DIN522A"]
["D00125B005ALHV200",82,"DIN125B","M5","碳钢",null,"三价锌3um","200-250HV"]
["DIN1440M06AH00000",82,"DIN1440","M6","碳钢",null,"三价黑锌","160-250HV"]
["G001230020GG00720",81.95,"GB1230","M20","45#钢","NULL","达克罗720无红","NULL"]
["G009785024AA140HV",81.94,"GB97-85","M24","碳钢","NULL","本色","140-250HV"]
["F010X021X002AA000",81.599999999999994,26011306,"10*21*2（10/97-76）","A3普碳钢","NULL","本色","昇沪"]
["ISO7089M06AN005UM",81.5,"ISO7089","M6","碳钢",null,"三价黑锌120/144/5","200-300HV"]
["F043X10X08SK00000",81.5,"BN20229/3370273","4.3*10*0.8","碳钢","NULL","三价锌72/150/5","100-200HV"]
["G084885012ACHV200",81,"GB848-85","M12","碳钢",null,"镀锌","200-300HV"]
["XXT0000241",81,"GB97-85","M10","Q235","NULL","三价锌72/144/5um","200HV"]
["D000433004BA00000",81,"DIN433","M4","不锈钢304",null,"不锈钢304"]
["F002677PW122500H1",80.5,"PW1225-H-1","17*32*3.5","45#钢",null,"热处理本色上油","HRC36-42"]
["ISO7089M12AL200HV",80.5,"ISO7089","M12","碳钢",null,"三价彩锌72/120/8上封闭","200-300HV"]
["ISO7089M12RR200HV",80.5,"ISO7089","M12","碳钢",null,"环保达克罗720无红","200-300HV"]
["F7371271113BK0000",80.099999999999994,"BN737/1271113","8.4*20*2","碳钢","NULL","三价锌","NULL"]
["D00125A004AKHV140",80,"DIN125A","M4","碳钢",null,"三价锌","140-250HV"]
["D00125A008BA00000",80,"DIN125A","M8","不锈钢304","NULL","不锈钢304","140HV"]
["DIN127BM03HA00000",80,"DIN127B","M3","黄铜","NULL","黄铜","NULL"]
["D006796003MN00000",80,"DIN6796","M3","50CrV4","NULL","黑磷化","420-490HV"]
["D00128A006MI00000",79.900000000000006,"DIN128A","M6","弹簧钢",null,"机械镀锌","44-51HRC"]
["D009021005AKHV140",79.8,"DIN9021","M5","碳钢",null,"三价锌","140-250HV"]
["G009685014AGHV200",79.599999999999994,"GB96-85","M14","碳钢",null,"达克罗500无红","200-300HV"]
["D009021006CA00000",79.5,"DIN9021","M6","不锈钢316",null,"不锈钢316"]
["XXT0000010",79.34,"BN45719 3331310","24H1347","Q235","NULL","三价锌TNTUV","NULL"]
["F00011808350176BA",79,"非标开口弹垫","8.35*11.8*1.76","不锈钢304","NULL","不锈钢304","NULL"]
["F00000000024M7463",78.900000000000006,"24M7463","6.4*18*1.6(6/9021)","Q235","NULL","环保达克罗960无红","200-300HV"]
["D00127B005IR00500",78.75,"DIN127B","M5","弹簧钢",null,"环保达克罗500无红"]
["GB5287M06AK000000",78.5,"GB5287","M6","碳钢",null,"三价锌72/144/5","100-200HV"]
["G009785010ABHV140",78,"GB97-85","M10","碳钢",null,"镀锌","140-250HV"]
["F064X25X18AK00000",78,"6.4*25*1.8","6.4*25*1.8","Q235",null,"三价锌3um","140HV"]
["XXT0000014",77.900000000000006,"24M7055","24M7055","Q235","NULL","三价锌TNTUV","NULL"]
["D006799008MD00000",77.78,"DIN6799","M8","65锰",null,"发黑"]
["D009021003BA00000",77.2,"DIN9021","M3","不锈钢304",null,"不锈钢304"]
["XXT0000007",77,"DIN125A","M5","Q235","NULL","达克罗1000无红","238.5-247.4HV"]
["F0065X018X002AL00",76.7,"BN90701   6130277","6.5*18*2","碳钢","NULL","三价彩锌72/144/8","NULL"]
["DIN2093AM10MN0000",76.5,"DIN2093A","20*10.2*1.1","50CrV4","NULL","黑磷化","NULL"]
["G009785016ABHV140",76.400000000000006,"GB97-85","M16","碳钢",null,"镀锌","140-250HV"]
["G001230022GG00720",76,"GB1230","M22","45#钢","NULL","达克罗720无红","NULL"]
["ISO7089M3X5AK0000",76,"ISO7089","M3.5","碳钢","NULL","三价锌96无红","200-300HV"]
["NFE25514LM05AN000",76,"NFE25-514L","M5","碳钢","NULL","灰色锌镍150无红","160-250HV"]
["A200002858",75.5,200002858,"DIN127B M10","弹簧钢",null,"机械镀锌","44-51HRC"]
["ISO7089M10GR200HV",75,"ISO7089","M10","碳钢","NULL","上海环保达克罗600无红","200-300HV"]
["ISO7093M06BA200HV",75,"ISO7093","M6","不锈钢304",null,"不锈钢304","200HV"]
["G0097X4008AK00000",75,"GB97.4S","M8","碳钢","NULL","三价锌24/72","200HV"]
["ISO7089A08ARHV200",75,"ISO7089","M8","碳钢",null,"环保达克罗720无红","200-300HV"]
["D006796012ME00000",74.95,"DIN6796","M12","65锰",null,"黑磷化","420-490HV"]
["F00024H1622AK0000",74.650000000000006,"24H1622","0.375*0.875*0.12","Q235B",null,"三价锌TNTUV12/144/5","<302HV"]
["D009021005AKHV200",74.5,"DIN9021","M5","碳钢",null,"三价锌","200-250HV"]
["D00006340016GG0000",74.099999999999994,"DIN6340","M16","45#钢","NULL","达克罗500无红","350-430HV"]
["GB97850M05AM200HV",74,"GB97-85","M5","碳钢",null,"三价锌72/144/5","200-300HV"]
["G009785010GD00000",74,"GB97-85","M10","45#钢",null,"发黑","300-370HV"]
["A000003$8NAAHV140",73.7,"美制N型","3/8N","碳钢","NULL","本色","140HV"]
["D00137B012MR10000",73.599999999999994,"DIN137B","M12","65锰","NULL","上海环保达克罗500无红(Deltaton)","NULL"]
["F0000AAL400P12000",73.400000000000006,"BN91170 6130883","L400P12","不锈钢304",null,"不锈钢304"]
["DIN128A016MR00000",73,"DIN128A","M16","弹簧钢",null,"环保达克罗500无红","44-51HRC"]
["XXT0000216",72.52,"GB97-85","M20","Q235","NULL","本色","100HV"]
["F00000000024M7299",72.25,"24M7299","10.5*30*2.5（10/9021）","Q235B","NULL","三价黑锌TNTUV12/144/5","200-300HV"]
["F0000000024M72510",72.2,"24M7251","6.4*18*1.6","碳钢",null,"三价黑锌TNTUV12/144/5","200-300HV"]
["D006796005ML00000",72,"DIN6796","M5","65锰","NULL","机械镀锌","420-490HV"]
["DIN6796016MR00000",71.459999999999994,"DIN6796","M16","50CrV4",null,"环保达克罗500无红","420-490HV"]
["F021X40X45GK00000",71.3,"500093431(原D4018545-TZ）","21*40*4.5","45#钢","NULL","三价锌48无白5um ","HRC39-43 "]
["G009685010AAHV200",71.3,"GB96-85","M10","碳钢",null,"本色","200-300HV"]
["X0000000M03BA2551",71,"NFE25-511M","M3","不锈钢304",null,"不锈钢304"]
["F00000000024M7518",71,"24M7518","6.4*12*1.6(6/125A)","Q235","NULL","环保达克罗960无红","200-300HV"]
["F000000000N280653",70.84,"N280653","0.656X1.25X0.125","45#",null,"热处理本色","HRC32-42"]
["ISO7089M12AT300HV",70.7,"ISO7089","M12","45#钢",null,"黑色锌镍8um","300-370HV"]
["F0000000LVU229010",70.12,"LVU22901","14*38*2.5","Q235B","NULL","三价黑锌TNTUV 12/144/5","200-300HV"]
["X000000M06MI25511",70.099999999999994,"NFE25-511M","M6","65锰",null,"机械镀锌","锥形压花垫"]
["G009685005AB200HV",70,"GB96-85","M5","碳钢",null,"镀锌","200-300HV"]
["DIN125AM06AGHV200",70,"DIN125A","M6","碳钢","NULL","环保达克罗720无红","200-250HV"]
["A000001$2NAK0000F",70,"美制非标平垫","0.406*1.25*0.071","Q235",null,"三价锌96无红","200HV"]
["A000003$8NBA00000",69.900000000000006,"美制N型","3/8N","不锈钢304",null,"不锈钢304"]
["A300001168",69.599999999999994,300001168,"非标平垫 13*25*3","45#",null,"机械镀锌8um,摩擦系数0.14-0.248/96","300-370HV"]
["G009785014AGHV200",69.599999999999994,"GB97-85","M14","碳钢",null,"达克罗500无红","200-300HV"]
["X000000M10MC25514",69.5,"NFE25-514M","M10","碳钢",null,"黄锌","160HV"]
["A200002848",69.5,200002848,"DIN127B M8","弹簧钢",null,"机械镀锌","44-51HRC"]
["F00011X28X4MA0000",69.099999999999994,"P1I1228040-00","11*28*4","35#钢",null,"热处理本色","300-390HV"]
["F0000000MH06012UM",69,"美制标准弹垫","6#","65锰","NULL","三价彩锌96/144/12","NULL"]
["000000000AKN402P9",69,"BN90701 6074805","N402P9B13","碳钢","NULL","三价锌72无红5um","NULL"]
["D00127B006ID00000",69,"DIN127B","M6","弹簧钢",null,"发黑"]
["F0000000024H13020",68.900000000000006,"24H1302","0.406*0.688*0.035","Q235B",null,"三价锌TNTUV 12/144/5","＜302HV"]
["G009387012IK00000",68.5,"GB93-87","M12","65锰",null,"三价锌","42-50HRC"]
["B00KAR4102MG00000",68.400000000000006,"NTSKAR41-05","弹簧螺母","65锰","NULL","达克罗","NULL"]
["F0000008X31x6X1x5",68.3,"8.5*31.6*1.5","8.5*31.6*1.5","A3普碳钢",null,"本色","深圳昇沪"]
["F084X18X16AK200HV",68,"BN90701 6297322","DIN522A 8.4*18*1.6","碳钢",null,"三价锌","200HV"]
["G009685005AC200HV",68,"GB96-85","M5","碳钢",null,"黄锌","200-300HV"]
["ISO07093M6AR200HV",68,"ISO7093","M6","碳钢",null,"环保达克罗720无红摩擦0.15-0.21","200-300HV"]
["X000SN70093008MI0",68,"SN70093","M8","65锰",null,"机械镀锌","440-520HV"]
["X00125A006BA140HV",68,"DIN125A","M6","不锈钢304",null,"不锈钢304 140HV","西门子"]
["XXT0000013",67.84,"NULL","NULL","NULL","NULL","NULL","NULL"]
["F05$16X075BA00000",67.7,"BN91170/3868170","5/16*0.75","不锈钢304",null,"不锈钢304","原BN91170/3757727"]
["XXT0000057",67.599999999999994,"NULL","NULL","NULL","NULL","NULL","NULL"]
["F291062073BA00000",67.5,"BN91170   6056053","0.291*0.62*0.073","不锈钢304","NULL","不锈钢304 钝化","NULL"]
["F0000000AK24M7250",67.2,"24M7250","M6.4*17*3","Q235",null,"三价锌TNTUV12/144/5","200-300HV"]
["X000000M04MI25511",67,"NFE25-511M","M4","65锰",null,"机械黄锌"]
["NF25514M04AN0000M",67,"NFE25-514M","M4","碳钢","NULL","灰色锌镍150无红"," 160-250HV"]
["D00127B008ID00000",66.8,"DIN127B","M8","弹簧钢","NULL","发黑","NULL"]
["DIN125AM06AN140HV",66.7,"DIN125A","M6","碳钢","NULL","黑色锌镍","140-250HV"]
["F00224X45X25MH000",66.69,"VF200660","22.4*45*2.5","65锰",null,"黑磷化","等温热处理420-490HV"]
["F000010X016X005000",66.5,"BN90701   6109333","10*16*0.5","碳钢","NULL","发黑","HRC40-50"]
["X06797A006MA00000",66,"DIN6797A","M6","65锰","NULL","热处理本色","350-425HV"]
["F0013X32X3AK140HV",65.900000000000006,"BN90701   6043501","13*32*3","碳钢",null,"三价锌6/24/3","140HV"]
["F00438X001X0083AK",65.8,"0.438*1*0.083","0.438*1*0.083","A3普碳钢",null,"三价锌","内销柏中"]
["F0000000024H18600",65.8,"24H1860","0.781*1.25*0.06","Q235B","NULL","三价锌TNTUV12/144/5","＜302HV"]
["F000000024M710600",65.37,"24M7106","10*18*2.5","Q235",null,"三价锌TNTUV12/144/5","160HV"]
["DIN6797JM08MK0000",65,"DIN6797J(8齿）","M8","65锰","NULL","三价彩锌48/72/3","HRC40-50"]
["X0L0000M05MC25514",65,"NFE25-514L","M5","碳钢",null,"黄锌","160HV"]
["F085X020X025AA000",65,"8.5*20*2.5","8.5*20*2.5","A3普碳钢",null,"本色","昇沪"]
["F064X19X2AK000000",65,"6.4*19*2","6.4*19*2","碳钢","NULL","三价锌","140HV"]
["ISO7093005CAHV200",64.8,"ISO7093","M5","不锈钢316",null,"不锈钢316","200HV"]
["ISO7093M08AR200HV",64.5,"ISO7093","M8","碳钢","NULL","环保达克罗 720无红,0.15-0.21摩擦","200-300HV"]
["F102X22X32GK00000",64.400000000000006,"XJ222010-TZ","10.2*22*3.2","45#钢",null,"三价锌 48无白5um","HRC39-46"]
["F025X122X15GN0000",64.3,"DIN2093A","25*12.2*1.5","50CrV4","NULL","黑磷化","NULL"]
["F02677PW1136000H1",64,"PW1136-2","3.4*7.0*0.8","45#钢",null,"热处理本色","HRC36-42"]
["D00128A012MG00000",63,"DIN128A","M12","弹簧钢",null,"达克罗","44-51HRC"]
["XXT0000049",63,"GB848-85","M6","45#","NULL","本色","300HV"]
["XXT0000325",62.637999999999998,"GB97.1-2002","M48","Q235","NULL","环保达克罗0/720","140HV"]
["F0000000L400P27K0",62.6,"BN90701 6207342","L400P27","碳钢",null,"三价彩锌48/72/5","140HV"]
["GB09387010MC00000",62.3,"GB93-87","M10","65锰",null,"黄锌48/72/5","42-50HRC"]
["ISO7089M10AA200HV",62,"ISO7089","M10","碳钢",null,"本色","200-300HV"]
["D10127B004CA00000",62,"DIN127B","M4","不锈钢316",null,"不锈钢316"]
["D007980006BA00000",61.9,"DIN7980","M6","不锈钢304",null,"不锈钢304"]
["FMGBN907046140862",61.7,"BN90704 6140862","10#锥垫","65锰",null,"环保达克罗","500无红"]
["G009785012GD00000",61.5,"GB97-85","M12","45#钢",null,"发黑","300-370HV"]
["GB09387008IK00000",61,"GB93-87","M8","65锰",null,"三价锌48无红5um","42-50HRC"]
["ISO7089A08GRHV300",61,"ISO7089","M8","45#钢",null,"环保达克罗720无红","300-370HV"]
["F084X15X05AL00000",61,"BN90701 6248189","8.4*15*0.5","碳钢",null,"三价彩锌72/120/5上封闭","按SN60007"]
["F0010501PW69700HL",61,"PW697-2","M4非标外锯齿锁紧垫（12齿）","65锰","NULL","热处理本色","400-480HV"]
["ISO7094006AN00000",60.9,"ISO7094","M6","低碳钢",null,"三价黑锌","100-200HV"]
["A300003742",60.84,300003742,"5/16美制非标平垫 8.64-9.09*17.8-18.2*1.8-2.2","碳钢",null,"六价彩锌3um"]
["ISO7092M08BA00000",60.35,"ISO7092","M8","不锈钢304","NULL","不锈钢304","200HV"]
["ISO7089M08AN200HV",60,"ISO7089","M8","碳钢","NULL","灰色锌镍96/150","200-300HV"]
["D00127B003CA00000",60,"DIN127B","M3","不锈钢316",null,"不锈钢316"]
["D00125A008ARHV300",60,"DIN125A","M8","45#钢",null,"上海环保达克罗,500无红","300-400HV"]
["D00125A012ALHV200",60,"DIN125A","M12","碳钢",null,"三价彩锌72/144/8","200-250HV"]
["F0000P8$12AA00000",60,"PW8-12","7.4*22*3.2","A3普碳钢",null,"本色"]
["D007349016AA00000",59.97,"DIN7349","M16","碳钢","NULL","本色","140HV"]
["F003046PW14370011",59.8,"PW1437-1","0.5*0.87*0.115","铝（5052H32）","NULL","本色","NULL"]
["G009387016ID00000",59.8,"GB93-87","M16","65锰",null,"发黑","42-50HRC"]
["GB97850M14AM200HV",59.6,"GB97-85","M14","碳钢",null,"三价锌72/144/5","200-300HV"]
["A0000001$4MI00000",59.6,"美制标准型弹垫","'1/4","65锰",null,"机械镀锌5um"]
["F0000AKN405P45B43",59.3,"BN90705 6074870","N405P45B43","65锰",null,"三价锌 72无红5um"]
["G009785024AA00000",59.07,"GB97-85","M24","碳钢",null,"本色"]
["G084885006AA00000",59,"GB848-85","M6","碳钢",null,"本色"]
["G009387005ID00000",59,"GB93-87","M5","65锰",null,"发黑","42-50HRC"]
["FBN90705614089900",59,"BN90705 6140899","1/4锥垫","65锰",null,"环保达克罗","500无红"]
["G009387006IG00000",59,"GB93-87","M6","65锰",null,"达克罗500无红","42-50HRC"]
["XXT0000224",59,"DIN127B","M8","65Mn","NULL","灰色锌镍去氢0/1008/12um","44-51HRC"]
["D00127B006IG05000",59,"DIN127B","M6","弹簧钢","NULL","黑色环保达克罗500无红","NULL"]
["D007980008II00000",59,"DIN7980","M8","弹簧钢",null,"机械镀锌"]
["D007980008IR00000",59,"DIN7980","M8","弹簧钢",null,"环保达克罗720无红"]
["DIN127BM06IL008UM",59,"DIN127B","M6","弹簧钢","NULL","三价彩锌72/216/8","NULL"]
["F0000000AK24H1887",58.8,"24H1887","0.344*1*0.134","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["DIN127BM010IR0720",58.5,"DIN127B","M10","弹簧钢","NULL","环保达克罗720无红","NULL"]
["F0026X044X004GA04",58.49,"DQ130033(A4)","26*44*4","45#钢",null,"不热处理本色上油"]
["NFE25511MM06MG000",58.1,"NFE25-511M","M6","65锰","NULL","环保达克罗1000无红","NULL"]
["D007980006IK005UM",58,"DIN7980","M6","弹簧钢",null,"三价锌5um"]
["D000126012AAHV100",57.8,"DIN126","M12","碳钢",null,"本色","100-250HV"]
["G001230012GG00720",57.5,"GB1230","M12","45#钢","NULL","达克罗720无红","NULL"]
["G009387012IG00000",57.5,"GB93-87","M12","65锰","NULL","达克罗500无红","42-50HRC"]
["ISO7093005BNHV200",57.3,"ISO7093","M5","不锈钢304",null,"不锈钢304 钝化","200HV"]
["F0000000024M72600",57.3,"24M7260","8.4*24*2（8/9021）","Q235B",null,"三价黑锌TNTUV12/144/5","200-300HV"]
["G0097x4008BA00000",57.1,"GB97.4N","M8","不锈钢304",null,"不锈钢304"]
["G009685006CA00000",57,"GB96-85","M6","不锈钢316",null,"不锈钢316"]
["XT0000187",57,"10*16*0.5","10*16*0.5","Q235","NULL","发黑","NULL"]
["A300002605",57,300002605,"5*20*1.0","Q235",null,"蓝白锌6/24","140HV"]
["D00125A004AL008UM",57,"DIN125A","M4","碳钢",null,"三价彩锌72无白5um","140-250HV"]
["GB862287M8MD00000",56.8,"GB862.2-87","M8","65锰","NULL","热处理发黑","HRC40-50"]
["F0000000024M74340",56.7,"24M7434","24M7434","1035钢",null,"机械镀锌48/96/8","300-370HV"]
["DIN7349012ANHV140",56.6,"DIN7349","M12","碳钢",null,"环保达克罗720无红0.15-0.21摩擦","140HV"]
["F0011X30X6MA00000",56.54,"P1N1230060-00-DQ","11*30*6","65锰",null,"不热处理本色"]
["F0060281PW65702TO",56.5,"PW657-2","M12(12.4*24*1.8)","65锰",null,"达克罗三涂三烘+封闭96/500/12"]
["G009785016AAHV300",56.4,"GB97-85","M16","45#钢",null,"本色","300-370HV"]
["G009785020GG00000",56.2,"GB97-85","M20","45#钢",null,"达克罗500无红","300-370HV"]
["A300000395",56,300000395,"8.4*20*2","304不锈钢",null,"本色","200-300HV"]
["D000433004BAHV200",56,"DIN433","M4","不锈钢304",null,"不锈钢304","200HV"]
["G907426012IA00000",55.8,"GB9074.26","M12","70#钢",null,"本色"]
["F025X0562X0065000",55.7,"BN90701   6162276","0.25*0.562*0.065","碳钢","NULL","三价黑锌5um","NULL"]
["XM05000BA25514M00",55.5,"NFE25-514M","M5","不锈钢304",null,"不锈钢304","160-250HV"]
["NFE25$513M8AG0000",55.5,"NFE25-513L","M8","碳钢",null,"达克罗","200HV"]
["D00125A010BAHV200",55.4,"DIN125A","M10","不锈钢304",null,"不锈钢304","200HV"]
["D00125A006CAHV200",55.3,"DIN125A","M6","不锈钢316",null,"不锈钢316","200HV"]
["X000000M04MK25511",55,"NFE25-511M","M4","65锰","NULL","机械镀锌","NULL"]
["XXY0000279",55,"NFE25-511M","M4","Q235","NULL","机械镀锌","NULL"]
["G009685006AB00000",55,"GB96-85","M6","碳钢",null,"镀锌"]
["F0BN48367$3401291",55,"BN48367/3401291","0.312*0.75*0.063","碳钢","NULL","三价锌","NULL"]
["D007980010ID00000",54.8,"DIN7980","M10","弹簧钢",null,"热处理发黑","HRC42-50"]
["F009X20X16AK140HV",54.6,"9*20*1.6","9*20*1.6","碳钢","NULL","三价锌48/72/5","140HV"]
["A200001599",54.2,200001599,"DIN6796 M8","65Mn",null,"机械镀锌","420-490HV"]
["F0162X225X012AK00",54.16,"24H1929","1.62*2.25*0.12","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["F01N7089M8000001B",54,"ISO7089","M8","碳钢",null,"镀锌48/72/5","200-300HV"]
["DIN0433M10AKHV200",54,"DIN433","M10","碳钢",null,"三价锌","200-300HV"]
["F016022005AA00000",53.9,"DIN988","16*22*0.5","碳钢","NULL","本色","NULL"]
["ISO7089M10ARHV200",53.5,"ISO7089","M10","碳钢",null,"达克罗1000无红","200-300HV"]
["D006916016GD00000",53.44,"DIN6916","M16","45#钢",null,"发黑","300HV"]
["F06A82110200000HL",53.4,"美制标准外齿锁紧垫","'1/4","65锰","NULL","热处理本色","HRC40-50"]
["G009785016GD00000",53.2,"GB97-85","M16","45#钢",null,"发黑","300-370HV"]
["F0000000AK24H1106",53.1,"24H1106","0.688*1.75*0.34","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["A00005$16WAKHV200",53,"美制W型","5/16W","碳钢",null,"三价锌96无红","200HV"]
["D00127A008MG00000",53,"DIN127A","M8（代加工）","弹簧钢","NULL","机械镀锌","NULL"]
["F0528X1902X16AK00",53,"5.28*19.02*1.6","5.28*19.02*1.6","碳钢","NULL","三价锌96无红","NULL"]
["F6X4X015X1X8HV140",53,"BN90701   6009327","6.4*15*1.8","碳钢","NULL","三价锌","140HV"]
["F00024M7616GR0000",52.86,"24M7616","9*16*1.6","35#钢","NULL","环保达克罗960无红","300-370HV"]
["ISO70932M8GRHV200",52.8,"ISO7093","M8","碳钢","NULL","环保达克罗720无红","200-300HV"]
["ISO7093M06BA00000",52.8,"ISO7093","M6","不锈钢304",null,"不锈钢304 钝化","200HV"]
["XXT0000056",52.8,"NULL","NULL","NULL","NULL","NULL","NULL"]
["F0162X32X45MK0000",52.7,"500093655（原DJ222016-TZ）","16.2*32*4.5","45#钢","NULL","三价锌48无白5um","HRC39-45"]
["DIN125AM08AKHV200",52.6,"DIN125A","M8","碳钢","NULL","三价锌72/96/8","140-250HV"]
["NFE25$511024MG000",52.6,"JB/ZQ4340","M24","65锰",null,"达克罗"]
["G009785020ACHV140",52.6,"GB97-85","M20","碳钢",null,"镀锌","140-250HV"]
["XXT0000047",52.5,"ISO7089","M10","65Mn","NULL","热锌","300HV"]
["F00000000G24M7547",52.5,"24M7547","21*34*3","35#钢",null,"环保达克罗960无红","300-370HV"]
["GB962002012AA0000",52.4,"GB96.1-2002","M12","碳钢",null,"本色","200-300HV"]
["DIN7349010AC008UM",52.2,"DIN7349","M10","碳钢","NULL","黄锌8um","200HV"]
["F0030511PW91800H3",52.04,"PW918-3","21.4*42*5","45#钢",null,"热处理本色","300-370HV"]
["F0064X0121X008AK0",52,"BN90701 6174502","6.4*12.1*0.8","碳钢","NULL","三价锌6/24/3","140HV"]
["XXT0000039",52,"DIN127B","M3","65Mn","NULL","发兰","NULL"]
["ISO7089M12AGHV200",51.5,"ISO7089","M12","碳钢",null,"达克罗1000无红","200-300HV"]
["F000000AK24H13700",51.43,"24H1370","0.656*1.375*0.134","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["G009785M14AGHV200",51.4,"GB97-85","M14","碳钢",null,"达克罗720无红","200-300HV"]
["F09X4X22X2GA00000",51,"PWH M10-14C","9.4*22*2","S50",null,"热处理本色","S50钢"]
["F0074X18X3GA300HV",51,"Q180817730","7.4*18*3","45#钢",null,"热处理本色","300-370HV"]
["D00125A008AK140HV",51,"DIN125A","M8","碳钢",null,"三价锌96无白8um","200-250HV"]
["F0128X225X0134AK0",50.87,"24H1499","1.281*2.25*0.134","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["GB9785M12AG200HV",50.5,"GB97-85","M12","碳钢",null,"环保达克罗500无红","200-300HV"]
["G009387012ID00000",50.393999999999998,"GB93-87","M12","65锰",null,"发黑","42-50HRC"]
["XXT0000011",50.3,"NFE25-511M","M6","不锈钢316","NULL","本色","270HV"]
["F0268X515X34AA000",50.27,"美制1N非标","1(26.8*51.5*3.4)","碳钢","NULL","本色","140-220HV"]
["F0010501PW95300QS",50,"PW953-1","5*9*0.3","不锈钢304",null,"不锈钢304"]
["F0025661PW71500HL",50,"PW715-4（同530015127）","5/16 异形垫","50#钢","NULL","黑磷化上油","HRC46-50"]
["DIN6798AM10MK0000",50,"DIN6798A","M10","65锰","NULL","三价锌72无红","350-425HV"]
["D00125A012AFHV140",50,"DIN125A","M12","碳钢",null,"热锌","140-250HV"]
["D00127B005BA00000",50,"DIN127B","M5","不锈钢304",null,"不锈钢304"]
["D00125A016AAHV140",50,"DIN125A","M16","碳钢",null,"本色","140-250HV"]
["D000433004AKHV140",50,"DIN433","M4","碳钢",null,"三价锌","140-250HV"]
["DIN127BM04NA00000",50,"DIN127B","M4","磷青铜","NULL","磷青铜","NULL"]
["DIN0434012AK2002",50,"DIN434-2000","M12","A3普碳钢",null,"三价锌"]
["DIN0125A06AL200HV",50,"DIN125A","M6","碳钢",null,"三价彩锌72/144/8","200-250HV"]
["ISO7093M06AKHV200",50,"ISO7093","M6","碳钢","NULL","三价锌48/72/5","200-300HV"]
["X00000M08MG25511S",50,"NFE25-511S","M8","65锰","NULL","环保达克罗1000无红","NULL"]
["X06798A006MA00000",50,"DIN6798A","M6","65锰","NULL","热处理本色","350-425HV"]
["G861187004MN00000",50,"GB861.1-87","M4","65锰",null,"黑磷化","40-50HRC"]
["GB09387012IK00000",50,"GB93-87","M12","65锰",null,"三价锌48无红5um","42-50HRC"]
["G009785008AG00000",50,"GB97-85","M8","碳钢",null,"达克罗500无红","140-250HV"]
["XXT0000243",49.82,"GB97-85","M16","Q235","NULL","本色","100HV"]
["G009785020AGHV200",49.6,"GB97-85","M20","碳钢",null,"达克罗500无红","200-300HV"]
["G009387012BA00000",49.6,"GB93-87","M12","不锈钢304",null,"不锈钢304"]
["X0L0000M10BA25514",49.5,"NFE25-514L","M10","不锈钢304",null,"不锈钢304"]
["X0000000M12BA2551",49.5,"NFE25-511M","M12","不锈钢304",null,"不锈钢304","锥形压花垫"]
["D00127B016II00000",49.5,"DIN127B","M16","弹簧钢",null,"机械镀锌"]
["D00125A012BAHV200",49.5,"DIN125A","M12","不锈钢304",null,"不锈钢304","200HV"]
["F0009X24X003AK5UM",49.33,"M8(9*24*3)","M8(9*24*3)","Q235",null,"三价锌72/144/5","200HV"]
["DIN4330M16ALHV200",49.2,"DIN433","M16","碳钢",null,"三价彩锌72/216/5","200-300HV"]
["X06797J08MD000000",49.1,"DIN6797J","M8","65锰","NULL","发黑","350-425HV"]
["ISO7089M06HN00000",49,"ISO7089","M6","黄铜","NULL","铜镀镍3um","NULL"]
["ISO7090M08BA140HV",49,"ISO7090","M8","不锈钢304",null,"不锈钢304","140-250HV"]
["G009685018AA200HV",49,"GB96-85","M8","碳钢",null,"本色","200-300HV"]
["D00125A008AL200HV",49,"DIN125A","M8","碳钢",null,"三价彩锌48/72/5","200-250HV"]
["000000A010DIN2093",49,"DIN2093A","M10（10.2*20*1.1）","65锰",null,"黑磷化"]
["DIN6796010GI012UM",49,"DIN6796","M10","65锰","NULL","机械镀锌72/144/12","420-490HV"]
["F00000L400P29AL00",49,"BN90701 6197052","L400P29","碳钢",null,"三价彩锌48/72/5","140HV"]
["DIN47060012Ml000",48.9,"DIN471","M12","65锰",null,"环保机械黄锌96无白"]
["F000000024H165700",48.8,"24H1657","24H1657","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["F074X24X25AA00000",48.64,"P1H0824025-00","7.4*24*2.5","20#钢","NULL","本色上蜡","NULL"]
["G085987010ID00000",48.3,"GB859-87","M10","70#钢","NULL","发黑","NULL"]
["D006796010BA00000",48.3,"DIN6796","M10","不锈钢304",null,"不锈钢304"]
["D007980005IK00000",48,"DIN7980","M5","弹簧钢","NULL","三价锌48无红","NULL"]
["DIN6799M06ML00000",48,"DIN6799","M6","65锰","NULL","环保机械黄锌72无白","NULL"]
["F00000000024M7429",47.8,"24M7429","13*24*2.5","35#钢","NULL","机械镀锌48/96/8","300-370HV"]
["F0000AK245A2902P2",47.8,"BN90701 6074824","245A2902P2","碳钢",null,"三价锌72无红5um"]
["F0105X50X5HD00000",47.5,"BN90704   6252441","10.5*50*2","50CrV4",null,"环保达克罗500无红","HRC40-46"]
["X000000M16MD25511",47.46,"NFE25-511M","M16","65锰","NULL","机械镀锌","NULL"]
["F0165X34X25AA0000",47.38,"美制平垫","5/8（16.5*34*2.5）","碳钢","NULL","本色","140-220HV"]
["F0105X22X002RT000",46.5,"BN90701   6147453","10.5*22*2","碳钢",null,"黑色环保达克罗500无红","200HV"]
["F0000000AK24H1291",46.5,"24H1291","0.328*1.469*0.109","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["A200000573",46.2,200000573,"DIN125A M12","304不锈钢",null,"本色","140-250HV"]
["F089X254X2AK00000",46.1,"3810S.080.001.C96","8.9*25.4*2","碳钢","NULL","三价彩锌96无红","NULL"]
["D006796003BA00000",46,"DIN6796","M3","不锈钢304",null,"不锈钢304"]
["DIN9021M04AKHV200",46,"DIN9021","M4","碳钢",null,"三价锌48/72/5不上封闭","200-250HV"]
["F00003$4AK0000000",45.88,"BN90701/4105966","3/4 type A","Q235B",null,"三价锌96无白8um"]
["D00125B010GDHV300",45.7,"DIN125B","M10","45#钢",null,"发黑","300-370HV"]
["G085388010AB00000",45.6,"GB853-88","M10","碳钢","NULL","镀锌","NULL"]
["F071X254X15AA0000",45.4,"7.1*25.4*1.5","7.1*25.4*1.5","A3普碳钢",null,"本色","昇沪"]
["X00125A008BA140HV",45,"DIN125A","M8","不锈钢304",null,"不锈钢304 140HV","西门子"]
["ISO7092M08AKHV200",45,"ISO7092","M8","碳钢",null,"三价锌12/36/3","200-300HV"]
["D00125A003AKHV200",45,"DIN125A","M3","碳钢",null,"三价锌","200-250HV"]
["DIN127BM04HA00000",45,"DIN127B","M4","黄铜","NULL","黄铜","NULL"]
["X0047115X1MD00000",44.97,"DIN471","M15*1","65锰",null,"发黑"]
["F031012001AA00000",44.6,"AW0040-6","3.1*12*1","65mn",null,"热处理本色","HRC26-32"]
["F025X35X05EA00000",44.38,"DIN988","25*35*0.5","65锰",null,"发黑上油"]
["F061X97X137AK0000",44,"BN90700   6152622","6.1*9.7*13.7","碳钢",null,"三价锌8um"]
["G009387010IG00000",44,"GB93-87","M10","65锰","NULL","达克罗500无红","42-50HRC"]
["X000SN70093006MI0",44,"SN70093","M6","65锰",null,"机械镀锌","柏中不用"]
["X06798A051BA00000",44,"DIN6798A","M5.1","不锈钢304",null,"不锈钢304","西门子"]
["F0129X38X3GA300HV",43.95,"P1J1438030-01","12.9*38*3","45#钢",null,"热处理本色","300-370HV"]
["D009021006AKHV140",43.8,"DIN9021","M6","碳钢",null,"三价锌","140-250HV"]
["ISO7093M06AN200HV",43.8,"ISO7093","M6","碳钢","NULL","灰色锌镍150无红","200-300HV"]
["F074X24X2GA000000",43.65,"Q180824020-1","7.4*24*2","35#钢",null,"热处理本色","300-370HV"]
["F0000000AK24M7038",43.1,"24M7038","13.5*24*2.5","Q235",null,"三价锌TNTUV12/144/5","100-200HV"]
["G084885006AK200HV",43,"GB848-85","M6","碳钢","NULL","三价锌5um","200-300HV"]
["G085987006IB00000",43,"GB859-87","M6","70#钢",null,"镀锌"]
["ISO7089M10GF300HV",43,"ISO7089","M10","45#钢",null,"热锌","300HV"]
["F000254X436X3AK00",42.74,"'03040209","7/8(25.4*43.6*3)","Q235","NULL","三价锌72/120/8","NULL"]
["F00000N402P15AK00",42.6,"BN90701 6196899","N402P15","碳钢","NULL","三价黄锌(518Y)48/72/5","140HV"]
["XXT0000230",42.2,"DIN6796","M8","50CrV4","NULL","上海环保达克罗0/500","420-470HV"]
["XXT0000036",42,"ISO7090","M8","Q235","NULL","三价锌48/72/5","200-300HV"]
["XXT0000288",42,"GB848-85","M6","Q235","NULL","三价锌72/0/12um","200HV"]
["ISO7090M06AR200HV",42,"ISO7090","M6","碳钢",null,"环保达克罗500无红","200-300HV"]
["DIN127B008IL008UM",42,"DIN127B","M8","弹簧钢",null,"三价彩锌72/216/8"]
["F00000000024M7617",41.7,"24M7617","17*30*3(16/125A)","45#","NULL","环保达克罗960无红","300-370HV"]
["XXT0000245",41.6,"3/4N typeA","3/4N typeA","Q235","NULL","三价锌96/0/13um","NULL"]
["DIN125A016AK200HV",41.4,"DIN125A","M16","碳钢",null,"三价锌48/72/5","200-250HV"]
["F0000000024M74660",41.1,"24M7466","10.5*20*2","45#钢",null,"三价锌TNTUV12/144/5","300-370HV"]
["F000000024M709700",41,"24M7097","17*28*2.5","Q235B","NULL","三价锌TNTUV12/144/5","200HV"]
["F00000000024M7132",41,"24M7132","8.4X18X1.5（8/NFE25-513m)）","Q235","NULL","三价锌TNTUV12/144/5","100HV"]
["A000003$8WAK008UM",41,"美制W型","3/8W","碳钢","NULL","三价彩锌72/144/8","NULL"]
["GB09387M12MK00000",41,"GB93-87","M12","65锰",null,"三价锌72/144/5","42-50HRC"]
["G009387006MG00000",41,"GB93-87","M6","65锰",null,"达克罗720无红","42-50HRC"]
["A200005466",40.700000000000003,200005466,"DIN126 M10","碳钢",null,"达克罗","100-250HV"]
["D00125A020AKHV200",40.700000000000003,"DIN125A","M20","碳钢",null,"三价锌","200-250HV"]
["XXT0000203",40.6,"GB93-87","M4","不锈钢304","NULL","A2","NULL"]
["NFE25511M12MR0000",40.5,"NFE25-511M","M12","65锰","NULL","环保达克罗500无红","420-510HV"]
["F084060003BA00000",40.43,"BN91170/3456164","8.4*60*3","不锈钢304","NULL","不锈钢304","NULL"]
["F000000024H131300",40.369999999999997,"24H1313","0.406*1.75*0.065","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["DIN6796020GG012UM",40.35,"DIN6796","M20","50CrV4","NULL","达克罗三涂三烘+封闭96/500/12","420-490HV"]
["D00125A005AAHV140",40,"DIN125A","M5","碳钢",null,"本色","140-250HV"]
["A300001451",40,300001451,"12*1","50#",null,"蓝白锌5um72/0","44-53HRC"]
["A300004092",40,300004092,"SN70093 M8","65Mn","NULL","环保达克罗500无红不上封闭","440-520HV"]
["A300004490",40,300004490,"3/8N WA-0001-00","Q235","NULL","三价锌≥3um","NULL"]
["D00137A008MR00000",40,"DIN137A","M8","65锰","NULL","上海环保达克罗(Deltaton)","NULL"]
["F062X18X07MD00000",40,"BN806   1282573","6.2*18*0.7","50CrV4",null,"黑磷化","锥垫"]
["GB09785012AA200HV",40,"GB97.1-2002","M12","碳钢",null,"本色","200-300HV"]
["G0097852X5AL00000",40,"GB97-85","M2.5","碳钢","NULL","三价彩锌","140-250HV"]
["ISO7089M08AA200HV",40,"ISO7089","M8","碳钢",null,"本色","200-300HV"]
["XXT0000183",40,"3/8美制弹垫99版","3/8美制弹垫99版","65Mn","NULL","机械镀锌","NULL"]
["XXT0000018",40,"GB93-87","M5","65Mn","NULL","三价锌8um","NULL"]
["XXT0000299",40,"4.3*14*0.8","4.3*14*0.8","Q235B","NULL","三价锌24/0/5","140HV"]
["XXT0000063",39.799999999999997,"NULL","NULL","NULL","NULL","NULL","NULL"]
["D006340008GK005UM",39.799999999999997,"DIN6340","M8","45#钢","NULL","三价锌72无红5um","350-430HV"]
["DIN128A020MR00000",39.799999999999997,"DIN128A","M20","弹簧钢",null,"环保达克罗500无红","44-51HRC"]
["F02223X381X3AK000",39.630000000000003,"'03040208","3/4(22.23*38.1*3)","Q235",null,"三价锌5um"]
["F00195X97X002BA00",39,"BN91170 6352512","0.195*9.7*0.02","不锈钢304","NULL","不锈钢304","200-300HV"]
["D009021006AAHV140",39,"DIN9021","M6","碳钢",null,"本色","140-250HV"]
["D006796006CA0000A",39,"DIN6796","M6","不锈钢316",null,"不锈钢316"]
["D00137B008MI00000",39,"DIN137B","M8","65锰",null,"机械镀锌"]
["D00125B012AAHV140",39,"DIN125B","M12","碳钢",null,"本色","140-250HV"]
["X06798A008MD00000",39,"DIN6798A","M8","65锰","NULL","发黑","350-425HV"]
["XXT0000310",39,"DIN125A","M6","Q235","NULL","三价锌","140-250HV"]
["G009685005AG00720",39,"GB96-85","M5","碳钢",null,"达克罗720无红","200-300HV"]
["GB962002010AK0000",38.799999999999997,"GB96.1-2002","M10","碳钢","NULL","三价锌48/72/5","200-300HV"]
["F0000000AK24H1625",38.799999999999997,"24H1625","0.531*1*0.12","碳钢",null,"三价锌TNTUV12/144/5","＜302HV"]
["A200002355",38.700000000000003,200002355,"GB93-87 M12","弹簧钢",null,"热镀锌","≥HRC30"]
["ISO7089M14AK200HV",38.700000000000003,"24M7085","M14/ISO7089","碳钢","NULL","三价锌TNTUV12/1114/5","200-300HV"]
["A00005$16NBA0000F",38.6,"美制平垫 B型","'5/16","不锈钢304",null,"不锈钢304"]
["DIN125BM12ALHV200",38.5,"DIN125B","M12","碳钢",null,"三价彩锌72/144/5","200-250HV"]
["F00135X024X25MJ00",38.5,"13.5*24*2.5（波垫）","13.5*24*2.5","65锰",null,"机械黄锌","厦门盛思"]
["XXT0000003",38.299999999999997,"NULL","NULL","NULL","NULL","NULL","NULL"]
["D0125A010AKHV2002",38,"DIN125A","M10","碳钢",null,"三价锌48/72/5","200-250HV"]
["D00125B005ALHV140",38,"DIN125B","M5","碳钢",null,"三价锌","140-250HV"]
["G009785016AGHV200",37.799999999999997,"GB97-85","M16","碳钢",null,"达克罗500无红","200-300HV"]
["F0BN91170$4014848",37.6,"BN91170/4014848","1/4标准型弹垫","不锈钢304","NULL","不锈钢304 钝化","NULL"]
["GB96850M16AM200HV",37.5,"GB96-85","M16","碳钢",null,"三价锌72/144/5","200-300HV"]
["A100005$16MH005UM",37.4,"美制标准弹垫","'5/16","65锰",null,"黄锌5um"]
["F0000000000T20168",37.4,"T20168","0.516*0.866*0.09","45#钢",null,"热处理本色","HRC30-40"]
["D00125A008AAHV200",37.1,"DIN125A","M8","碳钢",null,"本色","200-250HV"]
["F013X34X03AK200HV",37.01,"13*34*3","13*34*3","Q235",null,"机械镀锌96/144/12","200HV"]
["F000000024H174600",37,"24H1746","0.781*1.125*0.12","Q235B","NULL","三价锌TNTUV12/144/5","<302HV"]
["D00128A010MH00000",37,"DIN128A","M10","弹簧钢",null,"环保达克罗500无红","44-51HRC"]
["ISO07089M8AR200HV",37,"ISO7089","M8","碳钢",null,"环保达克罗720无红,0.15-0.21摩擦","200-300HV"]
["XXT0000015",37,"DIN9021","M4","Q235","NULL","三价锌5um","200HV"]
["XXT0000294",37,"DIN125A","M10","Q235B","NULL","环保达克罗0/720","200HV"]
["XXT0000318",37,"DIN125A","M8","Q235","NULL","三价彩锌0/150/5","200HV"]
["D00128A010MR00000",36.700000000000003,"DIN128A","M10","弹簧钢",null,"环保机械黄锌72/144/12","44-51HRC"]
["F0000L400P6AL0000",36.700000000000003,"3810R.060.001.Y96","L400P27","碳钢","NULL","三价黄锌（518Y）96无红","NULL"]
["A300004784",36.659999999999997,300004784,"1/4 美制标准型弹垫","65Mn","NULL","机械镀锌5um"]
["XXT0000234",36.6,"10.5*25*2.5","10.5*25*2.5","Q235","NULL","三价锌48/72/5","NULL"]
["F00AlN402P15B1300",36.5,"N402P15B13","N402P15B13","碳钢","NULL","三价锌72无红5um","NULL"]
["F0113X24X25GA0000",36,"P1J1224025-01-DQ","11.3*24*2.5","45#钢",null,"热处理本色上蜡","300-370HV"]
["F0000P6$14AA00000",36,"PW6-14","5.5*20*2.6","A3普碳钢",null,"本色"]
["G009785008ABHV200",36,"GB97-85","M8","碳钢",null,"镀锌","200-300HV"]
["D00125B008BAHV200",35.799999999999997,"DIN125B","M8","不锈钢304",null,"不锈钢304","200HV"]
["G009785016GG00000",35.6,"GB97-85","M16","45#钢",null,"达克罗500无红","300-370HV"]
["GB09785M16AK200HV",35.5,"GB97-85","M16","碳钢","NULL","三价锌12/24/3","200-300HV"]
["ISO7089M20AK200HV",35.5,"ISO7089","M20","碳钢","NULL","三价彩锌72/120/8上封闭","200-300HV"]
["D001440016AKHV140",35.5,"DIN1440","M16","碳钢",null,"三价锌"]
["F0000000AK24H1263",35.340000000000003,"24H1263","1.25*2.0*0.06","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["F000000AKN402AP13",35,"N402AP13B13","N402AP13B13","碳钢","NULL","三价锌 72无红5um","NULL"]
["ISO7093M08AK300HV",35,"ISO7093-2","M8","45#钢",null,"三价锌12/36/3","300-370HV"]
["NFE25514LM06AN000",35,"NFE25-514L","M6","碳钢","NULL","灰色锌镍150无红","160-250HV"]
["F0375X0875X0083GC",35,"0.375*0.875*0.083(F436)","0.375*0.875*0.083","45#钢","NULL","黄锌72/144/8","HRC38-45"]
["F0105X40X26AB0000",34.97,"13107-01326","10.5*40*2.6","Q235",null,"镀锌"]
["G005287016AA00000",34.799999999999997,"GB5287","M16","碳钢","NULL","本色","NULL"]
["A000001$4NGK00000",34.700000000000003,"美制N型","1/4N","45#钢","NULL","三价锌12无白5um","HRC38-45"]
["01B0011619X00942L",34.299999999999997,"BN90701   6009263","1619X00942L","碳钢","NULL","三价锌","NULL"]
["F0000000024H14240",34.200000000000003,"24H1424","0.906*1.5*0.06","Q235",null,"三价锌TNTUV12/144/5","200-300HV"]
["F0000000MH06005UM",34,"美制标准弹垫","6#","65锰","24.6硬度超高艾维不发","三价彩锌72/144/5","NULL"]
["F0000000024M71110",34,"24M7111","13*25*3","碳钢","NULL","三价锌TNTUV12/144/5","140-250HV"]
["D006796008MN00000",34,"DIN6796","M8","50CrV4","NULL","黑磷化","420-490HV"]
["DIN127B008AN00000",34,"DIN127B","M8","弹簧钢",null,"铁镀镍3um"]
["F084025018AK00000",34,"BN732 1270435","8.4*25*1.8","碳钢",null,"三价锌","140HV"]
["X0000000M8MG25511",34,"NFE25-511M","M8","65锰",null,"上海达克罗","500无红"]
["X00M06MG25511S720",34,"NFE25-511S","M6","65锰","NULL","环保达克罗720无红","NULL"]
["ISO7090M06NC200HV",34,"ISO7090","M6","碳钢","NULL","彩色锌镍168/600/5","200-300HV"]
["XXT0000312",34,"DIN9021","M5","Q235","NULL","三价彩锌72/120/5","200-250HV"]
["D00125A012BA00000",33.799999999999997,"DIN125A","M12","不锈钢304","NULL","不锈钢304","140-250HV"]
["F003051PW134900H1",33.700000000000003,"PW1349-1","15.5*28*4","45#钢",null,"热处理本色","300-370HV"]
["F003051PW133500H1",33.619999999999997,"PW1335-1","23*42*5","45#钢",null,"热处理本色","300-370HV"]
["D000434012AK0000",33.6,"DIN434","M12","A3普碳钢",null,"三价锌"]
["F00000000024H1950",33.4,"24H1950","0.344*0.3688*0.065","碳钢","NULL","环保达克罗960无红","<302HV"]
["F0000000000WA0084",33.200000000000003,"WA-0084-00(REV1)","WA-0084-00","H62铜","NULL","黄铜","NULL"]
["D006340008GR00000",33.200000000000003,"DIN6340","M8","45#钢","NULL","Geomet321A + VL500无红","350-430HV"]
["XXT0000226",33.200000000000003," 11*38*3"," 11*38*3","Q235`","NULL","三价锌48/72/12um","NULL"]
["F084X017X001AN000",33.200000000000003,"BN90701   6217799","8.4*17*1","A3普碳钢",null,"铁镀镍3um"]
["ISO7089M12AA200HV",33.1,"ISO7089","M12","碳钢",null,"本色","200-300HV"]
["ISO7090M06CA200HV",33,"ISO7090","M6","不锈钢316",null,"不锈钢316","200-300HV"]
["X06798A006MD00000",33,"DIN6798A","M6","65锰","NULL","发黑","350-425HV"]
["XXT0000027",33,"DIN6796","M8","50CrV4","NULL","上达环保500无红","420-490HV"]
["D009021004AKHV200",33,"DIN9021","M4","碳钢",null,"三价锌","200-250HV"]
["D00125A016BA00000",33,"DIN125A","M16","不锈钢304","NULL","不锈钢304 ","140HV"]
["DIN7349008AK005UM",33,"DIN7349","M8","碳钢","NULL","三价锌5um","200HV"]
["F000AlN402AP09B13",33,"N402AP9B13","N402AP9B13","A3普碳钢",null,"三价彩锌72无红5um"]
["F002677PW11350011",32.527000000000001,"PW1135-1","22*60*6","Q345B","NULL","不热处理本色","NULL"]
["F003046PW11260011",32.25,"PW1126-1","22.6*32*2","碳钢","NULL","本色","NULL"]
["F00000M005SN60075",32,"SN60075","M5","65锰",null,"黑磷化","400-500HV"]
["0000AKN402AP41B13",32,"N402AP41B13","N402AP41B13","碳钢","NULL","三价锌72无红5um","NULL"]
["D009021M08ACHV200",32,"DIN9021","M8","碳钢",null,"三价彩锌72/120/8","140-250HV"]
["F0338X0625X006GN0",32,"0.338*0.625*0.06","0.338*0.625*0.06","45#钢",null,"黑磷化","HRC38-45"]
["F0010X021X002BA00",31.98,"13107-00416","10.5*21*2","不锈钢304",null,"不锈钢304"]
["G009785024AB200HV",31.8,"GB97-85","M24","碳钢",null,"镀锌","200-300HV"]
["G009387020ID00000",31.7,"GB93-87","M20","65锰",null,"发黑","42-50HRC"]
["D00433012AK0HV140",31.7,"DIN433","M12","碳钢",null,"三价锌96无白8UM","140-250HV"]
["DIN127B012IR00720",31.6,"DIN127B","M12","弹簧钢","NULL","环保达克罗720无红","NULL"]
["F000000024H144100",31.6,"24H1441","1.016*1.5*0.048","Q235B","NULL","三价锌TNTUV 12/144/5","＜302HV"]
["XXT0000207",31.6,"DIN127B","M12","65Mn","NULL","机械镀锌","NULL"]
["G001230024GG00720",31.3,"GB1230","M24","45#钢","NULL","达克罗720无红","NULL"]
["D007980012BA00000",31.2,"DIN7980","M12","不锈钢304",null,"不锈钢304"]
["D00127B012IK00000",31,"DIN127B","M12","弹簧钢",null,"三价锌"]
["DIN0433M10AK140HV",31,"DIN433","M10","碳钢","NULL","三价锌48/72/5","140-250HV"]
["F0000L400P30AK00",31,"BN90701 6207346","L400P30","碳钢",null,"三价彩锌48/72/5","140-250HV"]
["DIN7349M06AK200HV",31,"DIN7349","M6","碳钢","NULL","三价锌5um","200HV"]
["F000AlN402P13B1300",31,"N402P13B13","N402P13B13","碳钢",null,"三价锌72无红5um"]
["GB97285M08BA000000",31,"GB97.2-85","M8","不锈钢304","NULL","不锈钢304","200HV"]
["F0000000024M72130",30.97,"24M7213","24M7213","Q235",null,"三价锌TNTUV12/144/5","200-300HV"]
["ISO7093M12AKHV200",30.9,"ISO7093","M12","碳钢","NULL","三价锌","200-300HV"]
["F0000000000909F46",30.84,"909F46(REV.1)","25.78*50.8*1.575","不锈钢304","NULL","不锈钢304","NULL"]
["F0000000024H18640",30.8,"24H1864","24H1864","Q235B",null,"三价锌TNTUV12/144/5","＜302HV"]
["F0000000024M70520",30.8,"24M7052","25*44*4","Q235",null,"三价锌TNTUV12/144/5","200-300HV"]
["GB084885M20GK20HV",30.61,"GB848-85","M20","45#钢（指定）","NULL","三价彩锌72/168/8","200-300HV"]
["A200005424",30.3,200005424,"DIN440 M6","碳钢",null,"蓝白锌5um24/72","100-250HV"]
["F0656X1312X009AK0",30.29,"24H1368","0.656*1.312*0.09","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["F122X28X22MI00000",30.2,"T22124","12.2*28*2.2","65锰","NULL","机械镀锌24/96","HRC42-50"]
["G009785012AFHV200",30.1,"GB97-85","M12","碳钢",null,"热锌","200-300HV"]
["F00000000024M7550",30.09,"24M7550","6.6*22*2(6/440)","Q235","NULL","环保达克罗960无红","100-200HV"]
["DIN9021M10AK00001",30,"DIN9021","M10","碳钢",null,"三价锌48/72/5加WD-40油不上封闭","140-250HV"]
["A300004694",30,300004694,"DIN125A M6","Q235","NULL","本色","140HV"]
["D000433010AKHV140",30,"DIN433","M10","碳钢",null,"三价锌","140-250HV"]
["D0125A010AKHV2001",30,"DIN125A","M10","碳钢",null,"三价锌96无白5um","200-250HV"]
["D007980016IL00000",30,"DIN7980","M16","弹簧钢",null,"机械镀锌"]
["GB8482002M12AA000",30,"GB848-2002","M12","碳钢","NULL","本色","200-300HV"]
["F05X13X1AK0000000",30,"DIN522A","5*13*1","碳钢","NULL","三价锌48/72/5","140HV"]
["ISO7090M10AD300HV",30,"ISO7090","M10","45#钢",null,"黑磷化","300-370HV"]
["ISO7089M08AGHV200",30,"ISO7089","M8","碳钢","NULL","环保达克罗1000无红","200-300HV"]
["X020000M06MN25514",30,"NFE25-514M","M6","碳钢","NULL","灰色锌镍 150无红"," 160-250HV"]
["F000000M12SN60075",29.9,"SN60075","M12","65锰",null,"黑磷化","400-500HV"]
["F00000000024M7346",29.82,"24M7436","15.3*32*4 ","35#钢","NULL","机械镀锌48/96/8","300-370HV"]
["F00000000AA400P12",29.7,"L400P12T","M12","低碳钢","NULL","本色","NULL"]
["G085388012AA00000",29.69,"GB853-88","M12","碳钢","NULL","本色","NULL"]
["XXT0000210",29.6,"DIN6796","M10","65Mn","NULL","机械镀锌24/72/5um","420-450HV"]
["DIN9021M08AK300HV",29.6,"DIN9021","M8","45#钢",null,"三价锌5um","300-370HV"]
["XXT0000044",29.5,"DIN127B","M10","65Mn","NULL","三价锌72无红8um","NULL"]
["G009387010MG00000",29.5,"GB93-87","M10","65锰",null,"达克罗720无红","42-50HRC"]
["G009785014ABHV140",29.4,"GB97-85","M14","碳钢",null,"镀锌","140-250HV"]
["D00125A016ACHV200",29.2,"DIN125A","M16","碳钢",null,"黄锌","200-250HV"]
["A300001250",29,300001250,"21*40*4.5","45#",null,"蓝白锌5um48/0","35-42HRC"]
["A0000001$2AC00000",29,"美制标准弹垫","‘1/2","65锰","NULL","黄锌48/72/5","NULL"]
["D10125A004ALHV200",29,"DIN125A","M4","碳钢",null,"三价彩锌48/96/5","200-250HV"]
["D007980008IK005UM",29,"DIN7980","M8","弹簧钢",null,"三价锌5um"]
["GB9387M8MN0000000",29,"GB93-87","M8","65锰","NULL","灰色锌镍500无红","42-50HRC"]
["G009387008MG00000",29,"GB93-87","M8","65锰",null,"达克罗720无红","42-50HRC"]
["ISO7089M12AG00000",29,"ISO7089","M12","碳钢","NULL","环保达克罗1000无红","200-300HV"]
["D000472028MD00000",28.96,"DIN472","M28","65锰",null,"发黑"]
["D00125A012AAHV140",28.9,"DIN125A","M12","碳钢",null,"本色","140-250HV"]
["DIN433M100AKHV200",28.8,"DIN433","M10","碳钢",null,"三价彩锌72/120/8","200-300HV"]
["SN70093M06MK00000",28.8,"SN70093","M6","65锰",null,"机械镀锌48/144/12","440-520HV"]
["G085388012AK005UM",28.66,"GB853-88","M12","碳钢","NULL","三价锌48/72/5","NULL"]
["G009387012MG01000",28.6,"GB93-87","M12","65锰",null,"达克罗1000无红","42-50HRC"]
["F0000L400P6AK0000",28.6,"3810R.060.001.C96","L400P27","碳钢","NULL","三价彩锌96无红","NULL"]
["F0000000000M43747",28.55,"M43747","25.78*37.34*1.12","1050钢",null,"本色（锥垫）","HRC44-48"]
["D000433016AKHV140",28.5,"DIN433","M16","碳钢",null,"三价锌","140-250HV"]
["D00127B010MG00000",28.5,"DIN127B","M10","弹簧钢","NULL","上海环保达克罗500无红","NULL"]
["F00602804PW0107TO",28.2,"PW0107-5","13.3*18*1.5","65锰","NULL","达克罗（三途三洪+封闭）96/500/12","HRC42-48"]
["F0000000024H14500",28.06,"24H1450","1.031*1.75*0.036","Q235B",null,"三价锌TNTUV12/144/5","<302HV"]
["D006796012GR012UM",28,"DIN6796","M12","65锰","NULL","环保机械黄锌72/144/12","420-490HV"]
["DIN127B004IT00000",27.5,"DIN127B","M4","弹簧钢",null,"灰色锌镍1008无红10um"]
["X00M12MG255112UM",27.3,"NFE25-511M","M12","65锰","NULL","达克罗（三涂三烘+封闭）96/500/12","NULL"]
["F000000000L173700",27.2,"L173700","L173700","Q235",null,"锌镍合金黑色200-300HV,","240无白504无红8um"]
["F00821X1533X002AK",27,"BN90701   6008979","8.21*15.33*2","碳钢","NULL","三价锌72/96/5","NULL"]
["D00128A010MI00000",27,"DIN128A","M10","弹簧钢",null,"机械镀锌","44-51HRC"]
["NFE25$513M05AN000",27,"NFE25-513M","M5","碳钢",null,"灰色锌镍72无白5um","100HV"]
["DIN137B024MR00000",26.9,"DIN137B","M24","65锰","NULL","上海环保达克罗500无红(Deltaton)","NULL"]
["D007980012IK00000",26.8,"DIN7980","M12","弹簧钢",null,"三价锌"]
["D00125A010MCHV200",26.8,"DIN125A","M10","碳钢",null,"黄锌","200-250HV"]
["G009785016AG00720",26.702999999999999,"GB97-85","M16","碳钢",null,"达克罗720无红","200-300HV"]
["D006796012Gi00000",26.66,"DIN6796","M12","65锰","NULL","机械镀锌","420-490HV"]
["G085388012AB00000",26.54,"GB853-88","M12","碳钢","NULL","镀锌","NULL"]
["F052X14X08KH00000",26.5,"BN91220   6043934","5.2*14*0.8","铜","7.8k偏厚不能用","铜镀镍3um","NULL"]
["F006002PW1240001S",26.5,"PW1240-1","8*15*0.8","不锈钢304",null,"不锈钢304(洗白钝化）","200-300HV"]
["ISO7089016GR300HV",26.4,"ISO7089","M16","45#钢",null,"环保达克罗 720无红，0.15-0.21摩擦","300-370HV"]
["F01127X28X3AA0000",26.37,88800205,"11.27*28*3","碳钢","NULL","本色+干油","NULL"]
["F0000000AK24H1626",26.35,"24H1626","0.656*2*0.06","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["F000000AK24H13110",26.34,"24H1311","0.406*1.25*0.22","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["D009021008CA200HV",26.3,"DIN9021","M8","不锈钢316",null,"不锈钢316","200HV"]
["DIN125AM05AK200HV",26,"DIN125A","M5","碳钢","NULL","三价彩锌72/44/8","200-250HV"]
["D00127B008IG05000",26,"DIN127B","M8","弹簧钢","NULL","黑色环保达克罗500无红","NULL"]
["A000001$4NAR00000",26,"美制N型","1/4N","碳钢","NULL","上海环保达克罗600无红","NULL"]
["F00000000000MAM10",26,"锥垫（海盐鼎丰）","M10","65锰","NULL","本色","NULL"]
["G009387016MG00000",25.8,"GB93-87","M16","65锰",null,"达克罗720无红","42-50HRC"]
["DIN125AM04AN140HV",25.783999999999999,"DIN125A","M4","碳钢","NULL","灰色锌镍500无红","140-250HV"]
["DIN9021M06AL200HV",25.5,"DIN9021","M6","碳钢",null,"三价彩锌72/120/5上封闭","200-300HV"]
["X06798A010MA00000",25.5,"DIN6798A","M10","65锰","NULL","热处理本色","350-425HV"]
["ISO7089M12ARHV200",25.2,"ISO7089","M12","碳钢",null,"环保达克罗720无红，0.15-0.21摩擦","200-300HV"]
["F084X32X25AK00000",25.1,"DIN522A","8.4*32*2.5","碳钢","NULL","三价锌48/72/5","NULL"]
["ISO7092M05AKHV200",25,"ISO7092","M5","碳钢",null,"三价锌5um","200-300HV"]
["X06798A010MD00000",25,"DIN6798A","M10","65锰","NULL","发黑","350-425HV"]
["X000000M12MC25514",25,"NFE25-514M","M12","碳钢",null,"黄锌","160HV"]
["F00000L400P26AL00",25,"BN90701   6197050","L400P26","碳钢",null,"三价彩锌48/72/5","140HV"]
["A00005$16NAL00000",25,"美制N型","5/16N","碳钢",null,"三价彩锌72/144/5"]
["NFE25511M0005AA00",24.9,"NFE25-511M","M5","不锈钢304","NULL","不锈钢304 钝化","NULL"]
["G009387016IG00000",24.8,"GB93-87","M16","65锰",null,"达克罗500无红","42-50HRC"]
["A200002773",24.79,200002773,"DIN128A M10","弹簧钢",null,"达克罗","44-51HRC"]
["F0010X30X3AK200HV",24.78,"10*30*3","10*30*3","碳钢",null,"三价锌72/144/5","200HV"]
["D00127B020ID00000",24.7,"DIN127B","M20","弹簧钢","NULL","发黑","NULL"]
["F0000000024H15120",24.64,"24H1512","24H1512","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["D007349008AA200HV",24.6,"DIN7349","M8","碳钢","NULL","本色","200HV"]
["G009785014AAHV200",24.5,"GB97-85","M14","碳钢",null,"本色","200-300HV"]
["ISO7089M10AN300HV",24.5,"ISO7089","M10","45#钢","NULL","彩色锌镍8um","300-370HV"]
["G009685016AB200HV",24.4,"GB96-85","M16","碳钢",null,"镀锌","200-300HV"]
["DIN7349M06AG200HV",24.4,"DIN7349","M6","碳钢","NULL","上海环保达克罗500无红","200HV"]
["DIN9250M10MI00000",24,"DIN9250","M10","65锰",null,"机械镀锌48/96/5","420-510HV"]
["D006796006GJ012UM",24,"DIN6796","M6","65锰","NULL","机械黄锌72/144/12","420-490HV"]
["D009021010AAHV140",24,"DIN9021","M10","碳钢",null,"本色","140-250HV"]
["D009021005ACHV140",24,"DIN9021","M5","碳钢",null,"黄锌","140-250HV"]
["A00F4361$4GC00000",24,"美制垫圈F436","'1/4","45#钢","NULL","黄锌72/144/8","NULL"]
["D000433010AAHV140",24,"DIN433","M10","碳钢",null,"本色","140-250HV"]
["ISO07089M5AR200HV",24,"ISO7089","M5","碳钢",null,"环保达克罗720无红,0.15-0.21摩擦","200-300HV"]
["F006057PW12900011",23.81,"PW1290-1","0.505*1.375*0.119","不锈钢316",null,"不锈钢316"]
["F0000000AK24H1162",23.8,"24H1162","0.531x1.25x0.06","Q235",null,"三价锌TNTUV96/96/5","<302HV"]
["A200001587",23.8,200001587,"DIN6796 M12","65Mn",null,"黑磷化","420-490HV"]
["G009685010AG00720",23.6,"GB96-85","M10","碳钢",null,"达克罗720无红","200-300HV"]
["XXT0000002",23.6,"XXT0000002","DIN6796 M8","65Mn","NULL","热处理本色","420-490HV"]
["X0095040115000MG0",23.56,"SN60075","M6","65锰",null,"达克罗","400-500HV"]
["ISO7093M10GA300HV",23.5,"ISO7093","M10","45#钢",null,"热处理本色","300-370HV"]
["X0L0000M08MC25514",23.5,"NFE25-514L","M8","碳钢",null,"黄锌","160HV"]
["F0000000MAL401P29",23.5,"L401P29M11","M12","65锰","NULL","热处理本色","HRC38-46"]
["F0000AK0024M70980",23.5,"24M7098","19*30*3","碳钢","NULL","三价锌TNTUV 12/144/5","200-300HV"]
["F135024020BA00000",23.4,"BN91170  6177410","13.5*24*2","不锈钢304",null,"不锈钢304","140HV"]
["A0000001$2BA00000",23.3,"美制标准型弹垫","'1/2","不锈钢304",null,"不锈钢304"]
["D0073490M6AC008UM",23,"DIN7349","M6","碳钢","NULL","黄锌8um","200HV"]
["DIN7349M08AG140HV",23,"DIN7349","M8","碳钢","NULL","环保达克罗720无红0.15-0.21摩擦","140HV"]
["F105025020AK00000",23,"BN737   1271121","10.5*25*2","碳钢","NULL","三价锌","140HV"]
["GB96X20M08AK200HV",23,"GB96.2-2002","M8","碳钢",null,"三价锌72/144/5","100-200HV"]
["D000434008AK2000",22.9,"DIN434-2000","M8","碳钢",null,"三价锌"]
["XXT0000213",22.8,"GB93-87","M12","65Mn","NULL","三价锌5um去氢","42-50HRC"]
["XXT0000205",22.7,"DIN127B","M12","65Mn","NULL","机械镀锌24/72/5um","NULL"]
["A300004393",22.7,300004393,"GB848-85 M8","Q235","NULL","本色","200HV"]
["DIN6796010MG00000",22.5,"DIN6796","M10","50CrV4",null,"环保达克罗500无红","420-490HV"]
["F0000000024H12870",22.5,"24H1287","0.281*0.625*0.065","碳钢",null,"三价锌 TNTUV12/144/5","<302HV"]
["F000000000M110698",22.5,"M110698","8.76*23.77*2","50#钢","NULL","机械镀锌48/96/8","30-38HRC"]
["F000000000T228611",22.391999999999999,"T228611","50.5*72.5*5","45#钢",null,"机械镀锌48/96/8","HRC30-38"]
["F0000000000909C66",22.34,"909C66(REV.2)","11.1*40.48*1.51","不锈钢304","NULL","不锈钢304","NULL"]
["ISO7092M30GA300HV",22.29,"KK54948","30/ISO7092","45#钢","NULL","本色","300HV"]
["F095X24X25AA00000",22.2,"非标组合平垫","9.5*24*2.5","碳钢","NULL","本色","140HV"]
["F154X41X6GA000000",22.18,"P1J1641060-00-DQ","15.4*41*6","45#钢",null,"不热处理本色上蜡"]
["ISO7093M16AL200HV",22.05,"ISO7093","M16","碳钢",null,"三价彩锌72/120/8上封闭","200-300HV"]
["ISO7089M08AG140HV",22,"ISO7089","M8","碳钢",null,"达克罗600无红","140-250HV"]
["X000000M06BA25514",22,"NFE25-514M","M6","不锈钢304",null,"不锈钢304"]
["F20453251165BA000",21.84,"WA-0020-00(REV0)","WA-0020-00","不锈钢304","NULL","不锈钢304","NULL"]
["F00153X30X3GA0000",21.8,"B-FP180047","15.3*30*3","45#钢","NULL","不热处理本色","NULL"]
["D00125A030BA00000",21.8,"DIN125A","M30","不锈钢304","NULL","不锈钢304","140HV"]
["DIN0433M12ALHV200",21.8,"DIN433","M12","碳钢",null,"三价彩锌72/120/8上封闭","200-300HV"]
["F0000000GIM155490",21.7,"M155490","26.18*44.45*2.66","45#钢","NULL","机械镀锌48/96/5","30-38HRC"]
["F00C0081104005500",21.6,"C00811040-055","1/2(13*35*1)","65锰","NULL","机械镀锌（外齿）45um","HRC40-50"]
["F0008X2195MA00000",21.5,"3-275DQ","8*21.95","65锰","NULL","热处理本色","360-430HV"]
["F0060120050AA0000",21.5,"DIN988","6*12*0.5","碳钢","NULL","本色","NULL"]
["F0000AN1619X03501",21.5,"BN90701 6056048","1619X03501","碳钢",null,"黑磷化"]
["F0003175X548X3AK0",21.49,"'03040211","1-1/8(31.75*54.8*3)","Q235","NULL","三价锌72/120/8","NULL"]
["ISO7090M16GN300HV",21.44,"ISO7090","M16","45#钢","NULL","灰色锌镍500无红","300-370HV"]
["DIN7349012AKHV200",21.4,"DIN7349","M12","碳钢","NULL","三价锌","200HV"]
["D00127B010CA00000",21.3,"DIN127B","M10","不锈钢316",null,"不锈钢316"]
["F01905X334X3HK000",21.12,"'03040312","5/8(19.05*33.4*3)","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["F0013X036X003AF00",21,"BN90701   6180456","13*36*3","碳钢","NULL","热锌","140HV"]
["F0000000AK24M7421",21,"24M7421","16.3X32X2","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["D6797J0080MC00000",21,"DIN6797J","M8","65锰",null,"黄锌"]
["F064X012X005MR000",21,"BN90704   6148006","6.4*12*0.5","65锰","类似DIN6797V","黑色环保达克罗500无红","NULL"]
["F00000000K24M7349",20.98,"24M7349","21*37*3","45#钢","NULL","三价锌TNTUV 12/144/5","300-370HV"]
["DIN471M30X15MG000",20.98,"DIN471","M30*1.5","65锰",null,"达克罗"]
["A200000426",20.94,200000426,"GB93-87 M8","304不锈钢",null,"本色"]
["F0BN91170$4014847",20.9,"BN91170/4014847","3/8标准型弹垫","不锈钢304","NULL","不锈钢304 钝化","NULL"]
["F135005000BA00000",20.65,"BN91170/5830641","0*13.5*0.5","不锈钢304",null,"不锈钢304","丹麦柏中"]
["DIN6340008GG00000",20.6,"DIN6340","M8","45#钢",null,"Geomet321A + ML","350-430HV"]
["F0000AK245A2902P5",20.5,"BN90701   6074827","245A2902P5","A3普碳钢",null,"三价锌72无红5um"]
["D000126012AKHV100",20.5,"DIN126","M12","碳钢",null,"三价锌","100-250HV"]
["F0651X125X0072AL0",20.5,"0.651*1.25*0.072","0.651*1.25*0.072","Q235B","NULL","三价彩锌72/144/5","NULL"]
["X06798JM12MN00000",20.5,"DIN6798J","M12","65锰","NULL","铁镀镍3um","350-425HV"]
["X00000M08CA25514M",20.399999999999999,"NFE25-514M","M8","不锈钢316",null,"不锈钢316"]
["D007349012GR300HV",20.399999999999999,"DIN7349","M12","45#钢",null,"环保达克罗720无红","300-370HV"]
["F005X125X001AC000",20.399999999999999,"BN90701 6200948","1/2B型(0.5*1.25*0.1)","碳钢",null,"黄锌 72无红","140HV"]
["D00128A012MF00000",20.3,"DIN128A","M12","弹簧钢","NULL","热锌","44-51HRC"]
["XXT0000006",20.29,"DIN7244","M8","65Mn","NULL","镀锌","NULL"]
["ISO7090M16AR300HV",20.2,"ISO7090","M16","45#钢","NULL","环保达克罗720无红","300-370HV"]
["F0000000000R78019",20.2,"R78019","R78019","1040#钢",null,"机械镀锌48/96/5","HRC30-38"]
["DIN7349010AK005UM",20.100000000000001,"DIN7349","M10","碳钢","NULL","三价锌5um","200HV"]
["F000PWH10$51C0000",20,"PWHX M10-01C","9.4*18*3","S50C",null,"热处理本色","HRC40-48"]
["D001440008AK00000",20,"DIN1440","M8","碳钢",null,"三价锌"]
["D006796008GG00000",20,"DIN6796","M8","65锰","NULL","达克罗500无红,","420-490HV"]
["D009021012AKHV140",20,"DIN9021","M12","碳钢",null,"三价锌","140-250HV"]
["D009021006AK005UM",20,"DIN9021","M6","碳钢",null,"三价锌6/24/5不上封闭","140-250HV"]
["DIN4303M12AK200HV",20,"DIN433","M12","碳钢","NULL","三价锌48/72/5","200-250HV"]
["A200005252",20,200005252,"DIN125A M16","碳钢",null,"蓝白锌5um","140-250HV"]
["ISO7089M10ANHV200",20,"ISO7089","M10","碳钢","NULL","灰色锌镍96/150","200-300HV"]
["ISO7089M16AH200HV",20,"ISO7089","M16","碳钢",null,"三价彩锌72/120/8上封闭","200-300HV"]
["ISO7093M06AK200HV",20,"ISO7093","M6","碳钢",null,"三价锌12/48/5不上封闭","200-300HV"]
["X000000M10MR25511",20,"NFE25-511M","M10","65锰","NULL","上海环保达克罗500无红","NULL"]
["X06797A008BM00000",20,"DIN6797A","M8","不锈钢304",null,"不锈钢304","西门子"]
["XXT0000208",20,"DIN6796","M6","65Mn","NULL","机械镀锌","420-490HV"]
["XXT0000197",20,"10#锥垫","10#锥垫","65Mn","NULL","环保达克罗0/500","44-51HRC"]
["F064015015BA00000",20,"BN91170  6045048","6.4*15*1.5","不锈钢304",null,"不锈钢304"]
["F0L401P26MK000000",20,"BN90704   6214926","L401P26（弹垫）","70#钢","NULL","机械镀锌","372-458HV"]
["GB97200206GA00000",20,"GB97.1-2002","M6","45#钢","NULL","不热处理本色","NULL"]
["ISO7089M06BA200HV",20,"ISO7089","M6","不锈钢304","NULL","不锈钢304","200-300HV"]
["GB09387005IK005UM",20,"GB93-87","M5","65锰",null,"三价锌5um","42-50HRC"]
["G907424008AA00000",20,"GB9074.24","M8","碳钢","NULL","本色","NULL"]
["DIN127B008IT00000",19.899999999999999,"DIN127B","M8","弹簧钢",null,"灰色锌镍1008无红10um"]
["D009021006BAHV200",19.899999999999999,"DIN9021","M6","不锈钢304",null,"不锈钢304","200HV"]
["F000000AK24H12220",19.87,"24H1222","0.531*1.375*0.112","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["A200002808",19.84,200002808,"DIN128A M20","弹簧钢",null,"环保达克罗","44-51HRC"]
["D00127B016IK00000",19.8,"DIN127B","M16","弹簧钢",null,"三价锌"]
["D007349006AA200HV",19.600000000000001,"DIN7349","M6","碳钢","NULL","本色","200HV"]
["XXT0000215",19.5,"38.5*50*0.5","38.5*50*0.5","不锈钢304","NULL","A2","NULL"]
["XXT0000301",19.5,"DIN6798J","M4","65Mn","NULL","三价锌8um","350-425HV"]
["F084X20X25AK00000",19.3,"ISO4759-3A","8.4*20*2.5","Q235",null,"三价锌5um"]
["DIN127B008IJ00000",19.3,"DIN127B","M8","弹簧钢","NULL","机械镀锌48/96/8","HRC44-51"]
["F013030030AF00000",19.149999999999999,"BN90701 6180453","13*30*3","碳钢","NULL","热锌","140HV"]
["F0000000K24M71450",19,"24M7145","15*24*2.5","碳钢",null,"三价锌TNTUV12/144/5","200-300HV"]
["D00128A008MI00000",19,"DIN128A","M8","弹簧钢",null,"机械镀锌","44-51HRC"]
["D000433006AKHV140",19,"DIN433","M6","碳钢",null,"三价锌","140-250HV"]
["G009785024ABHV140",19,"GB97-85","M24","碳钢",null,"镀锌","140-250HV"]
["G085388016AB00000",19,"GB853-88","M16","碳钢","NULL","镀锌","NULL"]
["X000SN70093004MI0",19,"SN70093","M4","65锰",null,"机械镀锌","440-520HV"]
["X000000M10BA25514",19,"NFE25-514M","M10","不锈钢304",null,"不锈钢304"]
["A300001605",18.98,300001605,"2020-01-02","65Mn",null,"本色"]
["XXT0000037",18.899999999999999,"DIN7349","M12","45#","NULL","三价锌8um","200HV"]
["X00125A016AF140HV",18.8,"DIN125A","M16","碳钢","NULL","热锌 140HV","西门子"]
["F0385X50X05BA0000",18.774999999999999,95210750000,"38.5*50*0.5","不锈钢304",null,"不锈钢304"]
["XXT0000066",18.7,"DIN7349","M5","Q235","NULL","环保达克罗720无红摩擦系数0.15-0.21","200HV"]
["SO7089M24GG300HV",18.579999999999998,"ISO7089","M24","45#钢",null,"环保达克罗720无红，0.15-0.21摩擦","300-370HV"]
["ISO7092M12GI300HV",18.5,"ISO7092","M12","45#钢",null,"机械镀锌","300-370HV"]
["XXT0000298",18.5,"BN90701 6288555","6.4*20*1.6","Q235","NULL","三价彩锌48/96/8um","200HV"]
["F105085004BA00000",18.5,"BN91170/3456466","10.5*85*4","碳钢","NULL","不锈钢304","NULL"]
["F002677PW127500H1",18.5,"PW1275-H-1","9*17*4","45#钢",null,"热处理本色上油","HRC36-42"]
["DIN125AM12AN008UM",18.3,"DIN125A","M12","碳钢",null,"彩色锌镍168/720/8","140-250HV"]
["D009021012AC005UM",18.3,"DIN9021","M12","45#钢",null,"黄锌5um","300-370HV"]
["D007349016AAHV300",18.2,"DIN7349","M16","45#钢","NULL","热处理本色","300HV"]
["F0000000000WA0018",18.11,"WA-0018-00(REV1)","WA-0018-00","不锈钢304","NULL","不锈钢304","NULL"]
["F000011X017X001GD",18,"BN90701 6106400","DIN988 11*17*1","45#钢","NULL","发黑","NULL"]
["F06X15X16AC000000",18,"6*15*1.6","6*15*1.6","碳钢","NULL","黄锌 96无红","200HV"]
["XXT0000059",18,"NFE25-514M","M8","Q235","NULL","三价彩锌3um","160-250HV"]
["XXT0000029",18,"0.406*0.812*0.065(3/8N)","0.406*0.812*0.065(3/8N)","Q235","NULL","三价锌5um","NULL"]
["F002677PW111100H1",17.97,"PW1111-H-1","13*24*2.5(12/125A)","45#钢","NULL","热处理本色","HRC36-42"]
["D00128A016MF00000",17.95,"DIN128A","M16","弹簧钢","NULL","热锌","44-51HRC"]
["GB97200220AA200HV",17.920000000000002,"GB97.1-2002","M20","碳钢",null,"本色","200-300HV"]
["F09X30X2GL0000000",17.899999999999999,"9*30*2","9*30*2","35#钢",null,"三价彩锌120/264/8"]
["F000L400P46AK0000",17.8,"3810W.050.001.C96","L400P46","碳钢","NULL","三价彩锌96无红","NULL"]
["F0032X008X008BA00",17.8,"BN91170   6166329","3.2*8*0.8","不锈钢304",null,"不锈钢304","200-300HV"]
["F00281X0625X004BA",17.7,"BN91170   6130989","0.281*0.625*0.04","不锈钢304",null,"不锈钢304"]
["A300001447",17.7,300001447,"8.4*18*1 锥形","50#",null,"热处理本色","40-45HRC"]
["D007980016AK00000",17.399999999999999,"DIN7980","M16","弹簧钢",null,"三价锌"]
["F018X34X4GC000000",17.399999999999999,"12601-02326","18*34*4","45#钢",null,"黄锌24/48/3","HRC38-45"]
["X000000M16AR2551M",17.399999999999999,"NFE25-511M","M16","65锰","NULL","上海环保达克罗1000无红","NULL"]
["XXT0000060",17,"DIN433","M12","Q235","NULL","达克罗600无红","200-300HV"]
["XXT0000074",17,"DIN127B","M5","Q235","NULL","机械镀锌48/96/8um","NULL"]
["XXT0000275",17,"0.291*0.62*0.073","0.291*0.62*0.073","不锈钢304","NULL","A2","NULL"]
["D007980006CA00000",17,"DIN7980","M6","不锈钢316",null,"不锈钢316"]
["DIN9021012AL200HV",16.850000000000001,"DIN9021","M12","碳钢",null,"三价彩锌72/120/8上封闭","200-300HV"]
["F105025002AK200HV",16.8,"10.5*25*2","10.5*25*2","Q235",null,"机械镀锌96/144/12","200HV"]
["DIN7349M16AG140HV",16.79,"DIN7349","M16","碳钢","NULL","环保达克罗720无红，0.15-0.21摩擦","140HV"]
["F00000AC24H161600",16.53,"24H1616","24H1616","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["ISO7093M08GN300HV",16.5,"ISO7093","M8","45#钢","NULL","黑色锌镍1000无红8um","300-370HV"]
["ISO7089M16GC200HV",16.5,"ISO7089","M16","碳钢",null,"黄锌72/144/8","200-300HV"]
["F0125X30X32X4AK00",16.350000000000001,"Z68970","12.5*30*32*4","Q235",null,"三价锌TNTVU 12/144/5"]
["X06798JM10MN00000",16.321999999999999,"DIN6798J","M10","65锰","NULL","铁镀镍3um","350-425HV"]
["ISO7089M20AR200HV",16.100000000000001,"ISO7089","M20","碳钢",null,"环保达克罗720无红,0.15-0.21摩擦","200-300HV"]
["NFE25513MM20AK000",16,"NFE25-513M","M20","碳钢","NULL","三价锌48/72/5","NULL"]
["F064024020AK00000",16,"DIN522A","6.4*24*2","碳钢","NULL","三价锌48/72/5","NULL"]
["A300004782",16,300004782,"8.4*17*1","A3普碳钢","NULL","铁镀镍3um"]
["A200001605",16,200001605,"DIN6796 M8","65Mn",null,"机械镀锌12UM72/144","420-490HV"]
["X0047112X1MD00000",15.997,"DIN471","M12*1","65锰",null,"发黑"]
["X0004712012MD0000",15.98,"DIN471","M20*1.2","65锰","NULL","发黑","NULL"]
["F105030004AA00000",15.948,"BN91100/3029172","10.5*30*4","不锈钢304","NULL","不锈钢304","NULL"]
["ISO7089M24AKHV200",15.9,"ISO7089","M24","碳钢",null,"三价锌","200-300HV"]
["F0000000024H11760",15.9,"24H1176","0.406*1.25*0.1","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["F0000000AK24H1276",15.69,"24H1276","1.312*2.5*0.149","Q235",null,"三价锌TNTVU12/144/5","<302HV"]
["F00000000L1159890",15.67,"L115989","25.5*45*2","Q235","NULL","三价锌TNTUV12/144/5","140HV"]
["F00135X255X003GA3",15.6,"DQ120754(A3)","13.5*25.5*3","45#钢",null,"不热处理本色上油"]
["D006796004GI00000",15.5,"DIN6796","M4","65锰",null,"机械镀锌","420-490HV"]
["D01D6796M500000H1",15.4,"DIN6796","M5","65锰","NULL","热处理本色上油","420-490HV"]
["G009785020ABHV200",15.4,"GB97-85","M20","碳钢",null,"镀锌","200-300HV"]
["G009387027ID00000",15.27,"GB93-87","M27","65锰",null,"发黑","42-50HRC"]
["X0095039914000MG0",15.2,"SN60075","M16","65锰",null,"达克罗","400-500HV"]
["DIN125AM16AI200HV",15.2,"DIN125A","M16","碳钢",null,"机械镀锌96/144/12","200-250HV"]
["F010X508X2BA00000",15.07,"13106-02620","10*50.8*2","不锈钢304",null,"不锈钢304"]
["F00000000024H1977",15.07,"24H1977","24H1977","Q235",null,"环保达克罗960无红"]
["D007980005II00000",15,"DIN7980","M5","弹簧钢",null,"机械镀锌"]
["A200000203",15,200000203,"DIN6797J M3","304不锈钢",null,"本色"]
["ASPRWASHERBA008BA",15,"美制标准型弹垫","8#","不锈钢304",null,"不锈钢304"]
["D00125A014BAHV140",15,"DIN125A","M14","不锈钢304",null,"不锈钢304","140HV"]
["D00125A010ANHV200",15,"DIN125A","M10","碳钢",null,"三价黑锌","200-250HV"]
["X000000M08BA25514",15,"NFE25-514M","M8","不锈钢304",null,"不锈钢304"]
["XXT0000058",15,"10#美制平垫","10#美制平垫","Q235","NULL","三价黑锌96无红5um","NULL"]
["XXT0000269",15,"DIN127B","M12","65Mn","NULL","三价锌","NULL"]
["G009387012MI00000",15,"GB93-87","M12","65锰",null,"机械镀锌","42-50HRC"]
["F064X15X15BA200HV",15,"6.4*15*1.5","6.4*15*1.5","不锈钢304","NULL","不锈钢304","200HV"]
["G7246012BA0000000",15,"GB7246","M12","不锈钢304",null,"不锈钢304"]
["D00125AM16AL200HV",14.9,"DIN125A","M16","碳钢","NULL","三价彩锌120/360/8","200-250HV"]
["DIN7349M06AR140HV",14.9,"DIN7349","M6","碳钢","NULL","环保达克罗720无红，0.15-0.21摩擦","140HV"]
["G007244012MC00000",14.8,"GB7244","M12","65锰",null,"黄锌","27K柏中不用"]
["F0562X125X0083AK0",14.7,500029974,"0.562*1.25*0.083 ","Q235","NULL","机械镀锌","140HV"]
["F002677PW114000H1",14.63,"PW1140-1","17*30*5","45#钢",null,"热处理本色","HRC36-42"]
["XXT0000289",14.54,"BN45719 3322995","24H1162（停用）","Q235","NULL","三价锌TNTUV","NULL"]
["XXT0000239",14.5,"ISO7093","M10","Q235","NULL","环保达克罗0/720，摩0.15-0.21","200-300HV"]
["G009387010IK00000",14.5,"GB93-87","M10","65锰",null,"三价锌","42-50HRC"]
["G109785012ACHV200",14.5,"GB97-85","M12","碳钢",null,"黄锌48/72/5","200-300HV"]
["D000126016AK005UM",14.5,"DIN126","M16","碳钢",null,"三价锌5UM","100-250HV"]
["D007980010IK00000",14.5,"DIN7980","M10","弹簧钢",null,"三价锌"]
["D007980012IR00000",14.5,"DIN7980","M12","弹簧钢",null,"机械镀锌"]
["DIN125AM12AT200HV",14.47,"DIN125A","M12","碳钢","NULL","灰色锌镍1008无红10um","200-250HV"]
["D006796012GI008UM",14.4,"DIN6796","M12","65锰","NULL","机械镀锌48/96/8um","420-490HV"]
["G085586M06AA00000",14.3,"GB855","M6","低碳钢","NULL","本色","NULL"]
["G009387016MG01000",14.3,"GB93-87","M16","65锰",null,"达克罗1000无红","42-50HRC"]
["G009785024AGHV200",14,"GB97-85","M24","碳钢",null,"达克罗500无红","200-250HV"]
["XXT0000065",14,"DIN125A","M10","Q235","NULL","彩色锌镍168/720/8um","200-250HV"]
["ISO7092M08AH200HV",14,"ISO7092","M8","碳钢","NULL","灰色锌镍720无红8um","200-300HV"]
["D007980M08IR00000",14,"DIN7980","M8","弹簧钢","NULL","环保达克罗500无红","NULL"]
["D000433006BAHV200",14,"DIN433","M6","不锈钢304",null,"不锈钢304","200HV"]
["F0043X009X008KA00",14,"4.3*9*0.8","4.3*9*0.8","黄铜",null,"黄铜（本色）","菊龙"]
["F0000MN1619X03110",13.9,"BN90701  6043285","1619X03110","65锰","NULL","三价黑锌","NULL"]
["GB962002016AB0000",13.9,"GB96.1-2002","M16","碳钢",null,"镀锌","200-300HV"]
["F0000ACL401P29000",13.8,"BN90704   6206346","L401P29","70#钢","NULL","机械镀锌8um","372-458HV"]
["DIN125A012AN00000",13.7,"DIN125A","M12","碳钢",null,"铁镀镍3um","140-250HV"]
["ISO7090M14GN300HV",13.62,"ISO7090","M14","45#钢","NULL","灰色锌镍500无红","300-370HV"]
["NFE25$513006AR000",13.6,"NFE25-513LL","M6","碳钢","NULL","环保达克罗720无红","NULL"]
["D0009021M08AR140HV",13.6,"DIN9021","M8","碳钢",null,"环保达克罗720无红","140-250HV"]
["F0095X24X3GA300HV",13.57,"P1J1024030-00","9.5*24*3","45#钢",null,"热处理本色","300-370HV"]
["D009021010CA00000",13.5,"DIN9021","M10","不锈钢316",null,"不锈钢316"]
["XXT0000061",13.45,"DIN7349","M16","50#","NULL","本色","300HV"]
["D000126010AKHV100",13.4,"DIN126","M10","碳钢",null,"三价锌","100-250HV"]
["F0115X27X3MA00000",13.4,"P1N1227030-00-DQ-LD","11.5*27*3","65锰",null,"热处理本色","HRC40-45"]
["F000000AK24H14620",13.28,"24H1462","1.062*1.5*0.06","Q235",null,"三价锌TNTVU12/144/5","<302HV"]
["DIN7349010AKHV200",13.2,"DIN7349","M10","碳钢","NULL","三价锌","200HV"]
["F0281X0625X004BA0",13.115,"AF074092","0.281*0.625*0.04","黄铜",null,"黄铜","140HV"]
["F0074X19X2GA300HV",13.1,"P1I0819020-00","7.4*19*2","35#钢","NULL","热处理本色","300-370HV"]
["DIN9021010AKHV140",13,"DIN9021","M10","碳钢",null,"三价锌48/72/5不上封闭","140-250HV"]
["F0001000MRSN60075",13,"SN60075","M6","65锰","NULL","上海环保达克罗1000无红（Delte Tone）","400-500HV"]
["D6797J0120MC00000",13,"DIN6797J","M12","65锰",null,"黄锌"]
["DIN137BM16BA00000",13,"DIN137B","M16","不锈钢304","NULL","不锈钢304","NULL"]
["D00128A003MA00000",13,"DIN128A","M3","弹簧钢","NULL","本色","44-51HRC"]
["G009387005CA00000",13,"GB93-87","M5","不锈钢316",null,"不锈钢316"]
["FBN911703337169BA",13,"BN91170/3337169","0.443*0.77*0.063","不锈钢304","NULL","不锈钢304","NULL"]
["NFE25514LM08200HV",13,"NFE25-514L","M8","碳钢","NULL","环保达克罗1000无红","200-300HV"]
["X00125A014AA140HV",13,"DIN125A","M14","不锈钢304",null,"不锈钢304 140HV","西门子"]
["ISO7089M10AR200HV",13,"ISO7089","M10","碳钢",null,"上海环保达克罗1000无红","200-300HV"]
["F00000000WA002502",12.948,"WA-0025-00(REV2)","WA-0025-00(REV2)","H70铜","NULL","H70铜","NULL"]
["F0000000000R325123",12.9,"R325123","25.4*34.925*1.524","45#钢",null,"机械镀锌48无白96无红8um","HRC38-45"]
["F0064X030X015AK00",12.9,"BN732 8027307","6.4*30*1.5","A3普碳钢","NULL","三价锌","140HV"]
["X200000M12ML25514",12.8,"NFE25-514M","M12","碳钢",null,"三价彩锌150无红上封闭","160HV,"]
["F017X30X6AK000000",12.75,"BN90700  6305320","SWT671 17*30*6","Q235",null,"三价锌12/36/5"]
["D006340016GK00000",12.7,"DIN6340","M16","45#钢","NULL","黄锌","350-430HV"]
["F0000000024M75250",12.6,"24M7525","17*50*3","45#钢","NULL","三价锌TNTUV12/144/5","300HV"]
["D06798A016MK00000",12.5,"DIN6798A","M16","65锰","NULL","三价锌","350-425HV"]
["A300002620",12.5,300002620,"M10/10.5*25*2","Q235",null,"机械镀锌12um","200HV"]
["XXT0000316",12.5,"DIN9021","M8","Q235","NULL","三价彩锌72/216/8um","200HV"]
["ISO7090M05AN200HV",12.478,"ISO7090","M5","碳钢","NULL","灰色锌镍500无红","200-300HV"]
["X0000000M14AR25514",12.4,"NFE25-514M","M14","碳钢","NULL","环保达克罗1000无红","160HV"]
["G009785016AC200HV",12.4,"GB97-85","M16","碳钢",null,"黄锌","200-300HV"]
["F002677PW12100011",12.1,"PW1210-1","0.781*1.5*0.03","碳钢",null,"本色上油"]
["F002677PW143600H1",12.1,"PW1436-H-1","5.5*10*1","45#钢","NULL","热处理本色","36-42HRC"]
["DIN7349M20AG140HV",12.06,"DIN7349","M20","碳钢","NULL","环保达克罗 720无红,0.15-0.21摩擦","140HV"]
["G0085688024AG0000",12.039,"GB856 加厚","M24","低碳钢","NULL","达克罗","NULL"]
["F135X24X2X5AL0000",12,"13109-2589","13.5*24*2.5(12/126)","碳钢","NULL","三价彩锌","100-250HV"]
["F547X125X018BA000",12,"2001-02-13","0.547*1.25*0.18","不锈钢304","NULL","不锈钢304","NULL"]
["G009785014ACHV300",12,"GB97-85","M14","45#钢",null,"黄锌","300-370HV"]
["G009785010BA200HV",12,"GB97-85","M10","不锈钢304","NULL","不锈钢304","200-300HV"]
["GB09785010AA200HV",12,"GB97.1-2002","M10","碳钢",null,"本色","200-300HV"]
["ISO7089M12RR300HV",12,"ISO7089","M12","45#钢",null,"环保达克罗500无红","300-370HV"]
["F0064X020X015BA00",12,"BN91170 6142741","6.4*20*1.5","不锈钢304","NULL","不锈钢304","NULL"]
["D000433008AKHV140",12,"DIN433","M8","碳钢",null,"三价锌","140-250HV"]
["D00127B008TA00000",12,"DIN127B","M8","磷青铜",null,"磷青铜"]
["D00127B008IE00000",12,"DIN127B","M8","弹簧钢",null,"黑磷化"]
["D00125B012AFHV200",12,"DIN125B","M12","碳钢",null,"热锌","200-250HV"]
["DIN137BM12MN00000",12,"DIN137B","M12","65锰","NULL","黑磷化","NULL"]
["XXT0000228",11.95,"NFE25-511M","M12","65Mn","NULL","上海环保达克罗0/500","420-510HV"]
["D00125A024AE200HV",11.9,"DIN125A","M10","碳钢",null,"黑磷化","200-250HV"]
["A000003$8WBA00000",11.9,"美制W型","3/8W","不锈钢304",null,"不锈钢304"]
["F0125X028X002GK00",11.9,"BN90701   6162921","12.5*28*2","45#钢",null,"黄锌24无白3um","300HV"]
["F0000000024H12900",11.8,"24H1290","0.328*0.75*0.035","Q235B",null,"三价锌TNTUV12/144/5","<302HV"]
["XXT0000303",11.7,"DIN6798A","M16","65Mn","NULL","三价锌5um","350-425HV"]
["XXT0000054",11.64,"NULL","NULL","NULL","NULL","NULL","NULL"]
["F003046PM19150011",11.61,"PM1915-1","0.75*4.625*0.06(簙钢板）","Q235","NULL","本色","NULL"]
["X0095041004000MG0",11.6,"SN60075","M12","65锰",null,"达克罗","400-500HV"]
["G009785020GD00000",11.6,"GB97-85","M20","45#钢",null,"发黑","300-370HV"]
["G084885020AY00000",11.6,"GB848-85","M20","碳钢","NULL","绿锌","140HV "]
["X0000M16AGNFE2551",11.5,"NFE25-511M","M16","65锰","NULL","环保达克罗500无红","420-510HV"]
["NFE25514L16AR0000",11.48,"NFE25-514L","M16","碳钢","NULL","环保达克罗1000无红","200HV"]
["ISO7089M20AR300HV",11.4,"ISO7089","M20","45#钢",null,"环保达克罗720无红 0.15-0.21摩擦","300-370HV"]
["F0455X10X1AA00000",11.4,"P1B0510010-00","4.55*10*1","SPCC","NULL","本色","NULL"]
["NFE25514L14AR0000",11.3,"NFE25-514L","M14","碳钢","NULL","环保达克罗1000无红","200-300HV"]
["GB96850M24AM200HV",11.22,"GB96-85","M24","碳钢",null,"三价锌72/144/5","200-300HV"]
["F0165X46X4GR300HV",11.22,"BN90701/6352238","16.5*46*4","45#钢","NULL","上海环保达克罗","300-370HV"]
["F084045002BA00000",11.21,"BN91170/3456163","8.4*45*2","碳钢","NULL","不锈钢304","NULL"]
["F0386X064X0064AR0",11.2,"12956-01209","0.386*0.64*0.064","碳钢","NULL","上海环保达克罗500无红","HRB50-100"]
["D009021003AGHV140",11.2,"DIN9021","M3","碳钢",null,"三价彩锌96无白6um","140-250HV"]
["DIN2093C28X142X08",11,"DIN2093C","14.2*28*0.8","50CrV4",null,"黑磷化"]
["DIN126M12AK000000",11,"DIN126","M12","碳钢","NULL","三价锌96无红","NULL"]
["D000679608GR012UM",11,"DIN6796","M8","65锰","NULL","环保机黄72/144/12","420-490HV"]
["X000SN70093012MI0",11,"SN70093","M12","65锰",null,"机械镀锌","440-520HV"]
["ISO7090M10AR200HV",11,"ISO7090","M10","碳钢","NULL","上海环保达克罗500无红","200-300HV"]
["XXT0000199",11,"1/4锥垫","1/4锥垫","65Mn","NULL","环保达克罗0/500","NULL"]
["XXT0000038",11,"DIN7349","M8","Q235","NULL","三价锌8um","200HV"]
["XXT0000045",11,"DIN433","M12","Q235","NULL","三价锌96无白8um","200-300HV"]
["D00137B020AD00000",10.98,"DIN137B","M20","65锰","NULL","发黑"," 其中6.6K费博瑞不能发"]
["GB97850M24AM200HV",10.96,"GB97-85","M24","碳钢","NULL","三价锌72/144/5","200-300HV"]
["DIN125AM12AL200HV",10.9,"DIN125A","M12","碳钢","NULL","三价彩锌48/72/8","200-250HV"]
["F003051PW11940004",10.9,"PW1194-4","0.688*1.25*0.105","碳钢","NULL","镀锌48/72/5","小于HRC30"]
["F00000000000909F8",10.9,"909F8(REV.1)","6.35*34.925*1.5875","不锈钢304","NULL","不锈钢304","NULL"]
["X000SN70093016MR0",10.85,"SN70093","M16","65锰",null,"环保达克罗500无红","440-520HV"]
["DIN7349M20AN100HV",10.77,"DIN7349","M20","碳钢","NULL","灰色锌镍240/1000","100HV"]
["F0000000000R70663",10.7,"R70663","R70663","45#钢",null,"机械镀锌48/96/8","30-40HRC"]
["F0060281PW3460011",10.7,"PW346-1","10.5*28*3","碳钢",null,"本色"]
["ISO7089M16CAHV200",10.6,"ISO7089","M16","不锈钢316",null,"不锈钢316","200-300HV"]
["0000000AB12000104",10.565,"1-2000-0104(REV.A1)",415060,"碳钢","NULL","镀锌","NULL"]
["DIN7349M16GR300HV",10.53,"DIN7349","M16","50CrV4",null,"上海环保达克罗1000无红","300-370HV"]
["F02858X50X3GK0000",10.53,"'03040315","1(28.58*50*3)","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["G009387010MR00000",10.5,"GB93-87","M10","65锰",null,"环保达克罗720无红","42-50HRC"]
["ISO7089M12GK300HV",10.5,"ISO7089","M12","45#钢","NULL","三价锌48/72/5","300-370HV"]
["X0L0000M08MA25514",10.5,"NFE25-514L","M8","碳钢",null,"本色"]
["XXT0000320",10.5,"DIN125B","M6","Q235","NULL","灰色锌镍0/500","200HV"]
["DIN7349M05AR140HV",10.5,"DIN7349","M5","碳钢",null,"环保达克罗 720无红,0.15-0.21摩擦,","140HV"]
["F0008X17X1HB00000",10.5,"BN91220   6243320","8*17*1","黄铜",null,"黄铜"]
["F020444839335KA40",10.5,"WA-0003-00(REV4)","WA-0003-00","H70铜",null,"H70铜"]
["F02677PW135705110",10.4,"PW1357-P-3","8.73*19.05*1.7","Q235","NULL","本色","NULL"]
["F0000000000909A46",10.39,"909A46(REV.0)","9.525*22.225*1.5875","不锈钢304","NULL","不锈钢304","NULL"]
["DIN7349M10AR200HV",10.3,"DIN7349","M10","碳钢",null,"环保达克罗720无红,0.15-0.21摩擦","200HV"]
["ISO70932M06CA0000",10.3,"ISO7093-2","M6","不锈钢316","NULL","不锈钢316","200HV"]
["F000000000N402P18",10.25,"11724-05954","N402P18","A3普碳钢","NULL","发黑上干油","140HV"]
["F003051PW144100H1",10.199999999999999,"PW1441-1","26*39*4","中碳钢 ","NULL","热处理本色","300-370HV"]
["ISO7092M12QG200HV",10.199999999999999,"ISO7092","M12","碳钢",null,"达克罗600无红","200-300HV"]
["NFE25511LM12BR000",10.199999999999999,"NFE25-511L","M12","65锰","NULL","环保达克罗1000无红","NULL"]
["XT0000183",10.199999999999999,"1619X03501","1619*03501","Q235B","NULL","黑磷化","NULL"]
["X0095024903000MG0",10.196999999999999,"DIN6799","M4","65锰",null,"达克罗","西门子"]
["F003070PW132100H1",10.19,"PW1321-1","23*44*6","65锰",null,"热处理本色","HRC36-45"]
["F0214X72X8AK00000",10.18,"SU52824","21.4*72*8","碳钢","NULL","三价锌TNTUV12/144/5","NULL"]
["DIN0433M16ALHV200",10.1,"DIN433","M16","碳钢",null,"三价彩锌72/120/8上封闭","200-300HV"]
["F064X16X15CA200HV",10.1,"6.4*16*1.5","6.4*16*1.5","不锈钢316","NULL","不锈钢316","200HV"]
["D000434012AF00000",10.02,"DIN434-1990","M12","碳钢",null,"热锌"]
["D00125A012AAHV200",10,"DIN125A","M12","碳钢",null,"本色","200-250HV"]
["D00125A012ADHV140",10,"DIN125A","M12","碳钢",null,"发黑","140-250HV"]
["00000AKN402AP42B6",10,"BN90701 6074865","N402AP42B6","碳钢","NULL","三价锌 72无红 5um","NULL"]
["ASPRWASHERBA05$16",10,"美制标准弹垫","'5/16","不锈钢316","NULL","不锈钢316","NULL"]
["DIN0433M04AKHV200",10,"DIN433","M4","碳钢",null,"三价彩锌48/72/5","200-300HV"]
["D009021010AGHV140",10,"DIN9021","M12","碳钢",null,"达克罗","140-250HV"]
["D00137B010JAL00000",10,"DIN137B","M10","65锰",null,"机械镀锌"]
["D00128A012BA00000",10,"DIN128A","M12","不锈钢304","NULL","不锈钢304","NULL"]
["D00127B016BA00000",10,"DIN127B","M16","不锈钢304",null,"不锈钢304"]
["F0011X33X12BA0000",10,"BN91170   6147437","11*33*1.2","不锈钢304","NULL","不锈钢304","NULL"]
["F000000000MK10-00",10,"美制标准型弹垫","10#","65锰",null,"机械镀锌36无红5um"]
["DIN7349M06AK5UM",10,"DIN7349","M6","碳钢","NULL","三价锌5um","NULL"]
["X0095020746000MG0",10,"DIN6799","M8","65锰",null,"达克罗","西门子"]
["X06798A010MK00000",10,"DIN6798A","M10","65锰","NULL","三价锌","350-425HV"]
["X0000000M10MI9250",10,"DIN9250","M10","65锰",null,"机械镀锌"]
["SN70093M10MK00000",10,"SN70093","M10","65锰",null,"机械镀锌48/144/12","440-520HV"]
["ISO7093M10AR00000",10,"ISO7093","M10","Q235",null,"GEOMET（R）500无红","200-300HV"]
["ISO7093M08ANHV200",10,"ISO7093","M8","碳钢","NULL","黑色锌镍720无红8um","200-300HV"]
["ISO7093M3X5AK0000",10,"ISO7093","M3.5","碳钢","NULL","三价锌96无红","200-300HV"]
["ISO7090M10AB200HV",10,"ISO7090","M10","碳钢",null,"镀锌96无红8um","200-300HV"]
["XXT0000022",10,"DIN9021","M12","Q235","NULL","Geomet321VL1000无红","200-300HV"]
["XXT0000204",10,"DIN6796","M6","65Mn","NULL","机械镀锌72/144/12um","420-490HV"]
["XXT0000052",10,"DIN125A","M5","Q235","NULL","三价锌96无白12um","200-250HV"]
["XXT0000311",10,"DIN9021","M8","Q235","NULL","黄锌48/72/5","140-250HV"]
["XXT0000277",10,"DIN9021","M16","Q235","NULL","三价彩锌72/216/8um","200-300HV"]
["D06796012ME50CRV4",9.9,"DIN6796","M12","50CrV4","NULL","黑磷化","420-510HV;7k封存"]
["A0000003$4MF015UM",9.8000000000000007,"美制标准弹垫","'3/4","65锰",null,"机械镀锌15um"]
["ISO7089016AR200HV",9.8000000000000007,"ISO7089","M16","碳钢",null,"上海环保达克罗500无红","200-300HV"]
["G009685024AB00000",9.6999999999999993,"GB96-85","M24","碳钢",null,"镀锌"]
["F00N400P45BA00000",9.6999999999999993,"BN91170   6204472","N400P45","不锈钢304","NULL","不锈钢304 钝化","200HV"]
["D007980012ID00000",9.6989999999999998,"DIN7980","M12","弹簧钢",null,"发黑","HRC42-50"]
["A00000001WBA00000",9.6769999999999996,"WA-0013-00(REV0)","1''W","不锈钢304","NULL","不锈钢304","NULL"]
["F0838X1703X318AK0",9.61,"12338-00224","8.38*17.03*3.18","A3普碳钢",null,"三价锌"]
["G009685014AA00000",9.6,"GB96-85","M14","碳钢",null,"本色"]
["GB962002016AK0000",9.6,"GB96.1-2002","M16","碳钢","NULL","三价锌48/72/5","200-300HV"]
["D00127B004IH00000",9.6,"DIN127B","M4","弹簧钢","NULL","三价黑锌","NULL"]
["D007349012AC140HV",9.6,"DIN7349","M12","碳钢","NULL","黄锌72无白8-12um","140HV"]
["F00203*0438*0063BA",9.6,"BN91170 6130987","0.203*0.438*0.063","不锈钢304","NULL","不锈钢304  ","200HV"]
["XXT0000238",9.5,"SN70093","M10","65Mn","NULL","机械镀锌上不封闭","440-520HV"]
["NFE25514M10AR0000",9.5,"NFE25-514M","M10","碳钢","NULL","环保达克罗1000无红","160-250HV"]
["F002677PW122600H1",9.41,"PW1226-H-1","25.4*40*5","45#钢",null,"热处理本色上油","HRC36-42"]
["D007349012AKHV140",9.1999999999999993,"DIN7349","M12","碳钢","NULL","三价锌","140HV"]
["D00125A016AC140HV",9.1999999999999993,"DIN125A","M16","碳钢",null,"黄锌","140-250HV"]
["ISO7093M12AK005UM",9.1999999999999993,"ISO7093","M12","碳钢","NULL","三价锌6/24/5不上封闭","200-300HV"]
["ISO7093M12CA00000",9.1999999999999993,"ISO7093","M12","不锈钢316","NULL","不锈钢316","NULL"]
["XXT0000024",9.1999999999999993,"ISO7093","M10","50#","NULL","本色","300HV"]
["DIN7349M16AN200HV",9.19,"DIN7349","M16","材质不指定",null,"灰色锌镍240/1000","200HV"]
["F050X615X2AK00000",9.1300000000000008,"BN90700  6305328","SWT671 50*61.5*2","Q235",null,"三价锌12/36/5"]
["F0000000024M73590",9.1,"24M7359","23*39*3","235B","NULL","三价锌TNTUV12/144/5","200-300HV"]
["F00000000024H1853",9,"24H1853","24H1853","A3普碳钢",null,"本色","外销柏中"]
["D0004332X5BA200HV",9,"DIN433","M2.5","不锈钢304","NULL","不锈钢304","200HV"]
["A200002523",9,200002523,"GB93-87 M12","弹簧钢",null,"发黑","42-50HRC"]
["D009021008AGHV140",9,"DIN9021","M8","碳钢","NULL","达克罗500无红","140-250HV"]
["DIN125B010AK200HV",9,"DIN125B","M10","碳钢",null,"三价锌96无红8um","200-250HV"]
["G009387010MG01000",9,"GB93-87","M10","65锰",null,"达克罗1000无红","42-50HRC"]
["F0BN90618$6084218",9,"BN90701 6084218","15*16.95","碳钢","NULL","本色","NULL"]
["G009785012BA200HV",9,"G97-85","M12","不锈钢304","NULL","不锈钢304","200-300HV"]
["XXT0000235",9,"NFE25-514M","M5","Q235","NULL","灰色锌镍0/72/8um","NULL"]
["X00M08000CA25514M",9,"NFE25-514M","M8","不锈钢316",null,"不锈钢316","150HV"]
["FBN90701$6103683C",8.89,"BN90701/6103683","19*55*3","碳钢","NULL","黄锌","NULL"]
["F0000000AK24H1138",8.83,"24H1138","1.062*2*0.134","Q235",null,"三价锌TNTVU12/144/5","<302HV"]
["X000000M14MK25511",8.8000000000000007,"NFE25-511M","M14","65锰","NULL","机械镀锌","NULL"]
["XXT0000008",8.8000000000000007,"DIN125A","M18","Q235B","NULL","三价锌48/72/8","NULL"]
["DIN6796M10MR00000",8.6999999999999993,"DIN6796","M10","65锰","NULL","环保达克罗720无红","420-490HV"]
["D009021012KC140HV",8.6999999999999993,"DIN9021","M12","碳钢",null,"三价彩锌72/144/8","140-250HV"]
["F003049PW96000011",8.65,"PW960-1","0.406*0.719*0.12","碳钢",null,"本色"]
["D007089027AAHV200",8.6,"ISO7089","M27","碳钢",null,"本色","200-300HV"]
["F003051PW115800@M",8.57,"PW1158-1","13*40*5","45#钢",null,"机械镀锌48/96/5","300-370HV"]
["D006340008GD00000",8.5,"DIN6340","M8","45#钢","NULL","发黑","350-430HV"]
["DIN127BM04MI00000",8.5,"DIN127B","M4","弹簧钢","NULL","三价锌5um ","NULL"]
["XT0000213",8.5,"8#美制弹垫B型","8#美制弹垫B型","不锈钢304","NULL","A2","NULL"]
["F00000000024H16280",8.49,"24H1628","24H1628","Q235",null,"三价锌TNTUV12/144/5","200-300HV"]
["F082X45X18X05BAE0",8.48,"DM-20234-012-AE","8.2*45*18*0.5","不锈钢304","NULL","不锈钢304","NULL"]
["ISO7089030GD300HV",8.4559999999999995,"ISO7089","M30","45#钢",null,"发黑上油","300-370HV"]
["D000435016AK00000",8.4499999999999993,"DIN435","M16","A3普碳钢",null,"三价锌"]
["GB09387M03ML00000",8.4,"GB93-87","M3","65锰",null,"三价彩锌72/144/5","42-50HRC"]
["G088588010AK00000",8.4,"GB855","M10","低碳钢","NULL","三价锌","NULL"]
["G085488012AA00000",8.4,"GB854","M12","低碳钢",null,"本色"]
["G009685012AG00000",8.4,"GB96-85","M12","碳钢",null,"达克罗500无红","140-250HV"]
["D00125B016CA200HV",8.3000000000000007,"GB97.2-85","M16","不锈钢316",null,"不锈钢316","200HV"]
["D007349010ANHV200",8.3000000000000007,"DIN7349","M10","材料不指定",null,"灰色锌镍240/1000","200HV"]
["F000000AK24H1737",8.2899999999999991,"24H1737","0.531*1.438*0.18","碳钢",null,"三价锌TNTUV12/144/5","<302HV"]
["F0656X275X018AK00",8.2690000000000001,"24H1852","0.656*2.75*0.18","Q235",null,"三价锌TNTVU12/144/5","<302HV"]
["XXT0000240",8.1999999999999993,"DIN6340","M8","45#","NULL","Geomet321A+ML","350-430hv"]
["F0000012NFE2511MI",8.1999999999999993,"NFE25-511M","M12","65锰",null,"机械镀锌"]
["X001440016BA140HV",8.1300000000000008,"DIN1440","M16","不锈钢304",null,"不锈钢304","西门子"]
["XXT0000081",8.1,"DIN7349","M12","50CrV4","NULL","达克罗720无红","300HV"]
["D00127B020IG00000",8.1,"DIN127B","M20","弹簧钢",null,"达克罗"]
["F000000AK24H13510",8.06,"24H1351","0.562*1.5*0.164","碳钢",null,"三价锌TNTUV 12/144/5","<302HV"]
["F000000024M731500",8.0500000000000007,"24M7315","17* 50* 3","Q235B",null,"三价锌TNTUV12/144/5","200-300HV"]
["F0000000AK24H1498",8,"24H1498","1.281 * 2.125 *0.12","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["D001440M08AA00000",8,"DIN1440","M8","碳钢",null,"本色","140HV"]
["D00125A008ABHV140",8,"DIN125A","M8","碳钢",null,"镀锌","140-250HV"]
["D000127B006IK0000",8,"DIN127B","M6","弹簧钢",null,"三价锌"]
["XDIN4712412MD0000",8,"DIN471","M24*1.2","65锰",null,"发黑"]
["XXT0000270",8,"GB93-87","M20","65Mn","NULL","三价锌5um","NULL"]
["XXT0000268",8,"DIN7349","M4","Q235","NULL","机械镀锌24/72/5um","200-300HV"]
["XXT0000313",8,"DIN1440","M8","Q235","NULL","三价锌","160-250HV"]
["NFE25514LM10AG000",8,"NFE25-514L","M10","碳钢","NULL","环保达克罗1000无红","160HV"]
["F085X19X12BA00000",8,"BN91170/6225397","8.5*19*1.2","不锈钢304",null,"不锈钢304"]
["F0406X125X018BA00",8,"'3/8-16","245A2902P8","A3普碳钢",null,"三价锌3um","140HV"]
["F105025025AI200HV",8,"BN91170   6166270","10.5*25*2","碳钢","NULL","机械镀锌12um","200HV"]
["G084885010ABHV200",8,"GB848-85","M10","碳钢",null,"镀锌","200-300HV"]
["D000472M42MG00000",7.984,"DIN472","M42*1.75","65锰",null,"磷化"]
["ISO7093M06GN300HV",7.9119999999999999,"ISO7093","M6","45#钢","NULL","灰色锌镍500无红","300-370HV"]
["X009300016AG00000",7.9,"DIN93","M16","碳钢","NULL","环保达克罗500无红","NULL"]
["F0LG623004B01GG00",7.9,"LG6230.04B-01","17*45*4","45#钢","NULL","达克罗720无红","NULL"]
["G085888036AD00000",7.8630000000000004,"GB858-88","M36","Q235","NULL","发黑","NULL"]
["F02677PW11320011P",7.83,"PW1132-P-2","19*60*9","40Cr","NULL","不热处理本色","NULL"]
["F003046PW11760011",7.82,"PW1176-1","0.687*1.25*0.25","45#钢",null,"不热处理本色"]
["D006340008GL005UM",7.8,"DIN6340","M8","45#钢","NULL","三价彩锌48/72/5","350-430HV"]
["DIN125A007BA140HV",7.8,"DIN125A","M7","不锈钢304",null,"不锈钢304","140-250HV"]
["ISO7092M22AK200HV",7.8,"ISO7092","M22","碳钢","NULL","三价彩锌120/264/8","200-300HV"]
["F002677PW11410011",7.7850000000000001,"PW1141-1","3.015*4.22*0.075","Q235",null,"不热处理本色"]
["DIN125A020ARHV200",7.7,"DIN125A","M20","碳钢",null,"上海环保达克罗500无红","200-250HV"]
["F064X195X15BA0000",7.7,"DM-20381-001-AA","6.4*19.5*1.5","不锈钢304",null,"不锈钢304"]
["F0000000000T47576",7.68,"T47576","0.905*1.496*0.194","45#",null,"热处理本色","30-38HRC"]
["XXT0000202",7.65,"5/8美制弹垫","5/8美制弹垫","65Mn","NULL","机械镀锌15um","NULL"]
["DIN440M010AA100HV",7.63,"DIN440","M10","碳钢",null,"本色","100-250HV"]
["F002677PW13370011",7.62,"PW1337-P-1","10.31*38.1*4.78","45#钢",null,"不热处理本色"]
["DINEN14399MB20000",7.5,"EN14399-6","M20","45#钢","NULL","镀锌","300-370HV"]
["D100433008AKHV200",7.5,"DIN433","M8","碳钢",null,"三价锌72无红5um","200-300HV"]
["A000001$2NBA00000",7.5,"美制N型","1/2N","不锈钢304",null,"不锈钢304"]
["XXT000014",7.5,"DIN9021","M8","Q235","NULL","黑色锌镍0/720/5um","200HV"]
["ISO7093M08ARHV200",7.5,"ISO7093","M8","碳钢","NULL","环保达克罗1000无红","200-300HV"]
["F064125016AK008UM",7.5,"BN90700   6156316","6.4*12.5*1.6","碳钢","NULL","三价黄锌72/144/8","NULL"]
["ISO7093M10AR200HV",7.46,"ISO7093","M10","碳钢",null,"环保达克罗720无红摩擦0.15-0.21","200-300HV"]
["XXT0000004",7.4,"NULL","NULL","NULL","NULL","NULL","NULL"]
["G009785020ACHV200",7.4,"GB97-85","M20","碳钢",null,"黄锌","200-300HV"]
["DIN7349008AL005UM",7.4,"DIN7349","M8","碳钢","NULL","三价彩锌48/72/5","200HV"]
["DIN634M010GK00000",7.4,"DIN6340","M10","45#钢","NULL","三价锌","350-430HV"]
["F003051PW1071000C",7.4,"PW1071-1","16.3*32*2","低碳钢","NULL","三价彩锌48/72/5","≤302HV"]
["F002677PW11740011",7.32,"PW1174-1","13.5*57*6","45#钢",null,"不热处理本色"]
["G009585030AF00000",7.3029999999999999,"GB95-85","M30","碳钢",null,"热锌"]
["F0032X045X05BA000",7.3,"DIN988","32*45*0.5","不锈钢304",null,"不锈钢304"]
["DIN09021008AG1000",7.3,"DIN9021","M8","碳钢",null,"达克罗1000无红","200-250HV"]
["D001440010BAHV140",7.3,"DIN1440","M10","不锈钢304","NULL","不锈钢304","NULL"]
["F0133X60X3GA00000",7.2,"P1I1460030-00","13.3*60*3","35#钢","NULL","不热处理本色","NULL"]
["D006340030GK00000",7.1950000000000003,"DIN6340","M30","65锰","NULL","黄锌","350-430HV"]
["G009685020AG200HV",7.15,"GB96-85","M20","碳钢",null,"达克罗500无红","200-300HV"]
["G085488020AG00000",7.1,"GB854","M20","低碳钢",null,"达克罗"]
["F00164X323X026000",7.1,"SN70093","M16","65锰",null,"机械镀锌12um","440-520HV"]
["F0043X014X08AK000",7,"BN90701   6147166","4.3*14*0.8","碳钢",null,"三价锌24无白","140HV"]
["F011X18X1BA000000",7,"13107-02076","11*18*1","不锈钢304","NULL","不锈钢304","NULL"]
["F00N418P11BA00000",7,"BN91170   6204474","N418P41(1/4弹垫）","不锈钢304","NULL","不锈钢304 不导磁（钝化）","NULL"]
["F0255X40X15AK0000",7,"BN90701/3777583","25.5*40*1.5","Q235",null,"三价锌","140HV"]
["D00125B010CAHV140",7,"DIN125B","M10","不锈钢316",null,"不锈钢316","140HV"]
["F0339X114X0108AH0",7,"BN90701 6343012","5/16(0.339*1.14*0.108)","碳钢","NULL","黑色环保达克罗840无红","NULL"]
["XXT0000048",7,"DIN125A","M10","65Mn","NULL","热锌","300HV"]
["XXT0000196",7,"6#N","6#N","Q235","NULL","上达环保0/600","NULL"]
["XXT0000200",7,"8.21*15.33*2","8.21*15.33*2","Q235","NULL","三价锌72/96/5","NULL"]
["X000432020AC00000",7,"DIN432","M8","碳钢",null,"黄锌","西门子"]
["F00152X002X0031BA",6.95,"BN91170  6130478","1.52*2*0.031","不锈钢304",null,"不锈钢304","200HV"]
["G089486060MD00000",6.8979999999999997,"GB894.1","M60","65锰",null,"发黑"]
["A300004093",6.89,300004093,"DIN6799 M8","65Mn","NULL","达克罗"]
["D009021012AC008UM",6.8,"DIN9021","M12","碳钢","NULL","黄锌72/144/8","140-250HV"]
["X0004712012MG0000",6.8,"DIN471","M20*1.2","65锰","NULL","达克罗500无红","NULL"]
["G085288016AA00000",6.75,"GB852-88","M16","碳钢","NULL","本色","NULL"]
["ISO7089M18AK200HV",6.7249999999999996,"ISO7089","M18","碳钢","NULL","三价锌48/72/5","200-300HV"]
["F040X204X25HN0000",6.7,"BN806  1283316","40*20.4*2.5（锥垫）","50Crv4","NULL","黑磷化","NULL"]
["F02X0375X0036AK00",6.7,"BN90701 6334005","0.2*0.375*0.036","碳钢","NULL","三价锌24/72/5","200-300HV"]
["F0281X075X001AK00",6.6,"BN90701   6111252","0.281*0.75*0.1","碳钢",null,"三价黄锌48/72/5","140HV"]
["NFE25$518LM10AG00",6.6,"NFE25-518L","M10","45#钢","NULL","环保达克罗1000无红","310HV"]
["D007349010ACHV200",6.6,"DIN7349","M10","碳钢","NULL","黄锌5um"," 200HV"]
["D00127B016IG00720",6.5,"DIN127B","M16","弹簧钢","NULL","环保达克罗720无红","NULL"]
["D009021012AFHV200",6.5,"DIN9021","M12","碳钢",null,"热锌","200-250HV"]
["A200001743",6.5,200001743,"SN70093 M16","65Mn",null,"环保达克罗0/500","440-520HV"]
["F0000000AK0600000",6.5,"12061-01624","6# 美制非标平垫","Q235","NULL","三价锌","NULL"]
["XXT0000067",6.5,"DIN433","M8","Q235","NULL","环保达克罗 720无红","200-250HV"]
["XXT0000308",6.5,"5*12*1.5","5*12*1.5","Q235B","NULL","三价彩锌72/120/8um上封闭","160-250HV"]
["F055X20X16GA00000",6.5,"P1I0620016-01","5.5*20*1.6","35#钢",null,"不热处理本色"]
["F00N400P41BA00000",6.44,"BN91170   6201514","N400P41","不锈钢304",null,"不锈钢304"]
["F017X42X4AK000000",6.4,"BN90701   6043502","17*42*4","Q235",null,"三价锌","140HV"]
["F002577PW1085002F",6.4,"PW1085-2","17*34*2","碳钢",null,"黄锌48/72"]
["F00000000024M7526",6.4,"24M7526","31*50*4(30/433)","45#钢","NULL","环保达克罗960无红","300-370HV"]
["G009785020AG10000",6.4,"GB97-85","M20","45#钢",null,"达克罗1000无红","300-370HV"]
["XXT0000324",6.4,"DIN9021","M12","Q235","NULL","环保达克罗0/1000","200-300HV"]
["ISO7090M16AR200HV",6.4,"ISO7090","M16","碳钢","NULL","环保达克罗720无红","200-300HV"]
["F0BN45694$3731988",6.31,"24M7629","12.5*45*3","45#钢",null,"机械镀锌","300-370HV"]
["GB09387M24MK00000",6.3,"GB93-87","M24","65锰",null,"三价锌72/144/5","42-50HRC"]
["X00000M014AR25514L",6.3,"NFE25-514L","M14","碳钢","NULL","环保达克罗500无红","160-250HV"]
["F0000AK259A3370P1",6.3,"BN90700  6074861","259A3370P1","碳钢",null,"三价锌72无红5um"]
["XXT0000307",6.27,"21.5*42*5","21.5*42*5","45#","NULL","热处理本色","NULL"]
["F040X50X25AN00000",6.27,"DIN988","40*50*2.5","Q235","NULL","黑磷化+防锈油","NULL"]
["GB9387M16MH000000",6.2,"GB93-87","M16","65锰","NULL","三价黑锌","42-50HRC"]
["F000N402AP47AK000",6.2,"BN90701 6202918","N402AP47","碳钢",null,"三价黄锌(518Y)48/72/5","140HV"]
["D009021008CA00000",6.2,"DIN9021","M8","不锈钢316",null,"不锈钢316"]
["XXT0000064",6.0960000000000001,"NULL","NULL","NULL","NULL","NULL","NULL"]
["F003046PQ14360011",6.085,"PW1439-1","1.313*2.375*0.048","Q235","NULL","本色","NULL"]
["F0060120050AR0000",6,"DIN988","6*12*0.5","碳钢",null,"环保达克罗500无红"]
["F013X40X4AF000000",6,"BN90701 6302593","DIN522A  13*30*4","碳钢","NULL","热锌","200-250HV"]
["F016028003BA00000",6,"BN91170/3218613","16*28*3","不锈钢304","NULL","不锈钢304","NULL"]
["DIN0433016AKHV140",6,"DIN433","M16","碳钢",null,"三价锌5um","140-250HV"]
["D009021016AKHV200",6,"DIN9021","M16","碳钢",null,"三价锌","200-250HV"]
["DIN125AM10AH140HV",6,"DIN125A","M10","碳钢","NULL","三价黑锌5um","140-250HV"]
["D00127B012IF00000",6,"DIN127B","M12","弹簧钢",null,"热锌"]
["D007349008AL005UM",6,"DIN7349","M8","45#钢",null,"三价彩锌5um","200-300HV"]
["X00000M12BA25514M",6,"NFE25-514M","M12","不锈钢304",null,"不锈钢304"]
["X000471010MD00018",6,"DIN471","M10","65锰",null,"发黑","b=1.8(+0.2/-0.1）"]
["X009300010AC00000",6,"DIN93","M10","碳钢","西门子(单耳)西","黄锌","NULL"]
["ISO7093M03AL200HV",6,"ISO7093","M3","碳钢","NULL","三价彩锌72/120/5","200-300HV"]
["GB9387M12MN000000",6,"GB93-87","M12","65锰","NULL","灰色锌镍720无红8um","42-50HRC"]
["GB97200210GA00000",6,"GB97.1-2002","M10","45#钢","NULL","不热处理本色","NULL"]
["F7X25X15BA0000000",6,"12725-00205","7*25*1.5","不锈钢304",null,"不锈钢304"]
["D00125A024AAHV300",5.91,"DIN125A","M24","45#钢",null,"本色","300-400HV"]
["D006796022GM012UM",5.9,"DIN6796","M22","60Si2MnA",null,"达克罗500无红","420-490HV"]
["DIN127B020IR00720",5.9,"DIN127B","M20","弹簧钢",null,"环保达克罗720无红"]
["DIN434M16AR200000",5.9,"DIN434-2000","M16","Q235",null,"环保达克罗 720无红,0.15-0.21摩擦","100-250HV"]
["F023044004AK00000",5.9,"23*44*4","23*44*4","碳钢","NULL","三价锌","NULL"]
["F121226001BA00000",5.9,"BN91170 6075872","12.1*22.6*1","不锈钢304",null,"不锈钢304"]
["F07X14X08BA000000",5.9,"13109-06951","7*14*0.8","不锈钢304",null,"不锈钢304"]
["XXT0000291",5.9,"DIN125A","M14","Q235","NULL","环保达克罗0/500","200HV"]
["XXT0000040",5.8,"DIN125A","M4","Q235","NULL","三价锌5um","200-250HV"]
["X0095047857000CA0",5.8,"SWT671","50*61.5*2","碳钢","NULL","黄锌","西门子"]
["F0153X0322X0029AK",5.8,"BN90701   6220342","0.153*0.322*0.029","碳钢",null,"三价黄锌120无白8um"]
["F000115041032GA00",5.8,"Q181241032","11.5*41*3.2","45#钢",null,"不热处理本色","明泰"]
["F02677PW121300H2",5.75,"PW1213-H-2","10.2*40*3","45#钢",null,"本色上油","HRC36-42"]
["F0L401P35MG000000",5.7229999999999999,"BN90704   6233817","L401P35（弹垫）","65锰","NULL","环保达克罗720无红，0.15-0.21摩擦","HRC38-46"]
["X06798A024MD00000",5.7,"DIN6798A","M24","65锰","NULL","黑磷化","350-425HV"]
["A00000005$8MI0000",5.7,"美制标准型弹垫","'5/8","65锰",null,"机械镀锌15um","柏中可用"]
["F013X025X001BA000",5.66,"BN91170/3866835","13*25*1","不锈钢304",null,"不锈钢304"]
["F003046PW11760012",5.66,"PW1176-2","0.687*1.25*0.25","45#钢","NULL","不热处理本色","NULL"]
["XXT0000274",5.65,"WA-0038-04P","WA-0038-04P","45#","NULL","发黑","39-44HRC"]
["G08482002030AB000",5.65,"GB848-2002","M30","碳钢","NULL","镀锌","200-300HV"]
["G009585014AK00000",5.6,"GB95-85","M14","碳钢","NULL","三价锌6/24/3","NULL"]
["ISO7090M12AN200HV",5.6,"ISO7090","M12","碳钢","NULL","灰色锌镍500无红","200-300HV"]
["G085388010AA00000",5.5,"GB853-88","M10","碳钢","NULL","本色","NULL"]
["DIN125A016ARHV300",5.5,"DIN125A","M16","45#钢",null,"上海环保达克罗500无红","300-400HV"]
["D009021008AAHV200",5.5,"DIN9021","M8","碳钢",null,"本色","200-250HV"]
["D00137B016AI012UM",5.4,"DIN137B","M16","65锰",null,"机械镀锌"]
["F000N402AP75AK000",5.4,"BN90701   6202921","N402AP75","A3普碳钢",null,"三价黄锌(518Y)48/96/5","140HV"]
["F011X23X55AL00000",5.4,"DIN522A","11*23*5.5","碳钢","NULL","三价彩锌120/264/8上封闭","NULL"]
["D00125A014BAHV200",5.37,"DIN125A","M14","不锈钢316",null,"不锈钢316","200-250HV"]
["GB85688030AG00000",5.35,"GB856","M30*2","低碳钢","NULL","达克罗","NULL"]
["ISO70932M8BA200HV",5.3,"ISO7093-2","M8","不锈钢304",null,"不锈钢304","200HV"]
["ISO7094008AK100HV",5.3,"ISO7094","M8","碳钢",null,"三价锌48/72/5","100-200HV"]
["X0095040027000AA0",5.3,"DIN9021","M16","不锈钢304",null,"不锈钢304","西门子"]
["F095X25X2GA000000",5.24,"Q181025020-2","9.5*25*2","35#钢","NULL","本色","HRC20-29"]
["GB972M24GD0000000",5.2,"GB97.2-85","M24","45#钢","NULL","发黑","300-370HV"]
["XXT0000017",5.2,"DIN125A","M14","Q235","NULL","三价锌48/72/12um","200-250HV"]
["D00127B014ID00000",5.2,"DIN127B","M14","弹簧钢","NULL","发黑","NULL"]
["F0000000000A83999",5.165,"A83999","A83999","45#",null,"机械镀锌"]
["A300001691",5.1429999999999998,300001691,"29*88.9*4.76","65Mn",null,"达克罗0/500","30-38HRC"]
["F029X889X476MG000",5.1429999999999998,"BN90701  6149713","29*88.9*4.76","65锰",null,"达克罗500无红","HRC30-38"]
["F0BZ210A013MD4700",5.0999999999999996,"BZ210A-013","D47","65锰",null,"发黑HRC45-50","非标波型垫"]
["DIN434M12AG000000",5.0999999999999996,"DIN434-2000","M12","碳钢","NULL","环保达克罗720无红0.15-0.21摩擦","100-250HV"]
["F017X27X1QA000000",5.0999999999999996,"17*27*1","17*27*1","Q235",null,"本色上油","艾维尼尔森"]
["D007349024AR00000",5.0599999999999996,"DIN7349","M24","Q235","NULL","环保达克罗 720无红，0.15-0.21摩擦","140HV"]
["G085688016AK00000",5.0599999999999996,"GB856","M16","低碳钢",null,"三价锌"]
["F09X40X3CA0000000",5.0199999999999996,"BN91170 6336946","9*40*3","不锈钢316","NULL","不锈钢316","NULL"]
["F084X20X4AK000000",5,"BN90700  6305121","SWT671 8.4*20*4","Q235",null,"三价锌12/36/5"]
["X0L0000M20MR25514",5,"NFE25-514M","M20","碳钢",null,"上海环保达克罗","500无红"]
["XXT0000144",5,"DIN7349","M8","Q235","NULL","上海环保达克罗0/720，摩0.15~0.21","200~300HV"]
["XXT0000323",5,"DIN125A","M12","45#","NULL","上海环保达克罗0/1000","300HV"]
["X0047121X1MD00000",5,"DIN471","M21","65锰",null,"发黑"]
["SN70093010GI012UM",5,"SN70093","M10","65锰",null,"机械镀锌不上封闭48/144/12加Oil WD40","440-520HV"]
["ISO7093M05CAHV200",5,"ISO7093","M5","不锈钢316","NULL","不锈钢316钝化","200-300HV"]
["ISO7089M16AFHV200",5,"ISO7089","M16","碳钢",null,"热锌","200-300HV"]
["D00128A004MA00000",5,"DIN128A","M4","弹簧钢","NULL","本色","44-51HRC"]
["DIN127B010IR01000",5,"DIN127B","M10","弹簧钢","NULL","达克罗500无红","NULL"]
["DIN125B012AKHV200",5,"DIN125B","M12","碳钢",null,"三价锌96无红8um","200-250HV"]
["DIN125AM20AR140HV",5,"DIN125A","M20","碳钢","NULL","上海环保达克罗1000无红","140-250HV"]
["DIN127B006IA00000",5,"DIN127B","M6","弹簧钢",null,"本色","HRC44-51"]
["D000126006AKHV100",5,"DIN126","M6","碳钢",null,"三价锌","100-250HV"]
["A200000148",5,200000148,"DIN6797A M8","304不锈钢",null,"本色"]
["D00125A006AAHV200",5,"DIN125A","M6","碳钢",null,"本色","200-250HV"]
["F0121X20X2BA00000",5,"DM-20223-001-AA","12.1*20*2","不锈钢304",null,"不锈钢304"]
["DIN7349M12AG200HV",5,"DIN7349","M12","碳钢","NULL","环保达克罗720无红","200HV"]
["F0000000ALGP90672",5,"GP90672","GP90672","A3普碳钢",null,"三价彩锌","杰普洛"]
["XXT0000225",4.95,"DIN9021","M12","Q235","NULL","三价彩锌96/120/8um","100HV"]
["X0000000M16AR2551",4.9000000000000004,"NFE25-511M","M16","65锰","NULL","上海环保达克罗500无红","NULL"]
["F06027PW12650001S",4.9000000000000004,"PW1265-3","10.5*25*3","不锈钢316",null,"不锈钢316","94HRB"]
["G009685024ABHV140",4.9000000000000004,"GB96-85","M24","碳钢",null,"镀锌","140-250HV"]
["F000013028004AK00",4.9000000000000004,"BN716   1267876","13*28*4","碳钢","NULL","三价锌","NULL"]
["F013019005BA00000",4.9000000000000004,"BN91100 6012945","DIN988 13*19*0.5","不锈钢304","NULL","不锈钢304","NULL"]
["D007980012IK005UM",4.9000000000000004,"DIN7980","M12","弹簧钢",null,"三价锌5um"]
["DINEN14399M220000",4.84,"DIN EN14399-6","M22","45#钢","NULL","达克罗500无红","300-370HV"]
["DIN7349030ANHV200",4.8090000000000002,"DIN7349","M30","材质不指定","NULL","灰色锌镍240/1000","100HV"]
["F013X32X2AB000000",4.8,"DM-20229-002-AA","13*32*2","Q235A","NULL","镀锌9um","NULL"]
["D007980016AK005UM",4.8,"DIN7980","M16","弹簧钢",null,"三价锌5um"]
["D007980020IL00000",4.8,"DIN7980","M20","弹簧钢",null,"机械镀锌"]
["00000AK245A2902P5",4.8,"245A2902P5","245A2902P5","碳钢","NULL","三价锌 24无红 5um","NULL"]
["A200005155",4.8,200005155,"DIN125A M16","碳钢",null,"热镀锌","140-250HV"]
["G08482002024AD000",4.8,"GB848-2002","M24","碳钢","NULL","发黑","200-300HV"]
["G005287008AL00000",4.8,"GB5287","M8","碳钢","NULL","三价彩锌","NULL"]
["ISO7093M10AG00000",4.8,"ISO7093","M10","碳钢","NULL","环保达克罗1000无红","200-300HV"]
["ISO7093M12GD300HV",4.8,"ISO7093","M12","45#钢",null,"达克罗1000无红","300-370HV"]
["XXT0000028",4.8,"SN70093","M10","65Mn","NULL","机械镀锌不上封闭48/144/12","NULL"]
["F020X44X26X2BA000",4.7850000000000001,"DM-20260-001-AB","20*44*26*2(卡垫)","不锈钢304","NULL","不锈钢304","NULL"]
["DINEN14399M200000",4.7670000000000003,"DIN EN14399-6","M20","45#钢","NULL","达克罗","300-370HV"]
["F06X15X40X15BAE00",4.74,"DM-20234-001-AE","6*15*40*0.5","不锈钢304","NULL","不锈钢304","NULL"]
["G009387020MF00000",4.7,"GB93-87","M20","65锰",null,"热锌","HRC30"]
["F00L400P33AK00000",4.7,"BN90701  6308571","L400P33","Q235",null,"三价彩锌48/72/5"]
["F0000000AK24H1825",4.68,"24H1825","0.668*1.5*0.194","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["D00125B020AB00000",4.5999999999999996,"GB97.2-85","M20","碳钢",null,"镀锌"]
["D007349004AKHV140",4.5999999999999996,"DIN7349","M4","碳钢","NULL","三价锌","140HV"]
["D007349016AKHV200",4.5999999999999996,"DIN7349","M16","碳钢","NULL","三价锌","200HV"]
["F0002677PW1134011",4.57,"PW1134-P-1","63*100*9","碳钢",null,"本色","140HV"]
["F00265X005X0063BA",4.5,"BN91170   6130988","0.265*0.5*0.063","不锈钢304",null,"不锈钢304","200HV"]
["F0125X30X3AK200HV",4.5,"BN90701 6339074","12.5*30*3","碳钢","NULL","三价锌24/48/5","200-300HV"]
["DIN7349M12AR200HV",4.5,"DIN7349","M12","碳钢","NULL","Geomet+VL500无红","200HV"]
["D006796010GR012UM",4.5,"DIN6796","M10","65锰","NULL","环保机械黄锌72/144/12","420-490HV"]
["D00127B014IR00720",4.5,"DIN127B","M14","弹簧钢","NULL","环保达克罗720无红","NULL"]
["XXT0000035",4.5,"DIN125B","M16","45#","NULL","灰色锌镍500无红","300-370HV"]
["XXT0000309",4.5,"DIN9021","M8","Q235","NULL","黄锌5um","140-250HV"]
["X000471030MI00000",4.5,"DIN471","M32","65锰",null,"机械镀锌48/96/5","470-580HV"]
["X0095050772000BA0",4.4000000000000004,"950-50772-000","10.5*25*3","不锈钢304",null,"不锈钢304","西门子"]
["G009387020MK00000",4.4000000000000004,"GB93-87","M20","65锰",null,"三价锌5um","42-50HRC"]
["G009785030AB200HV",4.4000000000000004,"GB97-85","M30","碳钢",null,"镀锌","200-300HV"]
["F022030001BA00000",4.4000000000000004,"22*30*1","22*30*1","不锈钢304",null,"不锈钢304","内销柏中"]
["DIN6796020MR00000",4.37,"DIN6796","M20","50CrV4",null,"环保达克罗500无红","420-490HV"]
["F033157696004KA00",4.3650000000000002,"WA-0034-00(REV2)","WA-0034-00(REV2)","H70铜","NULL","H70铜","NULL"]
["G009785033AB00000",4.3,"GB97-85","M33","碳钢",null,"镀锌"]
["A300004087",4.3,300004087,"M10 非标单耳折弯","不锈钢304","NULL","本色"]
["F012X698X25BA0000",4.2770000000000001,"13106-04434","12*69.8*2.5","不锈钢304",null,"不锈钢304"]
["G009387022IG00000",4.25,"GB93-87","M22","65锰",null,"达克罗500无红","42-50HRC"]
["D00127B024II00000",4.24,"DIN127B","M24","弹簧钢",null,"机械镀锌"]
["D009021016AKHV140",4.2,"DIN9021","M16","碳钢",null,"三价锌","140-250HV"]
["A200001648",4.2,200001648,"NFE25-511M M16","65Mn",null,"达克罗","420-510HV"]
["ISO7089024GA300HV",4.2,"ISO7089","M24","45#钢",null,"热处理本色","300-370HV"]
["XXT0000201",4.2,"10.5*25*2.5","10.5*25*2.5","Q235B","NULL","三价锌","NULL"]
["DIN7349020GA300HV",4.0599999999999996,"DIN7349","M20","65锰","NULL","本色","300HV"]
["DIN7349M12AN200HV",4,"DIN7349","M12","材质不指定",null,"灰色锌镍240/1000","200HV"]
["F010X20X25GG00000",4,"C04243TD81440R16","10*20*2.5","45#钢",null,"Gemet321A(300-350HV)","常州君合镀锌厂"]
["A200001579",4,200001579,"DIN6796 M14","65Mn",null,"达克罗12UM96/500","420-490HV"]
["D00125A018AKHV140",4,"DIN125A","M18","碳钢",null,"三价锌","140-250HV"]
["DIN125AM10AN008UM",4,"DIN125A","M10","碳钢",null,"彩色锌镍168/720/8","140-250HV"]
["D006796016GE012UM",4,"DIN6796","M16","50CrV4","NULL","环保机械黄锌72/144/12","420-490HV"]
["XXT0000009",4,"DIN9021","M4","Q235","NULL","环保达克罗720无红","202-227HV"]
["X007989012BA140HV",4,"DIN7989","M12","不锈钢304",null,"不锈钢304","西门子"]
["NFE25$513012AG0LL",4,"NFE25-513LL","M12","碳钢",null,"达克罗","100HV"]
["X000000M8MG2551H",4,"NFE25-511M","M8","65锰",null,"达克罗500无红","锥形压花垫"]
["GB96200210AK200HV",4,"GB96.1-2002","M10","碳钢","NULL","三价锌","200-300HV"]
["F105X22X3AK000000",4,"BN90700  6305314","SWT671 10.5*22*3","Q235",null,"三价锌12/36/5"]
["D000472045MD00000",3.9980000000000002,"DIN472","M45","65锰",null,"发黑"]
["D00128A020MN00000",3.992,"DIN128A","M20","弹簧钢",null,"黑磷化","44-51HRC"]
["F002677PW114400H1",3.99,"PW1144-1","20.6*38*6","45#钢",null,"热处理本色","HRC36-42"]
["ISO7089M36AD300HV",3.99,"ISO7089","M36","45#钢","NULL","发黑上油","300-370HV"]
["F003070PW13390011",3.92,"PW1339-1","34.8*45*3.04","Q235",null,"本色"]
["D009021003ALHV140",3.9,"DIN9021","M3","碳钢",null,"三价彩锌","140-250HV"]
["XXT0000043",3.9,"DIN7349","M12","50CrV4","NULL","达克罗","300HV"]
["ISO7089020GR300HV",3.9,"ISO7089","M20","45#钢",null,"上海环保达克罗500无红","300-370HV"]
["G08482002024AB000",3.9,"GB848-2002","M24","碳钢","NULL","镀锌","200-300HV"]
["G009387030IF00000",3.8,"GB93-87","M30","65锰",null,"热锌","42-50HRC"]
["ISO7089M14AF200HV",3.8,"ISO7089","M14","碳钢","NULL","热锌","200-300HV"]
["F017X40X5AK000000",3.8,"BN90700  6305323","SWT671 17*40*5","Q235",null,"三价锌12/36/5"]
["DIN6796024GG012UM",3.79,"DIN6796","M24","50CRV4","NULL","达克罗三涂三烘+封闭96/500/12","420-490HV"]
["D000434016AF00000",3.75,"DIN434","M16","A3普碳钢",null,"热锌"]
["G009685020ABHV200",3.75,"GB96-85","M20","碳钢",null,"镀锌","200-300HV"]
["F017X25X075AK0000",3.7,"BN90700  6305319","SWT671 17*25*0.75","Q235",null,"三价锌12/36/5"]
["F09X024X002BA0000",3.61,"C1B427-04322-002","9*24*2","不锈钢304",null,"不锈钢304"]
["G009785027AB00000",3.6,"GB97-85","M27","碳钢",null,"镀锌"]
["GB09585020AF00000",3.6,"GB95-85","M20","碳钢","NULL","热锌","200HV"]
["ISO7093M12GG300HV",3.6,"ISO7093","M12","45#钢","NULL","达克罗500无红","300-370HV"]
["F0000000000A58549",3.58,"A58549","25*44*4.76","45#钢",null,"机械镀锌48/96","35-45HRC"]
["F0105X40X2AK00000",3.5,"DIN522","10.5*40*2","碳钢","NULL","三价锌48/72/5","140-250HV"]
["F0063X016X002JA00",3.5,"BN91230 6134743","6.3*16*2","紫铜",null,"紫铜"]
["ISO7092M05AAHV200",3.5,"ISO7092","M5","碳钢",null,"三价锌12/36/5","200-300HV"]
["XXT0000297",3.5,"DIN9021","M10","Q235","NULL","Geomet（R）0/500","200-300HV"]
["F0687X0859X0031BA",3.5,"BN91170 6340963","0.687*0.859*0.031","不锈钢304","NULL","不锈钢304","NULL"]
["F034X14X2GL000000",3.5,"BN90701 6307236","3.4*14*2","45#钢","NULL","三价彩锌16/72/5","HRC30-36"]
["F21X40X2AK0000000",3.5,"非标平垫","21*40*2","碳钢","NULL","三价锌48/72/5","公差按NFE25-513"]
["X000433016BA200HV",3.49,"DIN433","M16","不锈钢304",null,"不锈钢304","200HV"]
["F099X3962X229AK00",3.4,"13105-04858","9.9*39.62*2.29","碳钢","NULL","三价锌","NULL"]
["G085688M16AG00000",3.4,"GB856 ","M16*2","低碳钢","NULL","达克罗","NULL"]
["G009685016AB00000",3.4,"GB96-85","M16","碳钢",null,"镀锌"]
["F0053X012X002JA00",3.4,"BN91230  6134742","5.3*12*2","紫铜",null,"紫铜"]
["A000000008BA0000B",3.4,"美制平垫B型","8# B型","不锈钢304",null,"不锈钢304"]
["A300004795",3.4,300004795,"15*16.95","A3普碳钢","NULL","本色"]
["DIN126M010GI300HV",3.4,"DIN126","M10","45#钢","NULL","机械镀锌","300HV"]
["DIN125AM16AH200HV",3.4,"DIN125A","M16","碳钢","NULL","黑磷化","200-250HV"]
["F0000000AK24H1655",3.34,"24H1655","0.688*1.75*0.105","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["F21X31X4GG0000000",3.3,"BN90701   6266854","21*31*4","45#钢",null,"环保达克罗500无红","280-330HB"]
["ISO7093M16AR300HV",3.3,"ISO7093","M16","45#钢",null,"上海环保达克罗500无红","300-370HV"]
["F00000000000R99437",3.24,"R99437","R99437","45#钢",null,"机械镀锌48/96/8","35-45HRC"]
["F02677PW113200H10",3.206,"PW1132-H-1","19*60*9","45#钢","NULL","热处理本色","HRC36-42"]
["F0083X026X002AK00",3.2,"BN90700   6192429","8.3*26*2","碳钢","NULL","三价锌","NULL"]
["D006340012GD00000",3.2,"DIN6340","M12","45#钢","NULL","发黑","350-430HV"]
["D00125AM12ADHV300",3.2,"DIN125A","M12","45#钢",null,"发黑","300-370HV"]
["XXT0000051",3.2,"DIN9021","M10","Q235","NULL","三价彩锌150无红8um","200-300HV"]
["XXT0000237",3.2,"DIN125A","M12","Q235","NULL","三价锌3um","200HV"]
["F03493X603X3GK000",3.2,"'03040317","1-1/4(34.93*60.3*3)","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["F0391X571X15QK000",3.2,"13105-06104","39.1*57.1*1.5","Q235","NULL","三价彩锌96/120/5上封闭","NULL"]
["F03$8X13$16GC0000",3.2,"'11101304","3/8*13/16","45#钢","NULL","三价黄锌5um","HRC38-45"]
["GB962002M10AH0000",3.2,"GB96.1-2002","M10","碳钢","NULL","灰色锌镍96/150","200-300HV"]
["F508X873X3GK00000",3.12,"'03040217","1-7/8（50.8*87.3*3）","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["F053X025X015BA000",3.1,"BN10342 3061818","5.3*25*1.5","不锈钢304","NULL","不锈钢304","NULL"]
["GB97285M24AD200HV",3.1,"GB97.2-85","M24","碳钢",null,"发黑","200-300HV"]
["D000440012AAHV140",3.1,"DIN440","M12","碳钢",null,"黄锌5um"]
["DIN9021M10AKHV200",3.1,"DIN9021","M12","碳钢",null,"三价锌48/72/5","200-250HV"]
["G085388016AR00000",3.0750000000000002,"GB853-88","M16","碳钢",null,"环保达克罗500无红"]
["F011X24X4BA000000",3.0449999999999999,"C1B427-04322-006","11*24*4","不锈钢304",null,"不锈钢304"]
["GB96850M12AM300HV",3.024,"GB96-85","M12","碳钢","NULL","三价锌72/144/5","300-370HV"]
["F03051PW117300@B2",3.01,"PW1173-2","20.88*47.24*5.68","45#钢",null,"三价锌72/96/5","HRC38-45"]
["F089X032X024BA000",3,"BN91170 6143933","8.9*32*2.4","不锈钢304","NULL","不锈钢304","内销柏中"]
["F1905X3332X003AK00",3,"'03040002","5/8(19.05*33.32*3)","A3普碳钢",null,"三价锌5um","利拓"]
["GB97200212GA00000",3,"GB97.1-2002","M12","45#钢","NULL","不热处理本色","NULL"]
["G009685020AB00000",3,"GB96-85","M20","碳钢",null,"镀锌"]
["ISO7093M12AN200HV",3,"ISO7093","M12","碳钢",null,"Geomet321 VL 1000无红0.09-0.14摩擦","200-300HV"]
["ISO7093M08CA200HV",3,"ISO7093","M8","不锈钢316","NULL","不锈钢316","200-300HV"]
["ISO7089M08AL200HV",3,"ISO7089","M8","碳钢",null,"三价彩锌150无红，上封闭","200-300HV"]
["F013X35X4AK000000",3,"BN90700  6305318","SWT671 13*35*4","Q235",null,"三价锌12/36/5"]
["D000433M16AKHV200",3,"DIN433","M16","碳钢",null,"三价锌","200-300HV"]
["D00125A010AAHV200",3,"DIN125A","M10","碳钢",null,"本色","200-250HV"]
["D007349020AD00000",3,"DIN7349","M20","碳钢","NULL","发黑","NULL"]
["DIN125A005AK140HV",3,"DIN125A","M5","碳钢",null,"三价锌96无白5um","140-250HV"]
["F025X38X02BA00000",2.95,"BN91118   6288974","25*38*0.2","不锈钢304",null,"不锈钢304"]
["F013X25X3AK000000",2.9,"BN90700  6305317","SWT671 13*25*3","Q235",null,"三价锌12/36/5"]
["F064X20X16AK200HV",2.9,"BN90701   6288555","6.4*20*1.6","Q235",null,"三价彩锌48/96/5","200HV"]
["GB9387M16MN000000",2.8,"GB93-87","M16","65锰","NULL","灰色锌镍720无红8um","42-50HRC"]
["ISO7090M10AR140HV",2.8,"ISO7090","M10","碳钢",null,"Geomet321+VL,500无红","140-250HV"]
["DIN125AM20AR200HV",2.8,"DIN125A","M20","碳钢","NULL","上海环保达克罗1000无红","200-250HV"]
["DIN125AM27AK140HV",2.7,"DIN125A","M27","碳钢","NULL","三价锌48/72/5","140-250HV"]
["D006796016BA00000",2.7,"DIN6796","M16","不锈钢304",null,"不锈钢304"]
["F635X1905X12BA000",2.7,"BN91170   6166821","6.35*19.05*1.2","不锈钢304",null,"不锈钢304"]
["X000432008BA200HV",2.69,"DIN432","M8","不锈钢304",null,"不锈钢304","200HV"]
["A200004171",2.69,200004171,"DIN988 22*30*2","A3普碳钢","NULL","发黑"]
["F0232X05X0094BA00",2.68,"BN91170 6348599","0.232*0.5*0.094","不锈钢304","NULL","不锈钢304","NULL"]
["D00125A024AKHV140",2.6,"DIN125A","M24","碳钢",null,"三价锌","140-250HV"]
["NFE25518ZAG000000",2.6,"NFE25-518Z","M14","45#钢","NULL","环保达克罗1000无红","310HV"]
["XXT0000305",2.6,"DIN9021","M6","Q235","NULL","三价锌72/144/12","200-300HV "]
["XXT0000276",2.5499999999999998,"ISO7093","M16","Q235","NULL","三价彩锌72/216/8um","200-300HV"]
["GB962002016AI0000",2.5499999999999998,"GB96.1-2002","M16","碳钢","NULL","机械镀锌96/144/12","200-300HV"]
["F00277X338X0031BA",2.5499999999999998,"BN91170 6130479","2.77*3.38*0.031","不锈钢304",null,"不锈钢304","200HV"]
["F011X24X1BA000000",2.5,"C1B427-04322-003","11*24*0.5","不锈钢304",null,"不锈钢304"]
["D007349016AA200HV",2.5,"DIN7349","M16","50CrV4",null,"本色","200HV"]
["D007349024AA00000",2.5,"DIN7349","M24","碳钢","NULL","本色","100HV"]
["XXT0000319",2.5,"DIN125A","M20","Q235","NULL","Geomet321VL0/1000 摩0.09-0.14","200HV"]
["DIN2093A50X254X30",2.48,"DIN2093A","50*25.4*3","50CrV4",null,"黑磷化"]
["D006340012GA00000",2.46,"DIN6340","M20","45#钢","NULL","热处理本色","350-430HV"]
["XXT0000272",2.4300000000000002,"DIN126","M27","Q235","NULL","三价锌3um","100HV"]
["D007349016AD00000",2.4,"DIN7349","M16","碳钢","NULL","发黑","NULL"]
["F003051PW115000H2",2.4,"PW1150-2","17*37*5","45#钢",null,"热处理本色","300-370HV"]
["DIN125B030AKHV140",2.39,"DIN125B","M30","碳钢",null,"三价锌5um","140-250HV"]
["F0381X6985X03GA00",2.38,"'03040276","1-3/8(38.1*65.9*3)","50#钢","NULL","热处理本色(振动去毛刺）","HRC38-45"]
["F002677PW11390011",2.34,"PW1139-P-1","28*49*6","45#钢",null,"不热处理本色"]
["F05398X937X3GA000",2.3130000000000002,"'03040281","2(53.98*93.7*3)","50#钢","NULL","热处理本色(振动去毛刺）","HRC38-45"]
["F105X014X075AK000",2.2999999999999998,"BN90700 6305312","SWT671 10.5*14*0.75","碳钢","NULL","三价锌48/72/5","NULL"]
["F0DM20251001ACBA0",2.2999999999999998,"DM-20251-001-AC","M42双孔轴端挡圈","不锈钢304",null,"不锈钢304"]
["XXT0000322",2.2999999999999998,"GB97-85","M36","50CrV4","NULL","环保达克罗0/720，摩0.15-0.21","300HV"]
["ISO7090M10AN200HV",2.2999999999999998,"ISO7090","M10","碳钢","NULL","灰色锌镍500无红","200-300HV"]
["ISO7093M20GR300HV",2.2999999999999998,"ISO7093","M20","45#钢",null,"上海环保达克罗500无红","300-370HV"]
["ISO7093M12GN300HV",2.2999999999999998,"ISO7093","M12","45#钢",null,"黑磷化","300-370HV"]
["F02647X4496X025AD",2.2799999999999998,"11724-05162","26.47*44.96*2.5","A3普碳钢",null,"发黑140HV","快扣"]
["F003046PM16470011",2.2400000000000002,"PM1647-2(长方板）","0.12*3.75*6.5A569","低碳钢","NULL","本色","NULL"]
["DIN7989M30MG00000",2.2200000000000002,"DIN7989-2","M30","65锰","NULL","达克罗500无红","300-370HV"]
["ISO7089M36AK200HV",2.2200000000000002,"ISO7089","M36","碳钢",null,"三价锌6/24/3","200-300HV"]
["F000000000WA00290",2.2120000000000002,"WA-0029-00(REV2)","WA-0029-00","H70铜",null,"铜"]
["F003041PW1094001S",2.21,"PW1094-1","32.5*45*1","黄铜","NULL","黄铜","NULL"]
["F02WT440672AK0000",2.21,"2WT440672","1.38*2.256*0.0945","Q235A",null,"三价黄锌(518Y)5um","盛派"]
["F0125X035X015CA00",2.2000000000000002,"BN91170   6169204","12.5*35*1.5","不锈钢316",null,"不锈钢316","200HV"]
["DIN6796016MR01000",2.2000000000000002,"DIN6796","M16","50CrV4","NULL","环保达克罗1000无红","420-490HV"]
["F0000000AK24H1401",2.2000000000000002,"24H1401","0.781*1.75*0.194","Q235",null,"三价锌TNTUV12/144/5","<302HV"]
["DIN125AM20AN200HV",2.2000000000000002,"DIN125A","M20","碳钢",null,"黑磷化","200-250HV"]
["D009021004CA200HV",2.2000000000000002,"DIN9021","M4","不锈钢316",null,"不锈钢316","200HV"]
["F0021X44X8GR200HV",2.19,"BN90701 6188960","21*44*8","45#钢","NULL","Geomet  321B","200HV"]
["F0005398X937X3AK0",2.19,"'03040218","2(53.98*93.7*3)","Q235","NULL","三价锌72/120/8","NULL"]
["F003$4B$WBA000000",2.17,11641777,"美制平垫3/4B型 W","不锈钢304","NULL","不锈钢304","NULL"]
["G085688030AD00000",2.14,"GB856-88","M30","Q235B","NULL","发黑","NULL"]
["XXT0000229",2.13,"DIN125A","M30","Q235","NULL","环保达克罗0/720","200-250HV"]
["F032065010AF00000",2.1150000000000002,"32*65*10","32*65*10","碳钢","NULL","热锌 140HV","NULL"]
["XXT0000315",2.1,"DIN7349","M8","Q235","NULL","三价彩锌8um","200-300HV"]
["F22X42X4GC0000000",2.0449999999999999,"12601-02346","M20(22*42*4)","45#钢",null,"黄锌","HRC38-45"]
["ISO7093M22GR200HV",2.04,"ISO7093","M22","碳钢","NULL","环保达克罗720无红","200-300HV"]
["D007349020AF200HV",2.04,"DIN7349","M20","碳钢","NULL","热锌","200HV"]
["F20456426378BA000",2.0299999999999998,"WA-0014-00(REV1)","WA-0014-00","不锈钢304","NULL","不锈钢304","NULL"]
["ISO7089M24AK005UM",2.02,"ISO7089","M24","碳钢",null,"三价彩锌48/72/5","200-300HV"]
["F0010X50X3AK140HV",2.02,"10*50*3","10*50*3","Q235",null,"三价锌","140HV"]
["F0050X108X1AA0000",2.0099999999999998,"BN91550  6167633","50*108*1","碳钢","NULL","本色","NULL"]
["F0105X25X25AK0000",2,"DIN522C","10.5*25*2.5","碳钢","NULL","三价锌48/72/5","NULL"]
["F018X55X2AK000000",2,"C1B427-09079-003","18*55*2（多孔垫）","Q235","NULL","三价锌5um","NULL"]
["F017X38X4AK000000",2,"BN90700  6305322","SWT671 17*38*4","Q235",null,"三价锌12/36/5"]
["DIN7349M08AR140HV",2,"DIN7349","M8","碳钢","NULL","上海环保达克罗1000无红，0.15-0.21摩擦","140HV"]
["DIN7349M04AJ200HV",2,"DIN7349","M4","碳钢","NULL","机械镀锌","200-300HV"]
["F0000000006104670",2,"3/4非标平垫","19.53*35.05*1.6","Q235",null,"上海环保达克罗600无红"]
["D006340008GK00000",2,"DIN6340","M8","45#钢","NULL","三价锌","350-430HV"]
["D00127B024CA00000",2,"DIN127B","M24","不锈钢316",null,"不锈钢316"]
["D00127B018CA00000",2,"DIN127B","M18","不锈钢316",null,"不锈钢316"]
["D00127B020BA00000",2,"DIN127B","M20","不锈钢304",null,"不锈钢304"]
["D100433006AKHV200",2,"DIN433","M6","碳钢",null,"三价锌72无红5um","200-300HV"]
["D000433010AAHV200",2,"DIN433","M10","碳钢",null,"本色","200-300HV"]
["A0000001$2AA00000",2,"美制标型准弹垫","'1/2","65锰",null,"本色"]
["A000003$8NAR00000",2,"美制N型","3/8N","碳钢","NULL","上海环保达克罗600无红","NULL"]
["ISO7089M14AKHV200",2,"ISO7089","M14","碳钢",null,"三价锌48/72/5","200-300HV"]
["ISO7094M12BA100HV",2,"ISO7094","M12","不锈钢304","NULL","不锈钢304","100HV"]
["ISO7093M12AR200HV",2,"ISO7093","M12","碳钢",null,"环保达克罗 720无红","200-300HV"]
["ISO7090M20AR200HV",2,"ISO7090","M20","碳钢","NULL","环保达克罗720无红","200-300HV"]
["X0047134X15MD0000",2,"C1B810-42201-899","DIN471 34*1.5","65锰","NULL","磷化（停用）","NULL"]
["XXT0000232",2,"NFE25-514M","M10","Q235","NULL","六价彩锌12um","NULL"]
["XXT0000209",2,"13*36*3","13*36*3","Q235","NULL","热锌","140HV"]
["XXT0000193",2,"4.3*14*0.8","4.3*14*0.8","Q235","NULL","三价锌24/0","140HV"]
["G089486080MN00000",2,"GB894.1","M80*2.5","65锰","NULL","黑磷化上WD40油","NULL"]
["D000472055AG00000",1.98,"DIN472","M55*2","65锰","NULL","达克罗500无红","NULL"]
["DIN128A024MI00000",1.98,"DIN128A","M24","弹簧钢",null,"机械镀锌72/120/8","44-51HRC"]
["F04128X714X0030GK",1.92,"'03040319","1-1/2(41.28*71.4*3)","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["XXT0000032",1.9,"DIN9021","M6","不锈钢304","NULL","钝化本色","200HV"]
["DIN127B020IR00500",1.9,"DIN127B","M20","弹簧钢",null,"环保达克罗","500无红"]
["D00128A020MR00000",1.9,"DIN128A","M20","弹簧钢",null,"上海环保达克罗500无红","44-51HRC"]
["D000126024BAHV200",1.9,"DIN126","M24","不锈钢304",null,"不锈钢304","200HV"]
["F0105X24X2AKHV150",1.9,"12833-00551","10.5*24*2","碳钢","NULL","三价锌72无白8um","150-250HV"]
["ISO7093M20AF200HV",1.86,"ISO7093","M20","碳钢",null,"热锌","200-300HV"]
["ISO7093M10GN300HV",1.85,"ISO7093","M10","45#钢","NULL","灰色锌镍500无红","300-370HV"]
["F0BN91170$4058257",1.85,"BN91170/4058257","0.453*1.062*0.031","不锈钢304","NULL","不锈钢304 钝化","NULL"]
["X000434012AF00000",1.8,"DIN434","M12","碳钢","NULL","热锌","西门子"]
["F002677PW14450011",1.8,"PW1445-1","13.1*23.51*2.44","黄铜","NULL","H62铜（清洗）","NULL"]
["DIN7349010AKHV140",1.8,"DIN7349","M10","碳钢","NULL","环保达克罗 720无红，0.15-0.21摩擦","140HV"]
["A00005$16WAK00000",1.8,"美制W型","5/16W","碳钢","NULL","三价锌100无红5um","NULL"]
["F004445X778X003GK",1.7889999999999999,"'03040320","1-5/8(44.45*77.8*3)","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["XXT0000019",1.77,"DIN6340","M12","Q235","NULL","机械镀锌48/96/8","NULL"]
["GB09785024GGHV300",1.75,"GB97-85","M24","45#钢",null,"达克罗1000无红","300-370HV"]
["D00125B024GR200HV",1.75,"ISO7090","M24","45#钢","NULL","Geomet 321A+VL","300-370HV"]
["XXT0000214",1.71,"7.2*22*32*0.5","7.2*22*32*0.5","Q235","NULL","镀锌","NULL"]
["XXT0000031",1.7,"DIN7349","M12","50CrV4","NULL","环保达克罗720无红0.14-0.21摩擦","140HV"]
["ISO7092M20AF200HV",1.7,"ISO7092","M20","碳钢","NULL","热锌","200-300HV"]
["D007349012AKHV200",1.7,"DIN7349","M12","碳钢","NULL","达克罗","200HV"]
["D007349012AKHV300",1.7,"DIN7349","M12","45#钢","NULL","达克罗500无红","350-400HV"]
["F00PWHM8$1CGA0000",1.7,"PWH M8-1C","7.4*20*2.3","S50C","NULL","热处理本色","HRC38-46"]
["DIN6796M24NA00000",1.6779999999999999,"DIN6796","M24","50CrV4","NULL","热处理本色","420-470HV"]
["F0017X38X4AK200HV",1.67,"DIN522A","17*38*4","碳钢","NULL","热锌","200-250HV"]
["D00137B042MG00000",1.65,"DIN137B","M42","65锰","NULL","环保达克罗720无红","NULL"]
["X95052191000KA160",1.65,"950-52191-000","30.5*55*1.5","黄铜",null,"黄铜 160HV","西门子"]
["ISO7089M24AR72000",1.6,"ISO7089","M24","碳钢","NULL","环保达克罗720无红","200-300HV"]
["GB97200216GA00000",1.6,"GB97.1-2002","M16","45#钢","NULL","不热处理本色","NULL"]
["G009785030AB300HV",1.6,"GB97-85","M30","45#钢",null,"镀锌","300-370HV"]
["A300003861",1.6,300003861,"3/8-16245A2902P8","碳钢",null,"蓝白锌3-5um","140-250HV"]
["D006340020GG00000",1.59,"DIN6340","M20","45#钢","NULL","达克罗","350-430HV"]
["DIN6796020MR00720",1.59,"DIN6796","M20","50CRV4","NULL","环保达克罗720无红","420-490HV"]
["F00105X38X25200HV",1.55,"DIN522A","10.5*38*2.5","碳钢","NULL","三价彩锌72/120/8","200-250HV"]
["F003046PM16490011",1.548,"PM1649-2(长方板）","0.06*3.5*5.25A569","低碳钢","NULL","本色","NULL"]
["G009785036AB00000",1.52,"GB97-85","M36","碳钢",null,"镀锌"]
["G009685016ABHV140",1.5,"GB96-85","M16","碳钢",null,"镀锌","140-250HV"]
["G009685016AC200HV",1.5,"GB96-85","M16","碳钢",null,"黄锌","200-300HV"]
["ISO7089020AN200HV",1.5,"ISO7089","M20","碳钢",null,"黑磷化","200-300HV"]
["FISO7093CL10200HV",1.5,"ISO7093","M10","碳钢",null,"三价黄锌150无红","200-300HV"]
["ISO7089M36GG300HV",1.5,"ISO7089","M36","45#钢",null,"环保达克罗720无红0.15-0.21摩擦","300-370HV"]
["XXT0000073",1.5,"DIN125A","M12","Q235","NULL","发黑","200HV"]
["XXT0000070",1.5,"DIN988","50*62*2","Q235","NULL","本色","NULL"]
["XXT0000062",1.5,"GB97-85","M27","Q235","NULL","热锌","200HV"]
["F010X18X25GR00000",1.5,"BN90701   6230620","10*18*2.5","碳钢","NULL","GEOMET321A","160HV"]
["F021X30X3AK000000",1.5,"BN90700  6305325","SWT671 21*30*3","Q235",null,"三价锌12/36/5"]
["F0165X83X4AK00000",1.48,"LG0050DTGAIII.01.05.02-001","16.5*83*4","Q235B","NULL","三价锌72/144/5","NULL"]
["F003070PW13090211",1.43,"PW1309-1","0.406*1.5*0.12","Q235",null,"本色"]
["DIN7349020AKHV200",1.4,"DIN7349","M20","45#钢",null,"三价锌","200HV"]
["A200004128",1.4,200004128,"GB853-88 M16","碳钢",null,"蓝白锌"]
["XXT0000306",1.4,"DIN435","M16","Q235","NULL","三价锌12um","NULL"]
["ISO7089M30GR300HV",1.4,"ISO7089","M30","45#钢",null,"环保达克罗720无红,0.15-0.21摩擦","300-370HV"]
["F064X20X4AK000000",1.4,"BN90700  6305117","SWT671 6.4*20*4","Q235",null,"三价锌12/36/5"]
["GB85688036AG00000",1.4,"GB856","M36*2.5","低碳钢","NULL","达克罗","NULL"]
["G009685M12ARHV100",1.4,"GB96.2-2002","M12","碳钢","NULL","达克罗720无红","100HV"]
["F065X22X2BA000000",1.35,"C1B4L96-00088-001","6.5*22*2","不锈钢304","NULL","不锈钢304","NULL"]
["F056072002AA00000",1.35,"DIN988","56*72*2","碳钢","NULL","本色","NULL"]
["ISO7093M16AR200HV",1.35,"ISO7093","M16","碳钢",null,"环保达克罗720无红摩擦0.15-0.21","200-300HV"]
["D000126016GR300HV",1.35,"DIN126","M16","45#钢","NULL","上海环保达克罗","300HV"]
["ISO7094M24AD00000",1.32,"ISO7094","M24","碳钢","NULL","发黑","140HV"]
["F0395X52X2CA00000",1.32,"BN91170 6174562","39.5*52*2","不锈钢316",null,"不锈钢316"]
["F003046PM16480011",1.3029999999999999,"PM1648-2(钢板）","0.06*7.18*8.93GALV","低碳钢","NULL","本色","NULL"]
["F003070PW13070011",1.3,"PW1307-1","10.2*35*3","Q235",null,"本色"]
["DIN125A008AN200HV",1.3,"DIN125A","M8","碳钢",null,"环保锌镍","200-250HV"]
["F074X24X28MA00000",1.3,"198-26DQ","7.4*24*2.8","65锰","NULL","热处理本色上油","360-430HV"]
["G0009387020IG0000",1.3,"GB93-87","M20","65锰",null,"达克罗500无红","42-50HRC"]
["XXT0000302",1.3,"DIN9021","M12","45#","NULL","黄锌8um","300HV"]
["XXT0000053",1.3,"DIN7349","M16","50CrV4","NULL","黄锌","140HV"]
["XXT0000145",1.3,"DIN7349","M20","Q235","NULL","发黑","200HV"]
["F021X45X2AK000000",1.29,"BN90700  6305326","SWT671 21*45*2","Q235",null,"三价锌12/36/5"]
["D007349006CA200HV",1.27,"DIN7349","M6","不锈钢316",null,"不锈钢316","200HV"]
["F0455X14X12AA0000",1.27,"Q190514012","4.55*14*1.2","20#","NULL","本色","NULL"]
["ISO7094M16GN300HV",1.26,"ISO7094","M16","45#钢",null,"黑磷化","300HV"]
["F436034X55X6GA000",1.25,"11724-04113","F436  34*55*6","45#钢",null,"本色","HRC38-45"]
["F01872X1225X1$8GD",1.22,"13106-02169","1.872*1.225*1/8","45#钢",null,"发黑","300HV"]
["F022X70X70X7AK000",1.21,"BN752  1274384","M20(22*70*70*7)","Q235",null,"三价锌","100HV"]
["GB97200218GA00000",1.2,"GB97.1-2002","M18","45#钢","NULL","不热处理本色","NULL"]
["ISO7091M30AF200HV",1.2,"ISO7091","M30","Q235",null,"热锌","200HV"]
["ISO7089M36GR300HV",1.2,"ISO7089","M36","45#钢","NULL","环保达克罗720无红，0.15-0.21摩擦","200-300HV"]
["X0095049861000",1.2,"C1B950-49861-000","38*51.5*2","碳钢","NULL","黄锌","西门子"]
["XXT0000071",1.2,"DIN9021","M6","Q235","NULL","锌镍合金","200HV"]
["XXT0000278",1.2,"6.3*16*2","6.3*16*2","T2","NULL","本色","NULL"]
["G009585030AA300HV",1.1499999999999999,"GB95-85","M30","45#钢","NULL","发黑","300HV"]
["F4763X826X3GK0000",1.145,"'03040321","1-3/4(47.63*82.6*3)","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["F0547X125X018BA00",1.1399999999999999,"'1/2-13","0.547*1.25*0.18","不锈钢304","NULL","不锈钢304 不导磁","NULL"]
["XXT0000195",1.1000000000000001," 0.203*0.438*0.06"," 0.203*0.438*0.06","不锈钢304","NULL","A2","200HV"]
["F0034X115X1BA0000",1.1000000000000001,"BN91170  6353274","DIN522A 3.4*11.5*1","不锈钢304","NULL","不锈钢304","NULL"]
["DIN7349020GR300HV",1.1000000000000001,"DIN7349","M20","45#钢","NULL","环保达克罗720无红","300HV"]
["D009021016BAHV200",1.1000000000000001,"DIN9021","M16","不锈钢304",null,"不锈钢304","200HV"]
["F05398X937X3GK000",1.093,"'03040323","2(53.98*93.7*3)","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["F6668X1159X3GK000",1.085,"'03040325","2-1/2(66.68*115.9*3)","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["ISO7089M36GK00000",1.08,"ISO7089","M36","45#钢","NULL","三价锌","300-370HV"]
["XXT0000026",1.06,"DIN9021","M16","Q235","NULL","上海环保达克罗500无红","NULL"]
["F0344X075X005AL00",1.05,"BN90701 6344384","0.344*0.75*0.05","碳钢","NULL","三价彩锌96无白","100HV"]
["DIN6796M16HA00000",1.05,"DIN6796","M16","50CrV4","NULL","热处理本色","420-490HV"]
["G085888048AG00720",1.0469999999999999,"GB858-88","M48","低碳钢","NULL","达克罗720无红","NULL"]
["G009785036ACHV300",1.04,"GB97-85","M36","45#钢",null,"黄锌","300-370HV"]
["D007349020BAHV200",1.04,"DIN7349","M20","不锈钢304",null,"不锈钢304","200HV"]
["F09208X1604X3AK00",1.0269999999999999,"'03040224","3-1/2(92.08*160.4*3)","Q235","NULL","三价锌72/120/8","NULL"]
["F06033X4048X3GK00",1.026,"'03040324","2-1/4(60.33*104.8*3)","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["G085888055AK00000",1.0249999999999999,"GB858","M55","低碳钢","NULL","三价锌72/144/5","NULL"]
["F003046PM19160011",1.0069999999999999,"PM1916-1","3.75*6.5*0.0598(簙钢板）","Q235","NULL","本色","NULL"]
["F0021X30X3GC200HV",1,"BN90701/6348869","21*30*3","35#钢","NULL","黄锌72/144/12","200-300HV"]
["F016022005BA00000",1,"DIN988","16*22*0.5","不锈钢304","NULL","不锈钢304","NULL"]
["F0105X38X25AK0000",1,"BN90700  6305315","SWT671 10.5*38*2.5","Q235",null,"三价锌12/36/5"]
["F00L401P26MI00000",1,"BN90704   6267614","L401P26（弹垫）","70#钢","NULL","机械镀锌","372-458HV"]
["DIN6916M16GI00000",1,"DIN6916","M16","45#钢","NULL","机械镀锌","295-350HV"]
["D006796020NG10000",1,"DIN6796","M20","50CrV4","NULL","Geomet 321A 1000无红","420-490HV"]
["D00128A024MJ00000",1,"DIN128A","M24","弹簧钢",null,"发黑","44-51HRC"]
["D10125A024AGHV200",1,"DIN125A","M24","碳钢",null,"达克罗1000无红","200-250HV"]
["DIN1441X25X38X400",1,"DIN1441","25*38*4","不锈钢304","NULL","不锈钢304","NULL"]
["D00125A016BH00000",1,"DIN125A","M16","不锈钢304","NULL","不锈钢304（钝化）","NULL"]
["D00125A014AKHV200",1,"DIN125A","M14","碳钢",null,"三价锌","200-250HV"]
["F063X172X2AK140HV",1,"BN90701 6348290","6.3*17.2*2","碳钢","NULL","三价锌","140-250HV"]
["F105X040X015AK000",1,"BN90700 6305316","SWT671 10.5*40*1.5","碳钢","NULL","三价锌48/72/5","NULL"]
["G0085688016AK0000",1,"GB856","M16*1","低碳钢",null,"三价黄锌48/72/5"]
["ISO7089M24GF300HV",1,"ISO7089","M24","45#钢","NULL","热锌","300-370HV"]
["ISO7089M20AN200HV",1,"ISO7089","M20","碳钢",null,"Geomet 321VL1000无红0.09-0.14摩擦","200-300HV"]
["ISO7089M14AR200HV",1,"ISO7089","M14","碳钢",null,"环保达克罗500无红","200-300HV"]
["ISO7089M18AF200HV",1,"ISO7089","M18","碳钢","NULL","热锌","200-300HV"]
["ISO7093020AG200HV",1,"ISO7093","M20","碳钢",null,"环保达克罗720无红","200-300HV"]
["ISO7093M12AG00000",1,"ISO7093","M12","碳钢","NULL","环保达克罗1000无红","200-300HV"]
["NFE25511L10BA0000",1,"NFE25-513L","M10","不锈钢304","NULL","不锈钢304","NULL"]
["X0095051922000MG0",0.999,"DIN472","M110*4","65锰",null,"达克罗","西门子"]
["F01$4X1X125AJ0000",0.997,"BN90803 6176919","1/4*1.125（代加工）","NULL","NULL","机械镀锌12/48/5","NULL"]
["DIN471M32MI000000",0.99,"DIN471","M32","65锰","NULL","机械镀锌24/72/5","NULL"]
["DIN9021M12ARHV140",0.99,"DIN9021","M12","碳钢","NULL","环保达克罗720无红","200-300HV"]
["G089386090MD00000",0.99,"GB893.1","M90","65锰",null,"发黑"]
["F017X42X08AR00000",0.98,"12938-00075","17*42*8","碳钢","NULL","Geomet","NULL"]
["ISO7090M42GF300HV",0.97,"ISO7090","M42","42#钢","NULL","热锌","300-370HV"]
["ISO7090M33AF00000",0.95,"ISO7090","M33","碳钢","NULL","热锌","140-250HV"]
["D00128A030MI00000",0.95,"DIN128A","M30","弹簧钢",null,"机械镀锌","44-51HRC"]
["G0009387024IG0000",0.94,"GB93-87","M24","65锰",null,"达克罗500无红","42-50HRC"]
["G005287016AK00000",0.9,"GB5287","M16","碳钢","NULL","三价锌","100HV"]
["G009785033AB140HV",0.9,"GB97-85","M33","碳钢","NULL","镀锌","140-250HV"]
["X007349016AF200HV",0.9,"DIN7349","M16","碳钢","NULL","热锌","200HV"]
["XXT0000033",0.9,"DIN9021","M6","45#","NULL","灰色锌镍500无红","300HV"]
["XXT0000072",0.9,"DIN125A","M6","Q235","NULL","灰色锌镍","200HV"]
["XXT0000292",0.9,"DIN9021","M16","Q235","NULL","上海环保达克罗0/500","200HV"]
["D00127B024IR00000",0.9,"DIN127B","M24","弹簧钢","NULL","环保达克罗720无红","NULL"]
["F031X100X5AK00000",0.89500000000000002,"11724-04835","31*100*5","45#钢",null,"三价锌","200HB"]
["GB19722005M20A000",0.88,"GB1972-2005  A型","20*10.2*1.1","60Si2MnA","NULL","达克罗720无红","NULL"]
["ISO7089M24GRHV300",0.85,"ISO7089","M24","45#钢","NULL","上海环保达克罗1000无红","300-370HV"]
["A000000001MR00000",0.85,"BN90704 6344852","1\"美制标准弹垫","65锰","NULL","上海环保达克罗（TL245:OFL-T602）","NULL"]
["D007349016ACHV140",0.8,"DIN7349","M16","碳钢","NULL","黄锌72/144/8","140HV"]
["G009785018AGHV200",0.8,"GB97-85","M18","碳钢",null,"达克罗500无红","200-300HV"]
["F0017X50X3CA00000",0.79,"BN91170 6348291","17*50*3(异形垫）","不锈钢316","NULL","不锈钢316","NULL"]
["DIN6796020MI00000",0.78,"DIN6796","M20","50CrV4","NULL","机械镀锌","420-490HV"]
["F0017X50X5AK200HV",0.75,"DIN522A","17*50*5","碳钢","NULL","三价彩锌72/120/8","200-250HV"]
["D00125A039ACHV140",0.72,"DIN125A","M39","碳钢",null,"黄锌","140-250HV"]
["F013X305X2BA00000",0.71,"BN91170/6288764","13*30.5*2","不锈钢304",null,"不锈钢304"]
["F027X08X0058AA000",0.7,"13106-04151","0.27*0.8*0.058","Q235",null,"本色防锈油"]
["F064X30X125AK0000",0.7,"DIN522A","6.4*30*1.25","碳钢","NULL","三价彩锌72/144/5","160HV"]
["XXT000215",0.7,"18*55*0.5","18*55*0.5（停用）","Q235","NULL","三价锌5um","NULL"]
["XXT000324",0.66,"GB97-85","M36","50CrV4","NULL","三价锌12um","300HV"]
["ISO7091M39AK00000",0.65,"ISO7091","M39","碳钢","NULL","三价彩锌48/72/5","100-250HV"]
["ISO7090042GDHV300",0.6,"ISO7090","M42","45#钢",null,"本色","300-370HV"]
["ISO7090M06AN200HV",0.6,"ISO7090","M6","碳钢","NULL","灰色锌镍500无红","200-300HV"]
["XXT0000293",0.6,"DIN125B","M20","Q235","NULL","环保达克罗0/720","200HV"]
["XXT0000198",0.6,"DIN128A","M20","70#","NULL","上达环保0/500","44*51HRC"]
["XXT0000069",0.6,"ISO7093-1","M16","不锈钢304","NULL","本色","200HV"]
["XXT0000023",0.6,"DIN9021","M10","Q235","NULL","Geomet321+VL","200-300HV"]
["G009785027ABHV140",0.6,"GB97-85","M27","碳钢",null,"镀锌","140-250HV"]
["F07303X127X3GK000",0.58699999999999997,"'03040326","2-3/4(73.03*127*3)","50#钢","NULL","三价锌72/120/8","HRC38-45"]
["G009785039GV300HV",0.54,"GB97-85","M39","碳钢",null,"达克罗","200-300HV"]
["X0095024649000MG0",0.503,"DIN472","M120*4","65锰",null,"达克罗","西门子"]
["XXT0000271",0.5,"DIN6916","M16","45#","NULL","机械镀锌24/72/5um","300-350HV"]
["F013X32X05AB00000",0.5,"DM-20229-001-AA","13*32*0.5","Q235A","NULL","镀锌9um","NULL"]
["D00125A045AK00000",0.5,"DIN125A","M45","碳钢",null,"三价锌24/48/5","140-250HV"]
["X0004712012MI0000",0.49,"DIN471","M20","65锰","NULL","机械镀锌48无红","NULL"]
["G089386080MG00000",0.49,"GB893","M80","65锰",null,"达克罗"]
["F021X40X475GG0000",0.46,"NFE25-518Z","21*40*4.75","45#钢","NULL","达克罗1000无红","300HB,厚度4.5-5"]
["DIN6796M24UR00720",0.46,"DIN6796","M24","60Si2MnA","NULL","达克罗720无红","420-490HV"]
["D007349012AC012UM",0.45,"DIN7349","M12","碳钢","NULL","三价彩锌288无红12um","100HV"]
["D006340024GK00000",0.45,"DIN6340","M24","45#钢","NULL","三价彩锌5um","350-430HV"]
["DIN433M24AK0200HV",0.45,"DIN433","M24","碳钢","NULL","三价锌48/72/12","200-300HV"]
["G009387036BA00000",0.42,"GB93-87","M36","不锈钢304",null,"不锈钢304"]
["G009785030AB140HV",0.4,"GB97-85","M30","碳钢",null,"镀锌","140-250HV"]
["XXT0000025",0.4,"ISO7093-1","M16","Q235","NULL","Geomet500无红","200HV"]
["XXT0000236",0.4,"DIN125A","M16","Q235","NULL","三价锌3um","200HV"]
["D006796020NK00000",0.4,"DIN6796","M20","50CrV4","NULL","环保机械黄锌72/144/12","420-490HV"]
["D007089027AKHV200",0.4,"ISO7089","M27","碳钢",null,"三价锌","200-300HV"]
["A300004800",0.4,300004800,"4*13.2*3.5 方垫","碳钢","NULL","镀锌","200HV"]
["A300004802",0.4,300004802,"6*16.2*3.5 方垫","碳钢","NULL","镀锌","200HV"]
["A300004801",0.38,300004801,"5*14.2*3.5 方垫","碳钢","NULL","镀锌","200HV"]
["D000436020BAHV100",0.379,"DIN436","M20","不锈钢304",null,"不锈钢304","100HV"]
["DIN7349M14AA200HV",0.37,"DIN7349","M14","碳钢","NULL","本色","200HV"]
["G085688024AD00000",0.37,"GB856-88","M24","Q235B","NULL","发黑","NULL"]
["XXT0000304",0.36,"DIN125A","M42","45#","NULL","三价锌12um","200-300HV"]
["DINEN14399MB36000",0.35,"EN14399-6","M36","45#钢","NULL","本色","300-370HV"]
["XXT0000034",0.33,"GB97.2-2002","M14","45#","NULL","灰色锌镍500无红","300-360HV"]
["GB972002M52AF0000",0.32800000000000001,"GB97.1-2002","M52","碳钢",null,"热锌","200-300HV"]
["G085388030AB00000",0.32500000000000001,"GB853","M30","碳钢","NULL","镀锌","NULL"]
["G009387048FG00000",0.315,"GB93-87","M48","70#钢",null,"热锌","HRC30"]
["F083X16X3MA000000",0.315,"8.3*16*3","8.3*16*3","65锰","NULL","本色上油","﹥HRC30"]
["ISO7093M24GF00000",0.3,"ISO7093","M24","45#钢","NULL","热锌","232-239HV"]
["D00125A042AK005UM",0.3,"DIN125A","M42","碳钢",null,"三价锌5um","140-250HV"]
["D00127B010IK005UM",0.3,"DIN127B","M10","弹簧钢",null,"三价锌72无红5um"]
["A300004805",0.3,300004805,"12*29.6*3.5 方垫","碳钢","NULL","镀锌","200HV"]
["DIN2093C82X16X040",0.3,"DIN2093C","8.2*16*0.4","50CrV4","NULL","黑磷化","NULL"]
["A300004803",0.28000000000000003,300004803,"8*20*3.5 方垫","碳钢","NULL","镀锌","200HV"]
["D00125A048AKHV140",0.26700000000000002,"DIN125A","M48","碳钢",null,"三价锌5um","140-250HV"]
["D006340024GC00000",0.26400000000000001,"DIN6340","M24","45#钢","NULL","三价锌5um","350-430HV"]
["A300004806",0.24,300004806,"16*36.4*3.5 方垫","碳钢","NULL","镀锌","200HV"]
["A300004804",0.23,300004804,"10*23*3.5 方垫","碳钢","NULL","镀锌","200HV"]
["ISO7093M24AA100HV",0.21299999999999999,"ISO7093","M24","碳钢",null,"本色","100HV"]
["ISO7093M12GDHV300",0.2,"ISO7093","M12","45#钢","NULL","热处理发黑","300-370HV"]
["F08X24X3GA0000000",0.2,"方垫","8*24*3","45#钢","NULL","热处理本色","25-32HRC"]
["F06X24X3GA0000000",0.2,"方垫","6*24*3","45#钢","NULL","热处理本色","25-32HRC"]
["F05X24X3GA0000000",0.2,"方垫","5*24*3","45#钢","NULL","热处理本色","25-32HRC"]
["F04X24X3GA0000000",0.2,"方垫","4*24*3","45#钢","NULL","热处理本色","25-32HRC"]
["G009387024IF00000",0.2,"GB93-87","M24","65锰",null,"热锌"]
["D000126039AL00000",0.2,"DIN126","M39","碳钢",null,"三价彩锌48/72/5","100-250HV"]
["F000001000904P438",0.2,"BN90701 6009168","1000904P438","低碳钢","NULL","镀锌","NULL"]
["F014X47X4AF000000",0.2,"DM-61722-001-AB","14*47*4","Q235",null,"热锌"]
["F015$16X21$2X5$32",0.2,"BN90701 6351007","1-5/16*2-1/2*5/32","碳钢","NULL","热锌","NULL"]
["F0022X50X5AA200HV",0.2,"BN90701  6355028","22*50*5","碳钢","NULL","本色","200HV"]
["G00972002048GA000",0.19,"GB97.1-2002","M48","碳钢","NULL","热锌","200-300HV"]
["GB972002048AF0000",0.18,"GB97.1-2002","M48","碳钢","NULL","热锌","140-250HV"]
["F00015X24X3AC0000",0.18,"15*24*3（按图纸）","15*24*3","45#钢","NULL","黄锌72/144/8","HRC36-42"]
["DIN9021010AKHV200",0.18,"DIN9021","M12","碳钢",null,"三价锌5um","200-250HV"]
["F53X26X19X2GA0001",0.16500000000000001,"200-1DQ(试制）","5.3*26*19*2","50#钢","NULL","热处理本色","300-400HV"]
["ISO7089M36AN200HV",0.158,"ISO7089","M36","碳钢","NULL","Geomet 321VL 1000无红0.09-0.14摩擦","200-300HV"]
["DINEN14399M360000",0.14599999999999999,"EN14399-6","M36","45#钢","NULL","灰色锌镍240/1000","300-370HV"]
["X0095051236000CA0",0.14000000000000001,"950-51236-000","20*40*1","碳钢","NULL","黄锌","西门子"]
["G861187030CA00000",0.14000000000000001,"GB861.1","M30","不锈钢316","NULL","不锈钢316","NULL"]
["FAS1030010AA00000",0.113,"调整垫片","AS1-30-1.00","不锈钢304","NULL","不锈钢304","NULL"]
["FAS2X24X020BA0000",0.107,"调整垫片","As2-24-0.20","不锈钢304",null,"不锈钢304"]
["FAS2X24X050BA0000",0.105,"调整垫片","As2-24-0.50","不锈钢304",null,"不锈钢304"]
["FAS2X24X100BA0000",0.105,"调整垫片","As2-24-1.00","不锈钢304",null,"不锈钢304"]
["FAS2X24X005BA0000",0.105,"调整垫片","As2-24-0.05","不锈钢304",null,"不锈钢304"]
["FAS1036002AA00000",0.105,"调整垫片","AS1-36-0.20","不锈钢304","NULL","不锈钢304","NULL"]
["FAS1036005BA00000",0.104,"调整垫片","AS1-36-0.05","不锈钢304",null,"不锈钢304"]
["FAS1036010AA00000",0.104,"调整垫片","AS1-36-1.00","不锈钢304","NULL","不锈钢304","NULL"]
["FAS1030002AA00000",0.104,"调整垫片","AS1-30-0.20","不锈钢304","NULL","不锈钢304","NULL"]
["FAS1042020BA00000",0.104,"调整垫片","AS1-42-2","不锈钢304",null,"不锈钢304"]
["F0AS1X30X0050BA00",0.104,"调整垫片","AS1-30-0.05","不锈钢304",null,"不锈钢304"]
["F00AS1X30X010BA00",0.104,"调整垫片","AS1-30-0.10","不锈钢304",null,"不锈钢304"]
["F00AS1X30X050BA00",0.10299999999999999,"调整垫片","AS1-30-0.50","不锈钢304",null,"不锈钢304"]
["F00AS1X36X010BA00",0.10299999999999999,"调整垫片","AS1-36-0.10","不锈钢304",null,"不锈钢304"]
["F00AS1X42X020BA00",0.10299999999999999,"调整垫片","AS1-42-0.2","不锈钢304",null,"不锈钢304"]
["FAS1042005AA00000",0.10299999999999999,"调整垫片","AS1-42-0.5","不锈钢304","NULL","不锈钢304","NULL"]
["FAS1042010AA00000",0.10299999999999999,"调整垫片","AS1-42-1","不锈钢304","NULL","不锈钢304","NULL"]
["F00AS1X42X010BA00",0.10100000000000001,"调整垫片","AS1-42-0.1","不锈钢304",null,"不锈钢304"]
["DIN6916M20GD00000",0.1,"DIN6916","M20","45#钢","NULL","DELTA TONE + SEAL GZ BLACK，1000H≥10um，摩擦0.08-0.14","300-370HV"]
["D00125A052AKHV140",0.1,"DIN125A","M52","碳钢",null,"三价锌","140-250HV"]
["D00125A036AAHV300",0.1,"DIN125A","M36","45#钢",null,"本色","300-400HV"]
["FAS1030200AA00000",0.1,"调整垫片","AS1-30-2.00","不锈钢304",null,"不锈钢304"]
["FAS1036200AA00000",0.1,"调整垫片","AS1-36-2.00","不锈钢304",null,"不锈钢304"]
["GB848M14GG00300HV",0.1,"GB848-85","M14","45#钢","NULL","达克罗1000无红","300-370HV"]
["NFE25511MM08MG000",0.1,"NFE25-511M","M8","65锰","NULL","环保达克罗1000无红","NULL"]
["NFE25511MM10MG000",0.1,"NFE25-511M","M10","65锰","NULL","环保达克罗1000无红","NULL"]
["X00000M12MG2551E",0.1,"NFE25-511M","M12","65锰","NULL","环保达克罗1000无红","NULL"]
["XXT0000212",0.1,"DIN125A","M39","Q235","NULL","三价锌","200-250HV"]
["FAS2X24X200BA0000",9.9000000000000005E-2,"调整垫片","As2-24-2.00","不锈钢304",null,"不锈钢304"]
["FAS2X24X010BA0000",9.7000000000000003E-2,"调整垫片","As2-24-0.10","不锈钢304",null,"不锈钢304"]
["G085688M24AF00000",0.08,"GB856 ","M24*2","低碳钢","NULL","热锌","NULL"]
["NFE25514LM24AR000",0.08,"NFE25-514L","M24","碳钢",null,"上海环保达克罗","160-250HV"]
["G085388027AF00000",7.5999999999999998E-2,"GB853-88","M27","碳钢","NULL","热锌","NULL"]
["G089486295MN00000",7.4999999999999997E-2,"GB894","M295","65锰","NULL","发黑","NULL"]
["G089486345MN00000",6.9000000000000006E-2,"GB894","M345","65锰","NULL","发黑","NULL"]
["G089486395MN00000",6.9000000000000006E-2,"GB894","M395","65锰","NULL","发黑","NULL"]
["G089486032MA00000",0.05,"GB894.1","M32","65锰","NULL","本色","NULL"]
["G089386135MG00000",0.05,"GB893","M135","65锰",null,"达克罗"]
["F0517X0875X008950",0.05,"BN90701 6340638","0.517*0.875*0.0895","碳钢","NULL","三价锌","NULL"]
["G085388030AG00000",0.04,"GB853-88","M30","碳钢","NULL","达克罗","NULL"]
["G089386M290MG0000",2.7E-2,"JB/ZQ4343","M290","65锰","NULL","达克罗","NULL"]
["F015X24X3AC000000",0.02,"DIN522A","15*24*3","碳钢","NULL","黄锌72/144/8","HRC36-42"]
["F0175X50X6GK00000",1.4E-2,30871113200,"17.5*50*6","45#钢","NULL","三价锌72/144/5","HRC30-36"]
["G089386M310MG0000",2E-3,"JB/ZQ4343","M310","65锰","NULL","达克罗","NULL"]
["G0JB/ZQ4349100MB0",1E-3,"JB/ZQ4349","M100","碳钢","NULL","达克罗","NULL"]
["F000125000AG00000",1E-3,"JB/ZQ4349","M125","碳钢","NULL","达克罗","NULL"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}